(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 77)
    (no_connects 0)
    (area 115.013099 32.529199 193.409405 127.66975)
    (thickness 1.6)
    (drawings 475)
    (tracks 294)
    (zones 0)
    (modules 24)
    (nets 37)
  )
  (page A4)
  (title_block
    (title Versa64Cart)
    (date 2017-06-27)
    (rev 1.0)
    (comment 1 "Circuits drawn by BWACK")
    (comment 2 "Based on Jim Brain's Simple64Cart (eagle design)")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3048)
    (user_trace_width 0.508)
    (trace_clearance 0.2)
    (zone_clearance 0.000003)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.0254)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.826 4.826)
    (pad_drill 4.826)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 151.765 68.58)
    (grid_origin 150.495 78.105)
    (visible_elements 7FFFEF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 /A15)
  (net 2 D3)
  (net 3 /A12)
  (net 4 D4)
  (net 5 /A7)
  (net 6 D5)
  (net 7 /A6)
  (net 8 D6)
  (net 9 /A5)
  (net 10 D7)
  (net 11 /A4)
  (net 12 /A3)
  (net 13 /A10)
  (net 14 /A2)
  (net 15 /A1)
  (net 16 /A11)
  (net 17 /A0)
  (net 18 /A9)
  (net 19 D0)
  (net 20 /A8)
  (net 21 D1)
  (net 22 /A13)
  (net 23 D2)
  (net 24 /A14)
  (net 25 GND)
  (net 26 +5V)
  (net 27 "Net-(J1-PadF)")
  (net 28 "Net-(J1-PadH)")
  (net 29 "Net-(J1-PadJ)")
  (net 30 "Net-(D1-Pad2)")
  (net 31 "#GAME")
  (net 32 "#EXROM")
  (net 33 /#ROML)
  (net 34 "Net-(J5-Pad1)")
  (net 35 /#ROMH)
  (net 36 /#OE)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "#EXROM")
    (add_net "#GAME")
    (add_net +5V)
    (add_net /#OE)
    (add_net /#ROMH)
    (add_net /#ROML)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-PadF)")
    (add_net "Net-(J1-PadH)")
    (add_net "Net-(J1-PadJ)")
    (add_net "Net-(J5-Pad1)")
  )
  (net_class small ""
    (clearance 0.254)
    (trace_width 0.3048)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 164.465 76.2)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_5mm (layer F.Cu) (tedit 5952EA9E)
    (at 149.225 76.835)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (fp_text reference REF** (at 0.508 -4.064) (layer F.SilkS) hide)
    (fp_text value MountingHole_5mm (at 0 6) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.826 4.826) (drill 4.826) (layers *.Cu))
  )
  (module Housings_DIP:DIP-28_W15.24mm_LongPads (layer F.Cu) (tedit 594EFBCC)
    (at 141.605 102.235 90)
    (descr "28-lead dip package, row spacing 15.24 mm (600 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 15.24mm 600mil LongPads")
    (fp_text reference U1 (at -2.54 31.75 180) (layer F.SilkS))
    (fp_text value 27512 (at 7.62 35.41 90) (layer F.Fab))
    (fp_text user %R (at 7.62 16.51 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /A15))
    (pad 15 thru_hole oval (at 15.24 33.02 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 D3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /A12))
    (pad 16 thru_hole oval (at 15.24 30.48 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 D4))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /A7))
    (pad 17 thru_hole oval (at 15.24 27.94 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 D5))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /A6))
    (pad 18 thru_hole oval (at 15.24 25.4 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 D6))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /A5))
    (pad 19 thru_hole oval (at 15.24 22.86 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 D7))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /A4))
    (pad 20 thru_hole oval (at 15.24 20.32 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /A3))
    (pad 21 thru_hole oval (at 15.24 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /A10))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /A2))
    (pad 22 thru_hole oval (at 15.24 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /#OE))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /A1))
    (pad 23 thru_hole oval (at 15.24 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /A11))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /A0))
    (pad 24 thru_hole oval (at 15.24 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /A9))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 D0))
    (pad 25 thru_hole oval (at 15.24 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /A8))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 D1))
    (pad 26 thru_hole oval (at 15.24 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /A13))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 D2))
    (pad 27 thru_hole oval (at 15.24 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /A14))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 28 thru_hole oval (at 15.24 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-28_W15.24mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 594EF57C)
    (at 140.335 81.915 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value R (at 3.81 2.31 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 +5V))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /A14))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm (layer F.Cu) (tedit 594EFF8D)
    (at 125.095 89.535)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J5 (at -2.54 3.81 90) (layer F.SilkS))
    (fp_text value CONN_02X02 (at 1.27 4.87) (layer F.Fab) hide)
    (fp_text user %R (at -2.54 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /A13))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /#ROML))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /A13))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 594EFF88)
    (at 125.095 95.885)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J6 (at -2.54 6.35 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 1.27 7.41) (layer F.Fab) hide)
    (fp_text user %R (at -2.54 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /#OE))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /#ROML))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /#OE))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /#ROMH))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /#OE))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module UserLibraries:C64_EXPANSION_PORT (layer F.Cu) (tedit 594EE0D1)
    (at 150.495 116.078)
    (fp_text reference J1 (at 17.78 -5.08) (layer F.SilkS))
    (fp_text value EXPANSION_PORT_C64 (at -20.701 -6.223) (layer F.Fab) hide)
    (fp_text user Z (at 25.4 -5.08) (layer B.SilkS))
    (fp_text user A (at -27.94 -5.08) (layer B.SilkS))
    (fp_text user 1 (at -27.94 -5.08) (layer F.SilkS))
    (fp_text user 22 (at 25.4 -5.08) (layer F.SilkS))
    (pad 1 connect rect (at -27.94 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 25 GND))
    (pad 2 connect rect (at -25.4 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 26 +5V))
    (pad 3 connect rect (at -22.86 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 26 +5V))
    (pad 4 connect rect (at -20.32 0) (size 1.5 8) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -17.78 0) (size 1.5 8) (layers F.Cu F.Mask))
    (pad 6 connect rect (at -15.24 0) (size 1.5 8) (layers F.Cu F.Mask))
    (pad 7 connect rect (at -12.7 0) (size 1.5 8) (layers F.Cu F.Mask))
    (pad 8 connect rect (at -10.16 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 31 "#GAME"))
    (pad 9 connect rect (at -7.62 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 32 "#EXROM"))
    (pad 10 connect rect (at -5.08 0) (size 1.5 8) (layers F.Cu F.Mask))
    (pad 11 connect rect (at -2.54 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 33 /#ROML))
    (pad 12 connect rect (at 0 0) (size 1.5 8) (layers F.Cu F.Mask))
    (pad 13 connect rect (at 2.54 0) (size 1.5 8) (layers F.Cu F.Mask))
    (pad 14 connect rect (at 5.08 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 10 D7))
    (pad 15 connect rect (at 7.62 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 8 D6))
    (pad 16 connect rect (at 10.16 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 6 D5))
    (pad 17 connect rect (at 12.7 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 4 D4))
    (pad 18 connect rect (at 15.24 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 2 D3))
    (pad 19 connect rect (at 17.78 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 23 D2))
    (pad 20 connect rect (at 20.32 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 21 D1))
    (pad 21 connect rect (at 22.86 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 19 D0))
    (pad 22 connect rect (at 25.4 0) (size 1.5 8) (layers F.Cu F.Mask)
      (net 25 GND))
    (pad A connect rect (at -27.94 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 25 GND))
    (pad B connect rect (at -25.4 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 35 /#ROMH))
    (pad C connect rect (at -22.86 0) (size 1.5 8) (layers B.Cu F.Mask))
    (pad D connect rect (at -20.32 0) (size 1.5 8) (layers B.Cu F.Mask))
    (pad E connect rect (at -17.78 0) (size 1.5 8) (layers B.Cu F.Mask))
    (pad F connect rect (at -15.24 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 27 "Net-(J1-PadF)"))
    (pad H connect rect (at -12.7 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 28 "Net-(J1-PadH)"))
    (pad J connect rect (at -10.16 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 29 "Net-(J1-PadJ)"))
    (pad K connect rect (at -7.62 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 3 /A12))
    (pad L connect rect (at -5.08 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 16 /A11))
    (pad M connect rect (at -2.54 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 13 /A10))
    (pad N connect rect (at 0 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 18 /A9))
    (pad P connect rect (at 2.54 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 20 /A8))
    (pad R connect rect (at 5.08 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 5 /A7))
    (pad S connect rect (at 7.62 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 7 /A6))
    (pad T connect rect (at 10.16 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 9 /A5))
    (pad U connect rect (at 12.7 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 11 /A4))
    (pad V connect rect (at 15.24 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 12 /A3))
    (pad W connect rect (at 17.78 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 14 /A2))
    (pad X connect rect (at 20.32 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 15 /A1))
    (pad Y connect rect (at 22.86 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 17 /A0))
    (pad Z connect rect (at 25.4 0) (size 1.5 8) (layers B.Cu F.Mask)
      (net 25 GND))
  )
  (module Diodes_ThroughHole:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 594E5CC4)
    (at 130.175 104.775 180)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value D (at 3.81 2.06 180) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /#ROML))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 594E5CC6)
    (at 130.175 107.315 180)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value D (at 3.81 2.06 180) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /#ROMH))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 594D11E0)
    (at 147.32 81.915)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 0) (layer F.SilkS))
    (fp_text value R (at 3.81 2.31) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 +5V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /#OE))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 594EBB1A)
    (at 137.795 94.615 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value R (at 3.81 2.31 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 +5V))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /A15))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 594D11D6)
    (at 144.145 81.915 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value R (at 3.81 2.54 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 +5V))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /A13))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 594E505C)
    (at 135.255 107.061)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J4 (at 0 -1.6) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 1.6) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-PadF)"))
    (model Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_DIP_x5_W7.62mm_Slide (layer F.Cu) (tedit 594EF5C7)
    (at 125.095 81.915 90)
    (descr "5x-dip-switch, Slide, row spacing 7.62 mm (300 mils)")
    (tags "DIP Switch Slide 7.62mm 300mil")
    (fp_text reference SW1 (at 3.81 -3.48 90) (layer F.SilkS))
    (fp_text value SW_DIP_x05 (at 3.81 13.64 90) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 6 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 7 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /A14))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 8 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /A15))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 9 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "#EXROM"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 10 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "#GAME"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_DIP_x5_W7.62mm_Slide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer B.Cu) (tedit 594FAE9E)
    (at 130.81 101.6 90)
    (fp_text reference JP3 (at 1.905 0 180) (layer B.SilkS))
    (fp_text value JUMPER_2-PIN (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 35 /#ROMH))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 36 /#OE))
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer B.Cu) (tedit 594FAF54)
    (at 125.095 78.105 90)
    (fp_text reference JP4 (at 2.032 0 180) (layer B.SilkS))
    (fp_text value JUMPER_2-PIN (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 25 GND))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 31 "#GAME"))
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer B.Cu) (tedit 594FAF58)
    (at 127.635 78.105 90)
    (fp_text reference JP5 (at 2.032 0 180) (layer B.SilkS))
    (fp_text value JUMPER_2-PIN (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 25 GND))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 32 "#EXROM"))
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer B.Cu) (tedit 594FAF08)
    (at 133.223 92.329 270)
    (fp_text reference JP6 (at -2.032 0 360) (layer B.SilkS))
    (fp_text value JUMPER_2-PIN (at 0 0 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(J5-Pad1)"))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 22 /A13))
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer B.Cu) (tedit 594FAF0D)
    (at 130.683 92.329 90)
    (fp_text reference JP7 (at 2.032 0 180) (layer B.SilkS))
    (fp_text value JUMPER_2-PIN (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 33 /#ROML))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 22 /A13))
  )
  (module Connect:PINTST (layer F.Cu) (tedit 594E5064)
    (at 140.335 107.061)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J2 (at 0 -1.6) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 1.6) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-PadJ)"))
    (model Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 594E5050)
    (at 137.795 107.061)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J3 (at 0 -1.6) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 1.6) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-PadH)"))
    (model Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer B.Cu) (tedit 594FBB2D)
    (at 133.35 96.52 270)
    (fp_text reference JP1 (at -1.905 0 360) (layer B.SilkS))
    (fp_text value JUMPER_2-PIN (at 0 0 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 36 /#OE))
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer B.Cu) (tedit 594FBB27)
    (at 130.81 96.52 270)
    (fp_text reference JP2 (at -1.905 0 360) (layer B.SilkS))
    (fp_text value JUMPER_2-PIN (at 0 0 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 33 /#ROML))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 36 /#OE))
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 594F004E)
    (at 137.795 92.075 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C1 (at 4.445 0 180) (layer F.SilkS))
    (fp_text value C_Small (at 1.25 2.36 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 +5V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 48.912787 (width 0.3) (layer Dwgs.User)
    (gr_text "48,913 mm" (at 186.909405 96.206864 270.0297532) (layer Dwgs.User))
    (feature1 (pts (xy 178.181 71.755) (xy 188.246705 71.749773)))
    (feature2 (pts (xy 178.2064 120.66778) (xy 188.272105 120.662553)))
    (crossbar (pts (xy 185.572105 120.663955) (xy 185.546705 71.751175)))
    (arrow1a (pts (xy 185.546705 71.751175) (xy 186.133711 72.877374)))
    (arrow1b (pts (xy 185.546705 71.751175) (xy 184.960869 72.877983)))
    (arrow2a (pts (xy 185.572105 120.663955) (xy 186.157941 119.537147)))
    (arrow2b (pts (xy 185.572105 120.663955) (xy 184.985099 119.537756)))
  )
  (dimension 57.962801 (width 0.3) (layer Dwgs.User)
    (gr_text "57,963 mm" (at 149.225742 126.315939 0.007532311023) (layer Dwgs.User))
    (feature1 (pts (xy 178.2064 120.66778) (xy 178.20732 127.662129)))
    (feature2 (pts (xy 120.2436 120.6754) (xy 120.24452 127.669749)))
    (crossbar (pts (xy 120.244165 124.969749) (xy 178.206965 124.962129)))
    (arrow1a (pts (xy 178.206965 124.962129) (xy 177.080538 125.548698)))
    (arrow1b (pts (xy 178.206965 124.962129) (xy 177.080384 124.375856)))
    (arrow2a (pts (xy 120.244165 124.969749) (xy 121.370746 125.556022)))
    (arrow2b (pts (xy 120.244165 124.969749) (xy 121.370592 124.38318)))
  )
  (gr_text A13 (at 122.555 92.075 90) (layer F.SilkS))
  (gr_text "#OE" (at 122.555 99.695 90) (layer F.SilkS))
  (gr_text Switch (at 130.175 89.535) (layer F.SilkS))
  (gr_text 16K (at 130.175 92.075) (layer F.SilkS))
  (gr_text "#ROMH" (at 130.175 100.965) (layer F.SilkS))
  (gr_text "#ROML" (at 130.175 98.425) (layer F.SilkS))
  (gr_text A13 (at 135.255 83.82 315) (layer F.SilkS))
  (gr_text A14 (at 132.715 83.82 315) (layer F.SilkS))
  (gr_text A15 (at 130.175 83.82 315) (layer F.SilkS))
  (gr_text "#EXROM" (at 127.635 83.82 315) (layer F.SilkS))
  (gr_text "#GAME" (at 125.095 83.82 315) (layer F.SilkS))
  (gr_text 16K (at 130.175 95.885) (layer F.SilkS))
  (gr_line (start 120.269 119.253) (end 120.269 119.634) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 121.285 119.634) (end 121.285 120.65) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 178.181 119.634) (end 178.181 119.253) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 177.165 119.634) (end 178.181 119.634) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 120.269 71.755) (end 178.181 71.755) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 178.181 71.755) (end 178.181 119.253) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 120.269 71.755) (end 120.269 119.253) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 121.285 120.65) (end 177.165 120.65) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.2064 120.6754) (xy 120.2436 120.6754) (xy 120.2436 111.76) (xy 178.2064 111.76)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.2064 120.6754) (xy 120.2436 120.6754) (xy 120.2436 111.76) (xy 178.2064 111.76)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.054 103.505) (xy 176.784 103.505) (xy 176.784 100.33) (xy 178.054 100.33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.539 103.505) (xy 120.269 103.505) (xy 120.269 100.33) (xy 121.539 100.33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.34 110.49) (xy 118.11 110.49) (xy 118.11 108.585) (xy 180.34 108.585)
      )
    )
  )
  (zone (net 26) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.000003))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.41936 112.0775) (xy 128.19888 112.0775) (xy 128.18618 120.07596) (xy 124.45238 120.07596) (xy 124.45238 120.03024)
      )
    )
  )
)
