(kicad_pcb (version 4) (host pcbnew 4.0.0-stable)
  (general
    (links 263)
    (no_connects 0)
    (area 77.279499 33.909 198.186525 141.325601)
    (thickness 1.6002)
    (drawings 43)
    (tracks 1555)
    (zones 0)
    (modules 41)
    (nets 103)
  )
  (page USLetter)
  (title_block
    (title "XT-IDE Revision 3")
    (date 2016-05-14)
    (rev 3B)
    (company "The Glitch Works")
    (comment 1 "J. Chapman")
  )
  (layers
    (0 Component signal)
    (31 Copper signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (user_trace_width 1.27)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.381)
    (edge_width 0.381)
    (via_size 0.889)
    (via_drill 0.5842)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.2032)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.254)
    (pcb_text_size 1.016 1.524)
    (mod_edge_width 0.381)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0.254)
    (aux_axis_origin 74.93 140.97)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x014e0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 0)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 /*CS1FX)
  (net 2 /*CS3FX)
  (net 3 /*IOR-IDE)
  (net 4 /*IOW-IDE)
  (net 5 /*IOW-ISA)
  (net 6 /*MEMR)
  (net 7 /*RESET)
  (net 8 //CS_ROM)
  (net 9 /2)
  (net 10 /3)
  (net 11 /4)
  (net 12 /5)
  (net 13 /6)
  (net 14 /7)
  (net 15 /A0-IDE)
  (net 16 /A0-ISA)
  (net 17 /A1-IDE)
  (net 18 /A1-ISA)
  (net 19 /A10)
  (net 20 /A11)
  (net 21 /A12)
  (net 22 /A2-IDE)
  (net 23 /A2-ISA)
  (net 24 /A3)
  (net 25 /D10)
  (net 26 /D11)
  (net 27 /D12)
  (net 28 /D13)
  (net 29 /D14)
  (net 30 /D15)
  (net 31 /D8)
  (net 32 /D9)
  (net 33 /INTRQ)
  (net 34 /IRQ3)
  (net 35 /IRQ4)
  (net 36 /IRQ5)
  (net 37 /IRQ7)
  (net 38 /PC-DB0)
  (net 39 /PC-DB1)
  (net 40 /PC-DB2)
  (net 41 /PC-DB3)
  (net 42 /PC-DB4)
  (net 43 /PC-DB5)
  (net 44 /PC-DB6)
  (net 45 /PC-DB7)
  (net 46 /VCC_CF)
  (net 47 GND)
  (net 48 VCC)
  (net 49 "Net-(U5-Pad2)")
  (net 50 "Net-(U5-Pad5)")
  (net 51 "Net-(U5-Pad9)")
  (net 52 "Net-(U5-Pad10)")
  (net 53 "Net-(U5-Pad11)")
  (net 54 *MEMW)
  (net 55 AEN)
  (net 56 A14)
  (net 57 A13)
  (net 58 "Net-(R2-Pad2)")
  (net 59 /ROM_WE)
  (net 60 "Net-(RP2-Pad6)")
  (net 61 "Net-(RP2-Pad5)")
  (net 62 "Net-(RP2-Pad4)")
  (net 63 "Net-(RP2-Pad3)")
  (net 64 "Net-(RP1-Pad7)")
  (net 65 "Net-(RP1-Pad8)")
  (net 66 "Net-(RP2-Pad7)")
  (net 67 "Net-(RP2-Pad8)")
  (net 68 "Net-(RP1-Pad3)")
  (net 69 "Net-(RP1-Pad4)")
  (net 70 "Net-(RP1-Pad5)")
  (net 71 "Net-(RP1-Pad6)")
  (net 72 A19)
  (net 73 A18)
  (net 74 A17)
  (net 75 A16)
  (net 76 A15)
  (net 77 A9)
  (net 78 A8)
  (net 79 A7)
  (net 80 A6)
  (net 81 A5)
  (net 82 A4)
  (net 83 "Net-(U4-Pad11)")
  (net 84 "Net-(J2-Pad2)")
  (net 85 "Net-(J3-Pad2)")
  (net 86 *DASP)
  (net 87 "Net-(R4-Pad2)")
  (net 88 "Net-(D1-Pad1)")
  (net 89 "Net-(J5-Pad2)")
  (net 90 D7)
  (net 91 RESDRV)
  (net 92 IRQ2)
  (net 93 *IOR-ISA)
  (net 94 D6)
  (net 95 D5)
  (net 96 D4)
  (net 97 D3)
  (net 98 D2)
  (net 99 D1)
  (net 100 D0)
  (net 101 /CS_IDE)
  (net 102 /CARDSEL)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.889)
    (via_drill 0.5842)
    (uvia_dia 0.508)
    (uvia_drill 0.2032)
    (add_net *DASP)
    (add_net *IOR-ISA)
    (add_net *MEMW)
    (add_net /*CS1FX)
    (add_net /*CS3FX)
    (add_net /*IOR-IDE)
    (add_net /*IOW-IDE)
    (add_net /*IOW-ISA)
    (add_net /*MEMR)
    (add_net /*RESET)
    (add_net //CS_ROM)
    (add_net /2)
    (add_net /3)
    (add_net /4)
    (add_net /5)
    (add_net /6)
    (add_net /7)
    (add_net /A0-IDE)
    (add_net /A0-ISA)
    (add_net /A1-IDE)
    (add_net /A1-ISA)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A2-IDE)
    (add_net /A2-ISA)
    (add_net /A3)
    (add_net /CARDSEL)
    (add_net /CS_IDE)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D14)
    (add_net /D15)
    (add_net /D8)
    (add_net /D9)
    (add_net /INTRQ)
    (add_net /IRQ3)
    (add_net /IRQ4)
    (add_net /IRQ5)
    (add_net /IRQ7)
    (add_net /PC-DB0)
    (add_net /PC-DB1)
    (add_net /PC-DB2)
    (add_net /PC-DB3)
    (add_net /PC-DB4)
    (add_net /PC-DB5)
    (add_net /PC-DB6)
    (add_net /PC-DB7)
    (add_net /ROM_WE)
    (add_net A13)
    (add_net A14)
    (add_net A15)
    (add_net A16)
    (add_net A17)
    (add_net A18)
    (add_net A19)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net A8)
    (add_net A9)
    (add_net AEN)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net IRQ2)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(RP1-Pad3)")
    (add_net "Net-(RP1-Pad4)")
    (add_net "Net-(RP1-Pad5)")
    (add_net "Net-(RP1-Pad6)")
    (add_net "Net-(RP1-Pad7)")
    (add_net "Net-(RP1-Pad8)")
    (add_net "Net-(RP2-Pad3)")
    (add_net "Net-(RP2-Pad4)")
    (add_net "Net-(RP2-Pad5)")
    (add_net "Net-(RP2-Pad6)")
    (add_net "Net-(RP2-Pad7)")
    (add_net "Net-(RP2-Pad8)")
    (add_net "Net-(U4-Pad11)")
    (add_net "Net-(U5-Pad10)")
    (add_net "Net-(U5-Pad11)")
    (add_net "Net-(U5-Pad2)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U5-Pad9)")
    (add_net RESDRV)
  )
  (net_class Power ""
    (clearance 0.2032)
    (trace_width 1.2192)
    (via_dia 0.889)
    (via_drill 0.5842)
    (uvia_dia 0.508)
    (uvia_drill 0.2032)
    (add_net /VCC_CF)
    (add_net GND)
    (add_net VCC)
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer Component) (tedit 57279112)
    (at 175.26 88.265)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference C1 (at -2.54 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 3.81 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 48 VCC))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer Component) (tedit 5726C593)
    (at 119.38 38.1)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference C2 (at -2.54 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 3.81 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 48 VCC))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer Component) (tedit 572679B6)
    (at 107.95 38.1 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference C3 (at 10.16 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 3.81 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 48 VCC))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer Component) (tedit 57264A3D)
    (at 163.83 88.265 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference C4 (at 10.16 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 3.81 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 48 VCC))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer Component) (tedit 5726D868)
    (at 107.95 88.265 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference C5 (at 10.16 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 3.81 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 48 VCC))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer Component) (tedit 5726C3CD)
    (at 156.21 48.26 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference C7 (at 10.16 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 3.81 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 48 VCC))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer Component) (tedit 5726C3D2)
    (at 142.24 40.64 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference C8 (at 10.16 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 3.81 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 48 VCC))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer Component) (tedit 5727A761)
    (at 168.275 48.26 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference C9 (at 9.525 -1.27 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 3.81 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 48 VCC))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer Component) (tedit 5726C5EB)
    (at 172.72 45.72)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference C10 (at -3.175 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 3.81 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 48 VCC))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Component) (tedit 572FD418)
    (at 172.72 40.64 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 1.27 -1.905 180) (layer F.SilkS))
    (fp_text value 470R (at 5.08 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 88 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 86 *DASP))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module dip_sockets:DIP-20__300_ELL (layer Component) (tedit 57264ED7)
    (at 179.07 104.14 270)
    (descr "20 pins DIL package, elliptical pads")
    (tags DIL)
    (fp_text reference U1 (at 15.875 1.905 360) (layer F.SilkS))
    (fp_text value 74LS245 (at 3.556 1.016 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 *IOR-ISA))
    (pad 2 thru_hole oval (at -8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /PC-DB0))
    (pad 3 thru_hole oval (at -6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /PC-DB1))
    (pad 4 thru_hole oval (at -3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /PC-DB2))
    (pad 5 thru_hole oval (at -1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /PC-DB3))
    (pad 6 thru_hole oval (at 1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /PC-DB4))
    (pad 7 thru_hole oval (at 3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /PC-DB5))
    (pad 8 thru_hole oval (at 6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /PC-DB6))
    (pad 9 thru_hole oval (at 8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /PC-DB7))
    (pad 10 thru_hole oval (at 11.43 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 11 thru_hole oval (at 11.43 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 90 D7))
    (pad 12 thru_hole oval (at 8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 94 D6))
    (pad 13 thru_hole oval (at 6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 95 D5))
    (pad 14 thru_hole oval (at 3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 96 D4))
    (pad 15 thru_hole oval (at 1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 97 D3))
    (pad 16 thru_hole oval (at -1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 D2))
    (pad 17 thru_hole oval (at -3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 D1))
    (pad 18 thru_hole oval (at -6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 D0))
    (pad 19 thru_hole oval (at -8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 /CS_IDE))
    (pad 20 thru_hole oval (at -11.43 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dip_sockets:DIP-20__300_ELL (layer Component) (tedit 57264EE1)
    (at 123.19 56.515 270)
    (descr "20 pins DIL package, elliptical pads")
    (tags DIL)
    (fp_text reference U2 (at 15.875 1.905 360) (layer F.SilkS))
    (fp_text value 74LS573 (at 3.556 1.016 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /2))
    (pad 2 thru_hole oval (at -8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 D0))
    (pad 3 thru_hole oval (at -6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 D1))
    (pad 4 thru_hole oval (at -3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 D2))
    (pad 5 thru_hole oval (at -1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 97 D3))
    (pad 6 thru_hole oval (at 1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 96 D4))
    (pad 7 thru_hole oval (at 3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 95 D5))
    (pad 8 thru_hole oval (at 6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 94 D6))
    (pad 9 thru_hole oval (at 8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 90 D7))
    (pad 10 thru_hole oval (at 11.43 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 11 thru_hole oval (at 11.43 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /3))
    (pad 12 thru_hole oval (at 8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D15))
    (pad 13 thru_hole oval (at 6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D14))
    (pad 14 thru_hole oval (at 3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D13))
    (pad 15 thru_hole oval (at 1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /D12))
    (pad 16 thru_hole oval (at -1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /D11))
    (pad 17 thru_hole oval (at -3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /D10))
    (pad 18 thru_hole oval (at -6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D9))
    (pad 19 thru_hole oval (at -8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D8))
    (pad 20 thru_hole oval (at -11.43 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dip_sockets:DIP-20__300_ELL (layer Component) (tedit 57264EE5)
    (at 104.14 56.515 270)
    (descr "20 pins DIL package, elliptical pads")
    (tags DIL)
    (fp_text reference U3 (at 15.875 1.905 360) (layer F.SilkS))
    (fp_text value 74LS573 (at 3.556 1.016 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 /4))
    (pad 2 thru_hole oval (at -8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D8))
    (pad 3 thru_hole oval (at -6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D9))
    (pad 4 thru_hole oval (at -3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /D10))
    (pad 5 thru_hole oval (at -1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /D11))
    (pad 6 thru_hole oval (at 1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /D12))
    (pad 7 thru_hole oval (at 3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D13))
    (pad 8 thru_hole oval (at 6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D14))
    (pad 9 thru_hole oval (at 8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D15))
    (pad 10 thru_hole oval (at 11.43 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 11 thru_hole oval (at 11.43 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 /5))
    (pad 12 thru_hole oval (at 8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 90 D7))
    (pad 13 thru_hole oval (at 6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 94 D6))
    (pad 14 thru_hole oval (at 3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 95 D5))
    (pad 15 thru_hole oval (at 1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 96 D4))
    (pad 16 thru_hole oval (at -1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 97 D3))
    (pad 17 thru_hole oval (at -3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 D2))
    (pad 18 thru_hole oval (at -6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 D1))
    (pad 19 thru_hole oval (at -8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 D0))
    (pad 20 thru_hole oval (at -11.43 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dip_sockets:DIP-20__300_ELL (layer Component) (tedit 5726C9F5)
    (at 138.43 56.515 270)
    (descr "20 pins DIL package, elliptical pads")
    (tags DIL)
    (fp_text reference U4 (at 15.875 1.905 360) (layer F.SilkS))
    (fp_text value 74LS245 (at 3.556 1.016 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 2 thru_hole oval (at -8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /*CS3FX))
    (pad 3 thru_hole oval (at -6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /*CS1FX))
    (pad 4 thru_hole oval (at -3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A2-IDE))
    (pad 5 thru_hole oval (at -1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A0-IDE))
    (pad 6 thru_hole oval (at 1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A1-IDE))
    (pad 7 thru_hole oval (at 3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /*IOR-IDE))
    (pad 8 thru_hole oval (at 6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /*IOW-IDE))
    (pad 9 thru_hole oval (at 8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /*RESET))
    (pad 10 thru_hole oval (at 11.43 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 11 thru_hole oval (at 11.43 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(U4-Pad11)"))
    (pad 12 thru_hole oval (at 8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /*IOW-ISA))
    (pad 13 thru_hole oval (at 6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 *IOR-ISA))
    (pad 14 thru_hole oval (at 3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A1-ISA))
    (pad 15 thru_hole oval (at 1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(J3-Pad2)"))
    (pad 16 thru_hole oval (at -1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A2-ISA))
    (pad 17 thru_hole oval (at -3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /7))
    (pad 18 thru_hole oval (at -6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /6))
    (pad 19 thru_hole oval (at -8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 20 thru_hole oval (at -11.43 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dip_sockets:DIP-14__300_ELL (layer Component) (tedit 5726CA03)
    (at 164.465 60.325 270)
    (descr "14 pins DIL package, elliptical pads")
    (tags DIL)
    (fp_text reference U5 (at 12.065 1.905 360) (layer F.SilkS))
    (fp_text value 74LS04 (at 1.27 1.27 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -7.62 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(J2-Pad2)"))
    (pad 2 thru_hole oval (at -5.08 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U5-Pad2)"))
    (pad 3 thru_hole oval (at -2.54 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 91 RESDRV))
    (pad 4 thru_hole oval (at 0 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(U4-Pad11)"))
    (pad 5 thru_hole oval (at 2.54 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U5-Pad5)"))
    (pad 6 thru_hole oval (at 5.08 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 /5))
    (pad 7 thru_hole oval (at 7.62 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 8 thru_hole oval (at 7.62 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /3))
    (pad 9 thru_hole oval (at 5.08 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U5-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U5-Pad10)"))
    (pad 11 thru_hole oval (at 0 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(U5-Pad11)"))
    (pad 12 thru_hole oval (at -2.54 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(R4-Pad2)"))
    (pad 13 thru_hole oval (at -5.08 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 86 *DASP))
    (pad 14 thru_hole oval (at -7.62 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dip_sockets:DIP-20__300_ELL (layer Component) (tedit 57264EC4)
    (at 104.14 104.14 270)
    (descr "20 pins DIL package, elliptical pads")
    (tags DIL)
    (fp_text reference U6 (at 15.875 1.905 360) (layer F.SilkS))
    (fp_text value 74LS688 (at 3.556 1.016 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 AEN))
    (pad 2 thru_hole oval (at -8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 A9))
    (pad 3 thru_hole oval (at -6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(RP1-Pad3)"))
    (pad 4 thru_hole oval (at -3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 A8))
    (pad 5 thru_hole oval (at -1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(RP1-Pad4)"))
    (pad 6 thru_hole oval (at 1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 A7))
    (pad 7 thru_hole oval (at 3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(RP1-Pad5)"))
    (pad 8 thru_hole oval (at 6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 9 thru_hole oval (at 8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 10 thru_hole oval (at 11.43 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 11 thru_hole oval (at 11.43 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 12 thru_hole oval (at 8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 13 thru_hole oval (at 6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 82 A4))
    (pad 14 thru_hole oval (at 3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(RP1-Pad8)"))
    (pad 15 thru_hole oval (at 1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 A5))
    (pad 16 thru_hole oval (at -1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(RP1-Pad7)"))
    (pad 17 thru_hole oval (at -3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 A6))
    (pad 18 thru_hole oval (at -6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(RP1-Pad6)"))
    (pad 19 thru_hole oval (at -8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 /CS_IDE))
    (pad 20 thru_hole oval (at -11.43 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dip_sockets:DIP-16__300_ELL (layer Component) (tedit 5726CAB0)
    (at 176.53 59.055 270)
    (descr "16 pins DIL package, elliptical pads")
    (tags DIL)
    (fp_text reference U7 (at 13.335 1.905 360) (layer F.SilkS))
    (fp_text value 74LS138 (at 1.27 1.27 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /*IOW-ISA))
    (pad 2 thru_hole oval (at -6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 *IOR-ISA))
    (pad 3 thru_hole oval (at -3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(J2-Pad2)"))
    (pad 4 thru_hole oval (at -1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 /CS_IDE))
    (pad 5 thru_hole oval (at 1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(J3-Pad2)"))
    (pad 6 thru_hole oval (at 3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U5-Pad10)"))
    (pad 7 thru_hole oval (at 6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 9 thru_hole oval (at 8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U5-Pad9)"))
    (pad 10 thru_hole oval (at 6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 /4))
    (pad 11 thru_hole oval (at 3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at -1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /2))
    (pad 14 thru_hole oval (at -3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U5-Pad5)"))
    (pad 15 thru_hole oval (at -6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole oval (at -8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dip_sockets:DIP-14__300_ELL (layer Component) (tedit 57277F72)
    (at 152.4 60.325 270)
    (descr "14 pins DIL package, elliptical pads")
    (tags DIL)
    (fp_text reference U8 (at 12.065 1.905 360) (layer F.SilkS))
    (fp_text value 74LS32 (at 6.35 -1.27 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -7.62 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 /CS_IDE))
    (pad 2 thru_hole oval (at -5.08 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U5-Pad2)"))
    (pad 3 thru_hole oval (at -2.54 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /6))
    (pad 4 thru_hole oval (at 0 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(J2-Pad2)"))
    (pad 5 thru_hole oval (at 2.54 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 /CS_IDE))
    (pad 6 thru_hole oval (at 5.08 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /7))
    (pad 7 thru_hole oval (at 7.62 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 8 thru_hole oval (at 7.62 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(U5-Pad11)"))
    (pad 9 thru_hole oval (at 5.08 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A2-ISA))
    (pad 10 thru_hole oval (at 2.54 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A1-ISA))
    (pad 11 thru_hole oval (at 0 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at -2.54 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 13 thru_hole oval (at -5.08 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 14 thru_hole oval (at -7.62 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dip_sockets:DIP-20__300_ELL (layer Component) (tedit 572780C6)
    (at 160.02 104.14 270)
    (descr "20 pins DIL package, elliptical pads")
    (tags DIL)
    (fp_text reference U9 (at 15.875 1.905 360) (layer F.SilkS))
    (fp_text value 74LS688 (at -8.255 -1.27 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(R2-Pad2)"))
    (pad 2 thru_hole oval (at -8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(RP2-Pad3)"))
    (pad 3 thru_hole oval (at -6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 A16))
    (pad 4 thru_hole oval (at -3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(RP2-Pad4)"))
    (pad 5 thru_hole oval (at -1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 A15))
    (pad 6 thru_hole oval (at 1.27 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(RP2-Pad5)"))
    (pad 7 thru_hole oval (at 3.81 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(RP2-Pad7)"))
    (pad 8 thru_hole oval (at 6.35 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(RP2-Pad6)"))
    (pad 9 thru_hole oval (at 8.89 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(RP2-Pad8)"))
    (pad 10 thru_hole oval (at 11.43 3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 11 thru_hole oval (at 11.43 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 12 thru_hole oval (at 8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 13 thru_hole oval (at 6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 14 thru_hole oval (at 3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 A17))
    (pad 15 thru_hole oval (at 1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 16 thru_hole oval (at -1.27 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 73 A18))
    (pad 17 thru_hole oval (at -3.81 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 18 thru_hole oval (at -6.35 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 A19))
    (pad 19 thru_hole oval (at -8.89 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 //CS_ROM))
    (pad 20 thru_hole oval (at -11.43 -3.81 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dip_sockets:DIP-28__600_ELL (layer Component) (tedit 57277F58)
    (at 123.19 99.06 270)
    (descr "28 pins DIL package, elliptical pads, width 600mil")
    (tags DIL)
    (fp_text reference U10 (at 20.955 5.08 360) (layer F.SilkS))
    (fp_text value 28C256 (at 8.89 4.445 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -16.51 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 A14))
    (pad 2 thru_hole oval (at -13.97 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A12))
    (pad 3 thru_hole oval (at -11.43 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 A7))
    (pad 4 thru_hole oval (at -8.89 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 A6))
    (pad 5 thru_hole oval (at -6.35 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 A5))
    (pad 6 thru_hole oval (at -3.81 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 82 A4))
    (pad 7 thru_hole oval (at -1.27 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A3))
    (pad 8 thru_hole oval (at 1.27 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A2-ISA))
    (pad 9 thru_hole oval (at 3.81 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A1-ISA))
    (pad 10 thru_hole oval (at 6.35 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A0-ISA))
    (pad 11 thru_hole oval (at 8.89 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /PC-DB0))
    (pad 12 thru_hole oval (at 11.43 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /PC-DB1))
    (pad 13 thru_hole oval (at 13.97 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /PC-DB2))
    (pad 14 thru_hole oval (at 16.51 7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 15 thru_hole oval (at 16.51 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /PC-DB3))
    (pad 16 thru_hole oval (at 13.97 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /PC-DB4))
    (pad 17 thru_hole oval (at 11.43 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /PC-DB5))
    (pad 18 thru_hole oval (at 8.89 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /PC-DB6))
    (pad 19 thru_hole oval (at 6.35 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /PC-DB7))
    (pad 20 thru_hole oval (at 3.81 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 //CS_ROM))
    (pad 21 thru_hole oval (at 1.27 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A10))
    (pad 22 thru_hole oval (at -1.27 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /*MEMR))
    (pad 23 thru_hole oval (at -3.81 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A11))
    (pad 24 thru_hole oval (at -6.35 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 A9))
    (pad 25 thru_hole oval (at -8.89 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 A8))
    (pad 26 thru_hole oval (at -11.43 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 A13))
    (pad 27 thru_hole oval (at -13.97 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 /ROM_WE))
    (pad 28 thru_hole oval (at -16.51 -7.62 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (model dil/dil_28-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Component) (tedit 572649B6)
    (at 147.32 85.09 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R7 (at 12.7 0 180) (layer F.SilkS))
    (fp_text value 10K (at 5.08 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 48 VCC))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 59 /ROM_WE))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Component) (tedit 572649BB)
    (at 137.16 87.63)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at -2.54 0) (layer F.SilkS))
    (fp_text value 10K (at 5.08 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 48 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 58 "Net-(R2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Array_SIP9 (layer Component) (tedit 5726500C)
    (at 95.25 104.14 270)
    (descr "Connecteur 10 pins")
    (tags "CONN DEV")
    (fp_text reference RP1 (at 13.97 0 360) (layer F.SilkS))
    (fp_text value 10K (at -11.43 1.905 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -11.43 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 2 thru_hole circle (at -8.89 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -6.35 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(RP1-Pad3)"))
    (pad 4 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(RP1-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(RP1-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(RP1-Pad6)"))
    (pad 7 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(RP1-Pad7)"))
    (pad 8 thru_hole circle (at 6.35 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(RP1-Pad8)"))
    (pad 9 thru_hole circle (at 8.89 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at 11.43 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model Resistors_ThroughHole.3dshapes/Resistor_Array_SIP9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Array_SIP9 (layer Component) (tedit 57265009)
    (at 151.13 104.14 270)
    (descr "Connecteur 10 pins")
    (tags "CONN DEV")
    (fp_text reference RP2 (at 13.97 0 360) (layer F.SilkS))
    (fp_text value 10K (at -11.43 1.905 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -11.43 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 2 thru_hole circle (at -8.89 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 90 D7))
    (pad 3 thru_hole circle (at -6.35 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(RP2-Pad3)"))
    (pad 4 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(RP2-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(RP2-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(RP2-Pad6)"))
    (pad 7 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(RP2-Pad7)"))
    (pad 8 thru_hole circle (at 6.35 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(RP2-Pad8)"))
    (pad 9 thru_hole circle (at 8.89 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at 11.43 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model Resistors_ThroughHole.3dshapes/Resistor_Array_SIP9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dips-s:DIPS-DS08 (layer Component) (tedit 5726502C)
    (at 142.24 106.68 270)
    (tags "dip switch")
    (fp_text reference SW1 (at 12.7 3.175 360) (layer F.SilkS))
    (fp_text value "ROM OPT" (at -12.7 0 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8.89 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 2 thru_hole circle (at -6.35 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 3 thru_hole circle (at -3.81 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 4 thru_hole circle (at -1.27 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 5 thru_hole circle (at 1.27 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 56 A14))
    (pad 6 thru_hole circle (at 3.81 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 57 A13))
    (pad 7 thru_hole circle (at 6.35 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 55 AEN))
    (pad 8 thru_hole circle (at 8.89 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 54 *MEMW))
    (pad 9 thru_hole circle (at 8.89 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 59 /ROM_WE))
    (pad 10 thru_hole circle (at 6.35 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(R2-Pad2)"))
    (pad 11 thru_hole circle (at 3.81 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(RP2-Pad8)"))
    (pad 12 thru_hole circle (at 1.27 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(RP2-Pad7)"))
    (pad 13 thru_hole circle (at -1.27 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(RP2-Pad6)"))
    (pad 14 thru_hole circle (at -3.81 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(RP2-Pad5)"))
    (pad 15 thru_hole circle (at -6.35 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(RP2-Pad4)"))
    (pad 16 thru_hole circle (at -8.89 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(RP2-Pad3)"))
    (model dips/dips-ds08.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dips-s:DIPS-DS08 (layer Component) (tedit 57264F5A)
    (at 86.36 106.68 270)
    (tags "dip switch")
    (fp_text reference SW2 (at 12.7 3.175 360) (layer F.SilkS))
    (fp_text value "I/O ADDR" (at -12.7 0 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8.89 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 2 thru_hole circle (at -6.35 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 3 thru_hole circle (at -3.81 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 4 thru_hole circle (at -1.27 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 5 thru_hole circle (at 1.27 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 6 thru_hole circle (at 3.81 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 7 thru_hole circle (at 6.35 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at 8.89 3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole circle (at 8.89 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at 6.35 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole circle (at 3.81 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(RP1-Pad8)"))
    (pad 12 thru_hole circle (at 1.27 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(RP1-Pad7)"))
    (pad 13 thru_hole circle (at -1.27 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(RP1-Pad6)"))
    (pad 14 thru_hole circle (at -3.81 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(RP1-Pad5)"))
    (pad 15 thru_hole circle (at -6.35 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(RP1-Pad4)"))
    (pad 16 thru_hole circle (at -8.89 -3.81 270) (size 1.778 1.778) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(RP1-Pad3)"))
    (model dips/dips-ds08.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Component) (tedit 572649AF)
    (at 137.16 82.55)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference C6 (at -2.54 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 5.08 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 48 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x20 (layer Component) (tedit 5726CEA6)
    (at 85.09 88.265 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference IDE1 (at 5.08 15.24 270) (layer F.SilkS) hide)
    (fp_text value CONN_20X2 (at 5.08 2.54 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /*RESET))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 90 D7))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D8))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 94 D6))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D9))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 95 D5))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /D10))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 96 D4))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /D11))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 97 D3))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /D12))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 98 D2))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D13))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 99 D1))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D14))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 100 D0))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D15))
    (pad 19 thru_hole oval (at 0 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 20 thru_hole oval (at 2.54 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /VCC_CF))
    (pad 21 thru_hole oval (at 0 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 22 thru_hole oval (at 2.54 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 23 thru_hole oval (at 0 27.94 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /*IOW-IDE))
    (pad 24 thru_hole oval (at 2.54 27.94 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 25 thru_hole oval (at 0 30.48 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /*IOR-IDE))
    (pad 26 thru_hole oval (at 2.54 30.48 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 27 thru_hole oval (at 0 33.02 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 28 thru_hole oval (at 2.54 33.02 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 29 thru_hole oval (at 0 35.56 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 30 thru_hole oval (at 2.54 35.56 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 31 thru_hole oval (at 0 38.1 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /INTRQ))
    (pad 32 thru_hole oval (at 2.54 38.1 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 33 thru_hole oval (at 0 40.64 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A1-IDE))
    (pad 34 thru_hole oval (at 2.54 40.64 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 35 thru_hole oval (at 0 43.18 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A0-IDE))
    (pad 36 thru_hole oval (at 2.54 43.18 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A2-IDE))
    (pad 37 thru_hole oval (at 0 45.72 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /*CS1FX))
    (pad 38 thru_hole oval (at 2.54 45.72 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /*CS3FX))
    (pad 39 thru_hole oval (at 0 48.26 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 86 *DASP))
    (pad 40 thru_hole oval (at 2.54 48.26 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer Component) (tedit 5726CDDD)
    (at 86.36 123.825 270)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C11 (at 4.445 3.81 360) (layer F.SilkS))
    (fp_text value 47uF (at 1.25 4.4 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-5MM (layer Component) (tedit 572FD59B)
    (at 175.895 40.64)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D1 (at -2.54 -2.54) (layer F.SilkS))
    (fp_text value LED (at -2.54 -2.54) (layer F.Fab) hide)
    (fp_text user K (at -1.905 1.905) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mounting:120mil_no_silkscreen (layer Component) (tedit 57277139)
    (at 186.69 128.27)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P6 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
  )
  (module mounting:120mil_no_silkscreen (layer Component) (tedit 57277139)
    (at 186.69 71.755)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P7 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
  )
  (module headers_with_detent:1x2 (layer Component) (tedit 5727882C)
    (at 101.6 82.55 270)
    (descr "Connecteur 3 pins")
    (tags "CONN DEV")
    (fp_text reference J1 (at 0 3.81 360) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 -3.937 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 VCC))
    (pad 2 thru_hole circle (at 0 1.27 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /VCC_CF))
    (model pins_array_3x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module headers_with_detent:1x3 (layer Component) (tedit 57277862)
    (at 148.59 40.513)
    (descr "Connecteur 3 pins")
    (tags "CONN DEV")
    (fp_text reference J2 (at -2.54 3.175) (layer F.SilkS))
    (fp_text value CONN_3 (at 0 -4.953) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 -2.413 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A3))
    (pad 2 thru_hole circle (at 0 0.127 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.667 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A0-ISA))
    (model pins_array_3x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module headers_with_detent:1x3 (layer Component) (tedit 57277866)
    (at 156.21 40.513)
    (descr "Connecteur 3 pins")
    (tags "CONN DEV")
    (fp_text reference J3 (at -2.54 3.175) (layer F.SilkS))
    (fp_text value CONN_3 (at 0 -4.953) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 -2.413 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A0-ISA))
    (pad 2 thru_hole circle (at 0 0.127 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(J3-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.667 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A3))
    (model pins_array_3x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module headers_with_detent:5x2 (layer Component) (tedit 5727788F)
    (at 107.95 127)
    (descr "Double rangee de contacts 2 x 5 pins")
    (tags CONN)
    (fp_text reference J4 (at -7.62 1.905) (layer F.SilkS))
    (fp_text value INTERRUPT (at 0 -5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -5.08 1.27) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 92 IRQ2))
    (pad 2 thru_hole circle (at -5.08 -1.27) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /INTRQ))
    (pad 3 thru_hole circle (at -2.54 1.27) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /IRQ3))
    (pad 4 thru_hole circle (at -2.54 -1.27) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /INTRQ))
    (pad 5 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /IRQ4))
    (pad 6 thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /INTRQ))
    (pad 7 thru_hole circle (at 2.54 1.27) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /IRQ5))
    (pad 8 thru_hole circle (at 2.54 -1.27) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /INTRQ))
    (pad 9 thru_hole circle (at 5.08 1.27) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /IRQ7))
    (pad 10 thru_hole circle (at 5.08 -1.27) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /INTRQ))
    (model pin_array/pins_array_5x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer Component) (tedit 57277956)
    (at 108.585 75.311)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082) (layer F.Fab) hide)
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Component) (tedit 57367E74)
    (at 186.055 50.165 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R4 (at 12.7 0 540) (layer F.SilkS))
    (fp_text value 470R (at 5.08 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 89 "Net-(J5-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 87 "Net-(R4-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module headers_with_detent:1x2 (layer Component) (tedit 573676F2)
    (at 184.785 40.64 90)
    (descr "Connecteur 3 pins")
    (tags "CONN DEV")
    (fp_text reference J5 (at -3.175 -1.27 180) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 -3.937 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 2 thru_hole circle (at 0 1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(J5-Pad2)"))
    (model pins_array_3x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module edge_connectors:ISA-8BIT-XT-IDE (layer Component) (tedit 57461671)
    (at 127 137.16)
    (descr "Connecteur Bus PC 8 bits")
    (tags "CONN PC ISA")
    (fp_text reference BUS1 (at 37.084 -6.35) (layer F.SilkS) hide)
    (fp_text value BUSPC (at -36.322 -6.35) (layer F.SilkS) hide)
    (pad 1 connect rect (at 38.1 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 47 GND))
    (pad 2 connect rect (at 35.56 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 91 RESDRV))
    (pad 3 connect rect (at 33.02 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 48 VCC))
    (pad 4 connect rect (at 30.48 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 92 IRQ2))
    (pad 8 connect rect (at 20.32 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 102 /CARDSEL))
    (pad 11 connect rect (at 12.7 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 54 *MEMW))
    (pad 12 connect rect (at 10.16 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 6 /*MEMR))
    (pad 13 connect rect (at 7.62 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 5 /*IOW-ISA))
    (pad 14 connect rect (at 5.08 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 93 *IOR-ISA))
    (pad 21 connect rect (at -12.7 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 37 /IRQ7))
    (pad 23 connect rect (at -17.78 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 36 /IRQ5))
    (pad 24 connect rect (at -20.32 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 35 /IRQ4))
    (pad 25 connect rect (at -22.86 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 34 /IRQ3))
    (pad 29 connect rect (at -33.02 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 48 VCC))
    (pad 31 connect rect (at -38.1 -0.254) (size 1.778 7.112) (layers Copper B.Mask)
      (net 47 GND))
    (pad 33 connect rect (at 35.56 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 45 /PC-DB7))
    (pad 34 connect rect (at 33.02 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 44 /PC-DB6))
    (pad 35 connect rect (at 30.48 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 43 /PC-DB5))
    (pad 36 connect rect (at 27.94 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 42 /PC-DB4))
    (pad 37 connect rect (at 25.4 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 41 /PC-DB3))
    (pad 38 connect rect (at 22.86 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 40 /PC-DB2))
    (pad 39 connect rect (at 20.32 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 39 /PC-DB1))
    (pad 40 connect rect (at 17.78 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 38 /PC-DB0))
    (pad 42 connect rect (at 12.7 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 55 AEN))
    (pad 43 connect rect (at 10.16 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 72 A19))
    (pad 44 connect rect (at 7.62 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 73 A18))
    (pad 45 connect rect (at 5.08 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 74 A17))
    (pad 46 connect rect (at 2.54 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 75 A16))
    (pad 47 connect rect (at 0 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 76 A15))
    (pad 48 connect rect (at -2.54 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 56 A14))
    (pad 49 connect rect (at -5.08 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 57 A13))
    (pad 50 connect rect (at -7.62 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 21 /A12))
    (pad 51 connect rect (at -10.16 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 20 /A11))
    (pad 52 connect rect (at -12.7 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 19 /A10))
    (pad 53 connect rect (at -15.24 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 77 A9))
    (pad 54 connect rect (at -17.78 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 78 A8))
    (pad 55 connect rect (at -20.32 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 79 A7))
    (pad 56 connect rect (at -22.86 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 80 A6))
    (pad 57 connect rect (at -25.4 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 81 A5))
    (pad 58 connect rect (at -27.94 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 82 A4))
    (pad 59 connect rect (at -30.48 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 24 /A3))
    (pad 60 connect rect (at -33.02 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 23 /A2-ISA))
    (pad 61 connect rect (at -35.56 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 18 /A1-ISA))
    (pad 62 connect rect (at -38.1 -0.254) (size 1.778 7.112) (layers Component F.Mask)
      (net 16 /A0-ISA))
  )
  (module Connect:PINTST (layer Component) (tedit 574618F5)
    (at 147.32 121.285)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP1 (at 2.54 0) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 102 /CARDSEL))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 56.515 (width 0.254) (layer Dwgs.User)
    (gr_text "2.2250 in" (at 194.31 100.0125 270) (layer Dwgs.User))
    (feature1 (pts (xy 186.69 128.27) (xy 195.58 128.27)))
    (feature2 (pts (xy 186.69 71.755) (xy 195.58 71.755)))
    (crossbar (pts (xy 193.04 71.755) (xy 193.04 128.27)))
    (arrow1a (pts (xy 193.04 128.27) (xy 192.453579 127.143496)))
    (arrow1b (pts (xy 193.04 128.27) (xy 193.626421 127.143496)))
    (arrow2a (pts (xy 193.04 71.755) (xy 192.453579 72.881504)))
    (arrow2b (pts (xy 193.04 71.755) (xy 193.626421 72.881504)))
  )
  (dimension 19.05 (width 0.254) (layer Dwgs.User)
    (gr_text "0.7500 in" (at 177.165 137.16) (layer Dwgs.User))
    (feature1 (pts (xy 167.64 135.255) (xy 167.64 135.255)))
    (feature2 (pts (xy 186.69 135.255) (xy 186.69 135.255)))
    (crossbar (pts (xy 186.69 135.255) (xy 167.64 135.255)))
    (arrow1a (pts (xy 167.64 135.255) (xy 168.766504 134.668579)))
    (arrow1b (pts (xy 167.64 135.255) (xy 168.766504 135.841421)))
    (arrow2a (pts (xy 186.69 135.255) (xy 185.563496 134.668579)))
    (arrow2b (pts (xy 186.69 135.255) (xy 185.563496 135.841421)))
  )
  (gr_text + (at 186.055 43.561) (layer F.SilkS))
  (gr_text "XT-IDE rev 03 - 2016 Glitch Works Respin\nhttp://www.glitchwrks.com/xt-ide" (at 112.395 76.2) (layer F.SilkS))
  (gr_text "J1 CLOSED FOR +5 ON PIN 20" (at 88.265 85.725) (layer F.SilkS))
  (gr_text "2-3 HI SPEED" (at 158.115 43.18) (layer F.SilkS))
  (gr_text "1-2 COMPAT" (at 158.115 38.1) (layer F.SilkS))
  (gr_text 8K (at 133.985 110.49) (layer F.SilkS))
  (gr_text 8K (at 133.985 107.95) (layer F.SilkS))
  (gr_text A13 (at 133.985 105.41) (layer F.SilkS))
  (gr_text A14 (at 133.985 102.87) (layer F.SilkS))
  (gr_text A15 (at 133.985 100.33) (layer F.SilkS))
  (gr_text A16 (at 133.985 97.79) (layer F.SilkS))
  (gr_text ENA (at 133.985 113.03) (layer F.SilkS))
  (gr_text WR (at 133.985 115.57) (layer F.SilkS))
  (gr_text A4 (at 78.74 110.49) (layer F.SilkS))
  (gr_text A5 (at 78.74 107.95) (layer F.SilkS))
  (gr_text A6 (at 78.74 105.41) (layer F.SilkS))
  (gr_text A7 (at 78.74 102.87) (layer F.SilkS))
  (gr_text A8 (at 78.74 100.33) (layer F.SilkS))
  (gr_text A9 (at 78.74 97.79) (layer F.SilkS))
  (gr_text 2 (at 102.87 123.19) (layer F.SilkS))
  (gr_text 7 (at 113.03 123.19) (layer F.SilkS))
  (gr_text 5 (at 110.49 123.19) (layer F.SilkS))
  (gr_text 4 (at 107.95 123.19) (layer F.SilkS))
  (gr_text 3 (at 105.41 123.19) (layer F.SilkS))
  (gr_line (start 77.47 132.08) (end 77.47 34.29) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 86.36 132.08) (end 77.47 132.08) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 191.135 34.29) (end 77.47 34.29) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 191.135 132.08) (end 191.135 34.29) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 177.8 132.08) (end 191.135 132.08) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 167.64 132.08) (end 177.8 132.08) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 167.64 140.97) (end 167.64 132.08) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 86.36 140.97) (end 167.64 140.97) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 86.36 132.08) (end 86.36 140.97) (angle 90) (layer Edge.Cuts) (width 0.381))
  (zone (net 47) (net_name GND) (layer Copper) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.69 131.445) (xy 178.435 131.445) (xy 178.435 131.445) (xy 78.105 131.445) (xy 78.105 34.925)
        (xy 190.5 34.925) (xy 190.5 131.445)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 140.97) (xy 86.36 140.97) (xy 86.36 132.715) (xy 167.64 132.715) (xy 167.64 140.97)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 140.97) (xy 86.36 140.97) (xy 86.36 132.715) (xy 167.64 132.715) (xy 167.64 140.97)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Eco1.User) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 140.97) (xy 86.36 140.97) (xy 86.36 132.715) (xy 167.64 132.715) (xy 167.64 140.97)
      )
    )
  )
)
