Run install.bat or follow the manual installation instructions below.

Manual installation instructions
--------------------------------
1. Copy the SBPCI folder to your c:\ drive
2. Copy the provided autoexec.bat file to your c:\ drive or edit your current one.
3. Copy the provided config.sys file to your c:\ drive or edit your current one.
4. If you have any problems getting your setup to work make sure your card is 
supported and view the important notes below.



The SBPCI.zip archive contains the dos sound card drivers for all Sound Blaster 
pci cards (excluding SBLive! and Audigy Models). They are setup and optimized 
for ArcadeOS and MAME but they should work well with any legacy dos game.

SBPCI.zip supports the following Sound Blaster PCI cards
-------------------------------------------------------------
SB Audio PCI 128
Creative AudioPCI
Sound Blaster 16 PCI
Sound Blaster PCI 128
Sound Blaster AudioPCI
Creative Ensoniq AudioPCI
Creative Vibra 128
Any of the following chipsets: 1371, 1373, 5880



Important Notes:

1. Your sound blaster pci card can not use irq 5.
2. Your sound blaster pci card should not use the same irq as your video card.
3. You must first uninstall your current sound blaster dos drivers in windows 
for the SBPCI drivers to work. Go to: 
Start/Settings/Control Panel/Add Remove Programs/Your Sound Card