***********************************************************************

                WINDOWS NT DRIVER SETUP INFORMATION
                               for
                      Trident 94x0 AGi Users


***********************************************************************
Windows NT Device Drivers Version 1.00                   Oct. 19, 1994
***********************************************************************

Contents

1.0     Introduction
2.0     Supported Resolutions
3.0     Installation Notes for Windows NT Version 3.1

*****************************

1.0     Introduction

This Accelerate Driver runs on the following products:

     Trident 94x0 AGi, VESA or PCI local bus adapter

The Graphics Device Drivers supplied here are for the Microsoft
Windows NT operating system version 3.1.

*****************************

2.0     Supported Resolutions.

                    16 colors     256 colors    65000 colors    16.7 million
     Resolutions    4 bpp         8 bpp         16 bpp          24 bpp

     640 x  480     0.5/1/2MB     0.5/1/2MB         1/2MB           1/2MB
     800 x  600     0.5/1/2MB     0.5/1/2MB         1/2MB             2MB
    1024 x  768     0.5/1/2MB         1/2MB         1/2MB             N/A
    1280 x 1024     1/2MB               2MB           N/A             N/A
    1600 x 1200     1/2MB               2MB           N/A             N/A

.5/1/4MB -  Supported on 0.5, 1 or 2 Megabyte trident 94x0 AGi products
N/A      -  Not Supported

****************************

3.0     Installation Notes for Windows NT

This driver package containing:

  - AGI.SYS             (Trident AGi graphics miniport driver)
  - AGI.DLL             (Trident AGi graphics display  driver)
  - OEMSETUP.INF        (setup files used by Windows NT Setup program)
  - README              This README file for Windows NT Version 3.1

Windows NT drivers are included on Disk #2 of this package.  They are
located in the \NT31 sub-directory.

Procedure:

1. Run the Windows NT Setup program located in Main group of Program
   Manager.

2. Select Change System Setting under the Options pulldown menu.

3. Select Other (Requires a disk from hard manufacturer) next to the
   display options.

4. Windows NT will prompt you for the correct path. Enter A:\NT31 if disk 2
   is loaded in drive A:.

5. A list of all modes will appear; select the resolution and color
   depth desired.

6. Restart Windows NT.  Windows NT will now use the Trident AGi drivers.

Note: If a color depth or resolution that is not supported by your
      card is selected, Windows NT will substitute 640x480, 256 colors mode
      as the current display mode.

