	<< Trident TGUI9440AGi PCI VGA Card WINDOWS 95 Driver >>

Introduction
============

  Windows 95 is the operation system  with Plug&Play feature  and  will
  auto-detect your card's configuration and set it. The user don't need
  to do anything for the adapter configuration.

Installation Procedures
=======================

 1. When log into Windows 95, click on the "Start" icon, then move the
    mouse to "Settings" icon and click on the "Control Panel".

 2. In the Control Panel window, click on the "Display" icon.

 3. In the Display Properties dialog box, choose the "Setting" item.
 
 4. Click the "Change Display Type..." button.

 5. Select "Adapter Type / Change..." item.

 6. In the Select Device dialog box, select "Have Disk..." item.

 7. Insert the driver diskette into drive A, and then click "OK" button.

 8. Select the "Trident 9440, Linear Accelerated For PCI V3.01.04",
    and then click "OK" button.

 9. Windows 95 would perform driver installation.
