(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 201)
    (no_connects 0)
    (area 56.995288 16.35 257.964715 154.634001)
    (thickness 1.6)
    (drawings 49)
    (tracks 751)
    (zones 0)
    (modules 61)
    (nets 98)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.0254)
    (user_trace_width 0.3048)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.0254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.27)
    (via_drill 0.635)
    (via_min_size 0.635)
    (via_min_drill 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerb/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 /CV)
  (net 4 +12VA)
  (net 5 -12VA)
  (net 6 "Net-(C6-Pad2)")
  (net 7 "Net-(C7-Pad2)")
  (net 8 "Net-(C7-Pad1)")
  (net 9 "Net-(C8-Pad2)")
  (net 10 "Net-(C9-Pad2)")
  (net 11 "Net-(C10-Pad1)")
  (net 12 "Net-(C10-Pad2)")
  (net 13 "Net-(C11-Pad2)")
  (net 14 "Net-(C12-Pad2)")
  (net 15 "Net-(C13-Pad1)")
  (net 16 "Net-(C14-Pad1)")
  (net 17 "Net-(C15-Pad1)")
  (net 18 "Net-(C17-Pad2)")
  (net 19 "Net-(C17-Pad1)")
  (net 20 "Net-(C18-Pad2)")
  (net 21 /IRQ3)
  (net 22 "Net-(P1-Pad2)")
  (net 23 /IRQ5)
  (net 24 /IRQ2)
  (net 25 /0x218)
  (net 26 /0x388)
  (net 27 /0x288)
  (net 28 /0x318)
  (net 29 "Net-(Q1-Pad2)")
  (net 30 /~IRQ)
  (net 31 "Net-(R4-Pad1)")
  (net 32 "Net-(R8-Pad1)")
  (net 33 "Net-(R14-Pad2)")
  (net 34 "Net-(J1-Pad3)")
  (net 35 "Net-(J1-Pad2)")
  (net 36 /OSC_14M3)
  (net 37 "Net-(U1-Pad12)")
  (net 38 "Net-(U1-Pad7)")
  (net 39 "Net-(U1-Pad9)")
  (net 40 /MCLK)
  (net 41 /A1)
  (net 42 /A2)
  (net 43 /A5)
  (net 44 /A6)
  (net 45 /A3)
  (net 46 "Net-(U2-Pad7)")
  (net 47 "Net-(U2-Pad9)")
  (net 48 "Net-(U2-Pad10)")
  (net 49 "Net-(U2-Pad11)")
  (net 50 "Net-(U2-Pad12)")
  (net 51 "Net-(U2-Pad13)")
  (net 52 "Net-(U2-Pad14)")
  (net 53 "Net-(U2-Pad15)")
  (net 54 /A4)
  (net 55 /A7)
  (net 56 /A8)
  (net 57 /AEN)
  (net 58 /A9)
  (net 59 "Net-(U3-Pad7)")
  (net 60 "Net-(U3-Pad11)")
  (net 61 "Net-(U3-Pad12)")
  (net 62 "Net-(U3-Pad15)")
  (net 63 /~READ)
  (net 64 /D0)
  (net 65 /D1)
  (net 66 /D2)
  (net 67 /D3)
  (net 68 /D4)
  (net 69 /D5)
  (net 70 /D6)
  (net 71 /DB5)
  (net 72 /DB4)
  (net 73 /DB3)
  (net 74 /DB2)
  (net 75 /DB1)
  (net 76 /DB0)
  (net 77 /D7)
  (net 78 /DB7)
  (net 79 /DB6)
  (net 80 /~IOR)
  (net 81 "Net-(U5-Pad11)")
  (net 82 /~IOW)
  (net 83 "Net-(U5-Pad6)")
  (net 84 /~WRITE)
  (net 85 /~RESET)
  (net 86 /RESET)
  (net 87 /A0)
  (net 88 "Net-(U6-Pad20)")
  (net 89 "Net-(U6-Pad21)")
  (net 90 "Net-(U6-Pad23)")
  (net 91 "Net-(U7-Pad2)")
  (net 92 /MP)
  (net 93 "Net-(U9-Pad1)")
  (net 94 "Net-(U9-Pad8)")
  (net 95 "Net-(J1-Pad4)")
  (net 96 "Net-(J1-Pad5)")
  (net 97 "Net-(R2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.3048)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12VA)
    (add_net -12VA)
    (add_net /0x218)
    (add_net /0x288)
    (add_net /0x318)
    (add_net /0x388)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /AEN)
    (add_net /CV)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /DB0)
    (add_net /DB1)
    (add_net /DB2)
    (add_net /DB3)
    (add_net /DB4)
    (add_net /DB5)
    (add_net /DB6)
    (add_net /DB7)
    (add_net /IRQ2)
    (add_net /IRQ3)
    (add_net /IRQ5)
    (add_net /MCLK)
    (add_net /MP)
    (add_net /OSC_14M3)
    (add_net /RESET)
    (add_net /~IOR)
    (add_net /~IOW)
    (add_net /~IRQ)
    (add_net /~READ)
    (add_net /~RESET)
    (add_net /~WRITE)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U5-Pad11)")
    (add_net "Net-(U5-Pad6)")
    (add_net "Net-(U6-Pad20)")
    (add_net "Net-(U6-Pad21)")
    (add_net "Net-(U6-Pad23)")
    (add_net "Net-(U7-Pad2)")
    (add_net "Net-(U9-Pad1)")
    (add_net "Net-(U9-Pad8)")
    (add_net VCC)
  )
  (module adlib:JACK_CUI_SJ1-3553NG (layer F.Cu) (tedit 5775EC76)
    (at 195.152 80.01 180)
    (fp_text reference J1 (at 2.874 -7.366 180) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 -11.557 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 2.5 180) (size 2.54 2.032) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 -2.5 180) (size 2.54 2.032) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(J1-Pad5)"))
    (pad 3 thru_hole oval (at 0 -5 180) (size 2.54 2.032) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 5 180) (size 2.54 2.032) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J1-Pad2)"))
    (pad 1 thru_hole oval (at -5 0 180) (size 2.032 2.54) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 0 thru_hole circle (at 0 0 180) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole circle (at -5 5 180) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole circle (at -5 -5 180) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS))
  )
  (module adlib:DIP600_24N (layer F.Cu) (tedit 5775DA58)
    (at 156.21 102.235)
    (fp_text reference U6 (at 0 1.651) (layer F.SilkS))
    (fp_text value YM3812 (at 13.462 -7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 /~IRQ))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 85 /~RESET))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 87 /A0))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 84 /~WRITE))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 63 /~READ))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 /0x388))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 27.94 -15.24) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 74 /DB2))
    (pad 14 thru_hole circle (at 25.4 -15.24) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 73 /DB3))
    (pad 15 thru_hole circle (at 22.86 -15.24) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 72 /DB4))
    (pad 16 thru_hole circle (at 20.32 -15.24) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 71 /DB5))
    (pad 17 thru_hole circle (at 17.78 -15.24) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 79 /DB6))
    (pad 18 thru_hole circle (at 15.24 -15.24) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 78 /DB7))
    (pad 19 thru_hole circle (at 12.7 -15.24) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 20 thru_hole circle (at 10.16 -15.24) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(U6-Pad20)"))
    (pad 9 thru_hole circle (at 20.32 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at 22.86 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 76 /DB0))
    (pad 11 thru_hole circle (at 25.4 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 75 /DB1))
    (pad 12 thru_hole circle (at 27.94 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 21 thru_hole circle (at 7.62 -15.24) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(U6-Pad21)"))
    (pad 22 thru_hole circle (at 5.08 -15.24) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole circle (at 2.54 -15.24) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(U6-Pad23)"))
    (pad 24 thru_hole circle (at 0 -15.24) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 40 /MCLK))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 5775DBF0)
    (at 156.845 66.675 90)
    (fp_text reference C4 (at -5.08 -0.0635 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +12VA))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 5775DBF0)
    (at 153.67 66.675 90)
    (fp_text reference C5 (at -4.8895 -0.0635 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 -12VA))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 -12VA))
  )
  (module adlib:DIOA500 (layer F.Cu) (tedit 5775DC25)
    (at 109.22 93.345 90)
    (fp_text reference D1 (at 8.255 0 180) (layer F.SilkS))
    (fp_text value D (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C11-Pad2)"))
    (pad 2 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:JMP3 (layer F.Cu) (tedit 577601A0)
    (at 130.81 105.41)
    (fp_text reference P1 (at 0 -3.302) (layer F.SilkS) hide)
    (fp_text value IRQ (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /IRQ3))
    (pad 2 thru_hole rect (at -2.54 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P1-Pad2)"))
    (pad 3 thru_hole rect (at 0 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /IRQ5))
    (pad 4 thru_hole rect (at 0 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P1-Pad2)"))
    (pad 5 thru_hole rect (at 2.54 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /IRQ2))
    (pad 6 thru_hole rect (at 2.54 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P1-Pad2)"))
  )
  (module adlib:JMP4 (layer F.Cu) (tedit 5776019D)
    (at 144.78 105.41)
    (fp_text reference P2 (at 0.381 -3.683) (layer F.SilkS) hide)
    (fp_text value ADDR (at -3.81 -3.04) (layer F.Fab))
    (pad 1 thru_hole rect (at -3.81 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /0x218))
    (pad 2 thru_hole rect (at -3.81 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /0x388))
    (pad 3 thru_hole rect (at -1.27 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /0x288))
    (pad 4 thru_hole rect (at -1.27 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /0x388))
    (pad 5 thru_hole rect (at 1.27 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /0x318))
    (pad 6 thru_hole rect (at 1.27 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /0x388))
    (pad 7 thru_hole rect (at 3.81 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /0x388))
    (pad 8 thru_hole rect (at 3.81 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /0x388))
  )
  (module adlib:TO92-IL (layer F.Cu) (tedit 5775E08B)
    (at 129.54 48.895 180)
    (fp_text reference Q1 (at 2.8575 0.254 180) (layer F.SilkS))
    (fp_text value 2N3904 (at -6.35 -2.54 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C12-Pad2)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 121.285 97.155 90)
    (fp_text reference R1 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value 8.2K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /~IRQ))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 117.475 80.645 90)
    (fp_text reference R2 (at -8.255 0 180) (layer F.SilkS))
    (fp_text value 2.2K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(R2-Pad2)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 121.285 80.645 90)
    (fp_text reference R3 (at -8.255 0 180) (layer F.SilkS))
    (fp_text value 2.2K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C6-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C7-Pad2)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 135.255 80.645 90)
    (fp_text reference R4 (at -8.255 0.0635 180) (layer F.SilkS))
    (fp_text value 12K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(R4-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C7-Pad1)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 132.715 80.645 90)
    (fp_text reference R5 (at -8.3185 0.0635 180) (layer F.SilkS))
    (fp_text value 10K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(R4-Pad1)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 124.46 80.645 90)
    (fp_text reference R6 (at -8.255 0 180) (layer F.SilkS))
    (fp_text value 2.2K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C9-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C7-Pad1)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 128.27 64.77 90)
    (fp_text reference R7 (at 8.763 0 90) (layer F.SilkS))
    (fp_text value 2.2K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C8-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C9-Pad2)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 117.475 64.77 270)
    (fp_text reference R8 (at -0.1905 2.54 360) (layer F.SilkS))
    (fp_text value 1.5K (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(R8-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C10-Pad1)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 124.46 64.77 90)
    (fp_text reference R9 (at 8.89 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(R8-Pad1)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 140.335 52.07 90)
    (fp_text reference R10 (at -5.842 -2.9845 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C10-Pad2)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 143.51 52.07 90)
    (fp_text reference R11 (at 8.4455 0.0635 180) (layer F.SilkS))
    (fp_text value 2.2K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C12-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C10-Pad2)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 112.395 93.345 90)
    (fp_text reference R12 (at 8.255 0 180) (layer F.SilkS))
    (fp_text value 2.2K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C11-Pad2)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 152.4 52.07 90)
    (fp_text reference R13 (at -8.255 0 180) (layer F.SilkS))
    (fp_text value 8.2K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C12-Pad2)"))
  )
  (module adlib:RESV_BOURNS_91A1A (layer F.Cu) (tedit 5775E654)
    (at 182.5625 54.61)
    (fp_text reference R14 (at -2.2225 9.525) (layer F.SilkS))
    (fp_text value POT (at 0.381 -10.033) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(R14-Pad2)"))
    (pad 3 thru_hole circle (at 0 -2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C13-Pad1)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 165.735 49.53 90)
    (fp_text reference R15 (at -8.382 0.0635 360) (layer F.SilkS))
    (fp_text value 10 (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C17-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 171.45 36.83 90)
    (fp_text reference R16 (at -9.0805 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C18-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 175.26 36.83 270)
    (fp_text reference R18 (at 9.144 0.0635 270) (layer F.SilkS))
    (fp_text value 10 (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at -6.35 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C18-Pad2)"))
  )
  (module adlib:RESA500 (layer F.Cu) (tedit 5775DBBF)
    (at 179.07 36.83 270)
    (fp_text reference R19 (at 9.144 0.0635 270) (layer F.SilkS))
    (fp_text value 10 (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J1-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C18-Pad2)"))
  )
  (module adlib:DIP300_16N (layer F.Cu) (tedit 5775D7AA)
    (at 76.835 117.475)
    (fp_text reference U1 (at 0 1.651) (layer F.SilkS))
    (fp_text value 74LS109 (at 5.461 -1.651) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 36 /OSC_14M3))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(U1-Pad12)"))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole circle (at 17.78 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at 15.24 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 40 /MCLK))
    (pad 11 thru_hole circle (at 12.7 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 12 thru_hole circle (at 10.16 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at 7.62 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 14 thru_hole circle (at 5.08 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 15 thru_hole circle (at 2.54 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 16 thru_hole circle (at 0 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
  )
  (module adlib:DIP300_16N (layer F.Cu) (tedit 5775D7AA)
    (at 105.41 117.475)
    (fp_text reference U2 (at 0 1.651) (layer F.SilkS))
    (fp_text value 74LS138 (at 5.461 -1.651) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 41 /A1))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 42 /A2))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 43 /A5))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 44 /A6))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 45 /A3))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U2-Pad7)"))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole circle (at 17.78 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U2-Pad9)"))
    (pad 10 thru_hole circle (at 15.24 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U2-Pad10)"))
    (pad 11 thru_hole circle (at 12.7 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U2-Pad11)"))
    (pad 12 thru_hole circle (at 10.16 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U2-Pad12)"))
    (pad 13 thru_hole circle (at 7.62 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U2-Pad13)"))
    (pad 14 thru_hole circle (at 5.08 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U2-Pad14)"))
    (pad 15 thru_hole circle (at 2.54 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(U2-Pad15)"))
    (pad 16 thru_hole circle (at 0 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
  )
  (module adlib:DIP300_16N (layer F.Cu) (tedit 5775D7AA)
    (at 130.81 117.475)
    (fp_text reference U3 (at 0 1.651) (layer F.SilkS))
    (fp_text value 74LS138 (at 5.461 -1.651) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 54 /A4))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 55 /A7))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 56 /A8))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 57 /AEN))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(U2-Pad15)"))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 58 /A9))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(U3-Pad7)"))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole circle (at 17.78 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 /0x388))
    (pad 10 thru_hole circle (at 15.24 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 28 /0x318))
    (pad 11 thru_hole circle (at 12.7 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(U3-Pad11)"))
    (pad 12 thru_hole circle (at 10.16 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(U3-Pad12)"))
    (pad 13 thru_hole circle (at 7.62 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 /0x288))
    (pad 14 thru_hole circle (at 5.08 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 /0x218))
    (pad 15 thru_hole circle (at 2.54 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(U3-Pad15)"))
    (pad 16 thru_hole circle (at 0 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
  )
  (module adlib:DIP300_20N (layer F.Cu) (tedit 5775D895)
    (at 156.21 117.475)
    (fp_text reference U4 (at 0 1.651) (layer F.SilkS))
    (fp_text value 74LS245 (at 11.303 -3.683) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 63 /~READ))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 64 /D0))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 65 /D1))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 66 /D2))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 67 /D3))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 68 /D4))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 69 /D5))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 70 /D6))
    (pad 13 thru_hole circle (at 17.78 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 71 /DB5))
    (pad 14 thru_hole circle (at 15.24 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 72 /DB4))
    (pad 15 thru_hole circle (at 12.7 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 73 /DB3))
    (pad 16 thru_hole circle (at 10.16 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 74 /DB2))
    (pad 17 thru_hole circle (at 7.62 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 75 /DB1))
    (pad 18 thru_hole circle (at 5.08 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 76 /DB0))
    (pad 19 thru_hole circle (at 2.54 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 /0x388))
    (pad 20 thru_hole circle (at 0 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 9 thru_hole circle (at 20.32 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 77 /D7))
    (pad 10 thru_hole circle (at 22.86 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 11 thru_hole circle (at 22.86 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 78 /DB7))
    (pad 12 thru_hole circle (at 20.32 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 79 /DB6))
  )
  (module adlib:DIP300_14N (layer F.Cu) (tedit 5775D6A3)
    (at 130.81 98.425)
    (fp_text reference U5 (at 13.97 -9.525) (layer F.SilkS))
    (fp_text value 74LS04 (at 7.366 -3.683) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 /~IRQ))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 80 /~IOR))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(U5-Pad11)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 82 /~IOW))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(U5-Pad6)"))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 84 /~WRITE))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(U5-Pad6)"))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 63 /~READ))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(U5-Pad11)"))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 85 /~RESET))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 86 /RESET))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
  )
  (module adlib:DIP300_8N (layer F.Cu) (tedit 5775D8F2)
    (at 156.21 81.915)
    (fp_text reference U7 (at 0 1.651) (layer F.SilkS))
    (fp_text value YM3014B (at 3.937 -3.683) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(U7-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(U6-Pad20)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(U6-Pad21)"))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(U6-Pad23)"))
    (pad 6 thru_hole circle (at 5.08 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole circle (at 2.54 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /CV))
    (pad 8 thru_hole circle (at 0 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 92 /MP))
  )
  (module adlib:DIP300_14N (layer F.Cu) (tedit 5775D6A3)
    (at 133.35 70.485)
    (fp_text reference U8 (at 0.635 1.905) (layer F.SilkS))
    (fp_text value RC4136 (at 7.366 -3.683) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(R4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C6-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C7-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(R2-Pad2)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(U7-Pad2)"))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(R2-Pad2)"))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 -12VA))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 92 /MP))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /CV))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 92 /MP))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 +12VA))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C10-Pad1)"))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C8-Pad2)"))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(R8-Pad1)"))
  )
  (module adlib:DIP300_8N (layer F.Cu) (tedit 5775D8F2)
    (at 149.86 41.148)
    (fp_text reference U9 (at -0.0635 -9.398) (layer F.SilkS))
    (fp_text value LM386N (at 3.937 -3.683) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(U9-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C14-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(R14-Pad2)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(C17-Pad1)"))
    (pad 6 thru_hole circle (at 5.08 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 +12VA))
    (pad 7 thru_hole circle (at 2.54 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C15-Pad1)"))
    (pad 8 thru_hole circle (at 0 -7.62) (size 1.5748 1.5748) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(U9-Pad8)"))
  )
  (module adlib:CAPA1000 (layer F.Cu) (tedit 5775DE06)
    (at 140.97 36.83 180)
    (fp_text reference C18 (at 25.4 -1.905 180) (layer F.SilkS))
    (fp_text value 10uF (at 13.208 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(C17-Pad1)"))
    (pad 2 thru_hole circle (at 25.4 0 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C18-Pad2)"))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 127.635 113.665 90)
    (fp_text reference C24 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 153.035 78.105 90)
    (fp_text reference C2 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 153.035 113.665 90)
    (fp_text reference C25 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 100.33 113.665 90)
    (fp_text reference C20 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 73.025 113.665 90)
    (fp_text reference C19 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 127 94.615 90)
    (fp_text reference C26 (at 0 -2.159 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 187.96 99.695 90)
    (fp_text reference C1 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 128.27 84.455 90)
    (fp_text reference C7 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 4700pF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C7-Pad2)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C7-Pad2)"))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 128.27 76.835 90)
    (fp_text reference C6 (at 4.445 1.905 180) (layer F.SilkS))
    (fp_text value 4700pF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C6-Pad2)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C6-Pad2)"))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 121.285 68.58 90)
    (fp_text reference C9 (at -3.81 -2.159 180) (layer F.SilkS))
    (fp_text value 4700pF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C9-Pad2)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C9-Pad2)"))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 121.285 60.96 90)
    (fp_text reference C8 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 4700pF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C8-Pad2)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C8-Pad2)"))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 147.955 55.88 90)
    (fp_text reference C12 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 1000pF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C12-Pad2)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C12-Pad2)"))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 147.955 48.26 90)
    (fp_text reference C14 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C14-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 161.925 37.465 90)
    (fp_text reference C16 (at 5.715 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +12VA))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +12VA))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 165.735 37.465 90)
    (fp_text reference C17 (at 5.715 0 90) (layer F.SilkS))
    (fp_text value 0.047uF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C17-Pad2)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(C17-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C17-Pad2)"))
  )
  (module adlib:CAP23 (layer F.Cu) (tedit 577823F9)
    (at 178.435 54.61 90)
    (fp_text reference C13 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 270pF (at 0 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:CAPAP200 (layer F.Cu) (tedit 57785228)
    (at 182.88 111.125 270)
    (fp_text reference C23 (at 6.985 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 2.54 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:CAPAP200 (layer F.Cu) (tedit 57785228)
    (at 189.865 117.475 270)
    (fp_text reference C21 (at 6.985 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 2.54 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 -12VA))
  )
  (module adlib:CAPAP200 (layer F.Cu) (tedit 57785228)
    (at 194.945 117.475 270)
    (fp_text reference C22 (at 6.985 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 2.54 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +12VA))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:CAPAP200 (layer F.Cu) (tedit 57785228)
    (at 105.41 94.615 270)
    (fp_text reference C11 (at -1.905 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 2.54 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C11-Pad2)"))
  )
  (module adlib:CAPAP200 (layer F.Cu) (tedit 57785228)
    (at 167.7035 75.565 270)
    (fp_text reference C3 (at 6.985 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 2.54 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /CV))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:CAPAP200 (layer F.Cu) (tedit 57785228)
    (at 135.89 48.895 270)
    (fp_text reference C10 (at -2.286 0 360) (layer F.SilkS))
    (fp_text value 4.7uF (at 2.54 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C10-Pad2)"))
  )
  (module adlib:CAPAP200 (layer F.Cu) (tedit 57785228)
    (at 145.415 34.925 270)
    (fp_text reference C15 (at -2.286 -0.127 360) (layer F.SilkS))
    (fp_text value 10uF (at 2.54 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C15-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module adlib:MNT_SPARE locked (layer F.Cu) (tedit 5778660A)
    (at 77.47 45.72)
    (attr virtual)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MNT_SPARE (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.9464 2.9464) (drill 2.9464) (layers *.Cu *.Mask F.SilkS))
  )
  (module adlib:BUS_PC_ADLIB (layer F.Cu) (tedit 5792B9FD)
    (at 140.97 130.81)
    (descr "Connecteur Bus AT ISA 16 bits")
    (tags "CONN BUS ISA")
    (fp_text reference BUS1 (at -22.86 -6.985) (layer F.SilkS) hide)
    (fp_text value BUSPC (at -43.815 -6.985) (layer F.Fab))
    (pad 1 connect rect (at 38.1 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 2 connect rect (at 35.56 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 86 /RESET))
    (pad 3 connect rect (at 33.02 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 2 VCC))
    (pad 4 connect rect (at 30.48 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 24 /IRQ2))
    (pad 7 connect rect (at 22.86 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 5 -12VA))
    (pad 9 connect rect (at 17.78 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 4 +12VA))
    (pad 10 connect rect (at 15.24 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 13 connect rect (at 7.62 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 82 /~IOW))
    (pad 14 connect rect (at 5.08 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 80 /~IOR))
    (pad 23 connect rect (at -17.78 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 23 /IRQ5))
    (pad 25 connect rect (at -22.86 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 21 /IRQ3))
    (pad 29 connect rect (at -33.02 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 2 VCC))
    (pad 30 connect rect (at -35.56 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 36 /OSC_14M3))
    (pad 31 connect rect (at -38.1 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 33 connect rect (at 35.56 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 77 /D7))
    (pad 34 connect rect (at 33.02 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 70 /D6))
    (pad 35 connect rect (at 30.48 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 69 /D5))
    (pad 36 connect rect (at 27.94 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 68 /D4))
    (pad 37 connect rect (at 25.4 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 67 /D3))
    (pad 38 connect rect (at 22.86 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 66 /D2))
    (pad 39 connect rect (at 20.32 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 65 /D1))
    (pad 40 connect rect (at 17.78 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 64 /D0))
    (pad 42 connect rect (at 12.7 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 57 /AEN))
    (pad 53 connect rect (at -15.24 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 58 /A9))
    (pad 54 connect rect (at -17.78 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 56 /A8))
    (pad 55 connect rect (at -20.32 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 55 /A7))
    (pad 56 connect rect (at -22.86 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 44 /A6))
    (pad 57 connect rect (at -25.4 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 43 /A5))
    (pad 58 connect rect (at -27.94 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 54 /A4))
    (pad 59 connect rect (at -30.48 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 45 /A3))
    (pad 60 connect rect (at -33.02 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 42 /A2))
    (pad 61 connect rect (at -35.56 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 41 /A1))
    (pad 62 connect rect (at -38.1 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 87 /A0))
  )
  (module adlib:MNT_KEYSTONE_9202 (layer F.Cu) (tedit 5792B570)
    (at 199.771 66.04)
    (fp_text reference MNT1 (at 0 0.889) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.2766 3.2766) (drill 3.2766) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 56.515) (size 3.2766 3.2766) (drill 3.2766) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model "C:/Data/Projects/Adlib/mech/keystone 9202.wrl"
      (at (xyz 0.24 -3.475 0.255))
      (scale (xyz 10 10 10))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 7.055683 (width 0.3) (layer Dwgs.User)
    (gr_text "0.2778 in" (at 231.790059 87.264047 0.0702587102) (layer Dwgs.User))
    (feature1 (pts (xy 235.312049 82.489377) (xy 235.319554 88.60972)))
    (feature2 (pts (xy 228.256371 82.498029) (xy 228.263876 88.618372)))
    (crossbar (pts (xy 228.260565 85.918374) (xy 235.316243 85.909722)))
    (arrow1a (pts (xy 235.316243 85.909722) (xy 234.190459 86.497524)))
    (arrow1b (pts (xy 235.316243 85.909722) (xy 234.189021 85.324683)))
    (arrow2a (pts (xy 228.260565 85.918374) (xy 229.387787 86.503413)))
    (arrow2b (pts (xy 228.260565 85.918374) (xy 229.386349 85.330572)))
  )
  (dimension 46.482 (width 0.3) (layer Dwgs.User)
    (gr_text "1.8300 in" (at 252.429 56.769 270) (layer Dwgs.User))
    (feature1 (pts (xy 241.681 80.01) (xy 253.779 80.01)))
    (feature2 (pts (xy 241.681 33.528) (xy 253.779 33.528)))
    (crossbar (pts (xy 251.079 33.528) (xy 251.079 80.01)))
    (arrow1a (pts (xy 251.079 80.01) (xy 250.492579 78.883496)))
    (arrow1b (pts (xy 251.079 80.01) (xy 251.665421 78.883496)))
    (arrow2a (pts (xy 251.079 33.528) (xy 250.492579 34.654504)))
    (arrow2b (pts (xy 251.079 33.528) (xy 251.665421 34.654504)))
  )
  (dimension 21.082 (width 0.3) (layer Dwgs.User)
    (gr_text "0.8300 in" (at 247.603 44.069 270) (layer Dwgs.User))
    (feature1 (pts (xy 241.554 54.61) (xy 248.953 54.61)))
    (feature2 (pts (xy 241.554 33.528) (xy 248.953 33.528)))
    (crossbar (pts (xy 246.253 33.528) (xy 246.253 54.61)))
    (arrow1a (pts (xy 246.253 54.61) (xy 245.666579 53.483496)))
    (arrow1b (pts (xy 246.253 54.61) (xy 246.839421 53.483496)))
    (arrow2a (pts (xy 246.253 33.528) (xy 245.666579 34.654504)))
    (arrow2b (pts (xy 246.253 33.528) (xy 246.839421 34.654504)))
  )
  (dimension 8.763 (width 0.3) (layer Dwgs.User)
    (gr_text "0.3450 in" (at 236.1565 72.31955) (layer Dwgs.User))
    (feature1 (pts (xy 231.775 76.962) (xy 231.775 70.96955)))
    (feature2 (pts (xy 240.538 76.962) (xy 240.538 70.96955)))
    (crossbar (pts (xy 240.538 73.66955) (xy 231.775 73.66955)))
    (arrow1a (pts (xy 231.775 73.66955) (xy 232.901504 73.083129)))
    (arrow1b (pts (xy 231.775 73.66955) (xy 232.901504 74.255971)))
    (arrow2a (pts (xy 240.538 73.66955) (xy 239.411496 73.083129)))
    (arrow2b (pts (xy 240.538 73.66955) (xy 239.411496 74.255971)))
  )
  (dimension 7.055683 (width 0.3) (layer Dwgs.User)
    (gr_text "0.2778 in" (at 228.750043 61.651262 0.0702587102) (layer Dwgs.User))
    (feature1 (pts (xy 232.272033 56.876592) (xy 232.279538 62.996935)))
    (feature2 (pts (xy 225.216355 56.885244) (xy 225.22386 63.005587)))
    (crossbar (pts (xy 225.220549 60.305589) (xy 232.276227 60.296937)))
    (arrow1a (pts (xy 232.276227 60.296937) (xy 231.150443 60.884739)))
    (arrow1b (pts (xy 232.276227 60.296937) (xy 231.149005 59.711898)))
    (arrow2a (pts (xy 225.220549 60.305589) (xy 226.347771 60.890628)))
    (arrow2b (pts (xy 225.220549 60.305589) (xy 226.346333 59.717787)))
  )
  (dimension 11.811 (width 0.3) (layer Dwgs.User)
    (gr_text "0.4650 in" (at 234.6325 45.64) (layer Dwgs.User))
    (feature1 (pts (xy 240.538 50.673) (xy 240.538 44.29)))
    (feature2 (pts (xy 228.727 50.673) (xy 228.727 44.29)))
    (crossbar (pts (xy 228.727 46.99) (xy 240.538 46.99)))
    (arrow1a (pts (xy 240.538 46.99) (xy 239.411496 47.576421)))
    (arrow1b (pts (xy 240.538 46.99) (xy 239.411496 46.403579)))
    (arrow2a (pts (xy 228.727 46.99) (xy 229.853504 47.576421)))
    (arrow2b (pts (xy 228.727 46.99) (xy 229.853504 46.403579)))
  )
  (dimension 106.68 (width 0.3) (layer Dwgs.User)
    (gr_text "4.2000 in" (at 62.531001 81.28 270) (layer Dwgs.User))
    (feature1 (pts (xy 67.945 134.62) (xy 61.181001 134.62)))
    (feature2 (pts (xy 67.945 27.94) (xy 61.181001 27.94)))
    (crossbar (pts (xy 63.881001 27.94) (xy 63.881001 134.62)))
    (arrow1a (pts (xy 63.881001 134.62) (xy 63.29458 133.493496)))
    (arrow1b (pts (xy 63.881001 134.62) (xy 64.467422 133.493496)))
    (arrow2a (pts (xy 63.881001 27.94) (xy 63.29458 29.066504)))
    (arrow2b (pts (xy 63.881001 27.94) (xy 64.467422 29.066504)))
  )
  (gr_text A (at 100.711 124.206) (layer F.SilkS))
  (gr_text 31 (at 102.87 122.047) (layer F.SilkS))
  (gr_text 1 (at 179.07 122.047) (layer F.SilkS))
  (gr_line (start 181.61 133.35) (end 181.61 128.27) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.34 134.62) (end 181.61 133.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 134.62) (end 180.34 134.62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.33 133.35) (end 101.6 134.62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.33 128.27) (end 100.33 133.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.2 127) (end 182.88 127) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.2 27.94) (end 203.2 127) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.945 27.94) (end 203.2 27.94) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.945 127) (end 67.945 27.94) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.06 127) (end 67.945 127) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 99.06 128.27) (end 99.06 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 182.88 128.27) (end 181.61 128.27) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text D (at 148.59 101.854) (layer F.SilkS))
  (gr_text C (at 146.05 101.854) (layer F.SilkS))
  (gr_text B (at 143.51 101.854) (layer F.SilkS))
  (gr_text A (at 140.97 101.854) (layer F.SilkS))
  (gr_text 2 (at 133.35 101.854) (layer F.SilkS))
  (gr_text 5 (at 130.81 101.854) (layer F.SilkS))
  (gr_text 3 (at 128.27 101.854) (layer F.SilkS))
  (gr_text "Replica of 1990 Ad Lib" (at 71.12 32.385) (layer F.SilkS))
  (dimension 135.255 (width 0.3) (layer Dwgs.User)
    (gr_text "5.3250 in" (at 135.5725 17.7) (layer Dwgs.User))
    (feature1 (pts (xy 203.2 27.94) (xy 203.2 16.35)))
    (feature2 (pts (xy 67.945 27.94) (xy 67.945 16.35)))
    (crossbar (pts (xy 67.945 19.05) (xy 203.2 19.05)))
    (arrow1a (pts (xy 203.2 19.05) (xy 202.073496 19.636421)))
    (arrow1b (pts (xy 203.2 19.05) (xy 202.073496 18.463579)))
    (arrow2a (pts (xy 67.945 19.05) (xy 69.071504 19.636421)))
    (arrow2b (pts (xy 67.945 19.05) (xy 69.071504 18.463579)))
  )
  (dimension 23.495 (width 0.3) (layer Dwgs.User)
    (gr_text "0.9250 in" (at 193.3575 138.128999) (layer Dwgs.User))
    (feature1 (pts (xy 205.105 132.08) (xy 205.105 139.478999)))
    (feature2 (pts (xy 181.61 132.08) (xy 181.61 139.478999)))
    (crossbar (pts (xy 181.61 136.778999) (xy 205.105 136.778999)))
    (arrow1a (pts (xy 205.105 136.778999) (xy 203.978496 137.36542)))
    (arrow1b (pts (xy 205.105 136.778999) (xy 203.978496 136.192578)))
    (arrow2a (pts (xy 181.61 136.778999) (xy 182.736504 137.36542)))
    (arrow2b (pts (xy 181.61 136.778999) (xy 182.736504 136.192578)))
  )
  (dimension 81.280025 (width 0.3) (layer Dwgs.User)
    (gr_text "3.2000 in" (at 140.967828 138.066143 359.9552377) (layer Dwgs.User))
    (feature1 (pts (xy 181.61 135.3185) (xy 181.606774 139.447893)))
    (feature2 (pts (xy 100.33 135.255) (xy 100.326774 139.384393)))
    (crossbar (pts (xy 100.328883 136.684394) (xy 181.608883 136.747894)))
    (arrow1a (pts (xy 181.608883 136.747894) (xy 180.481921 137.333434)))
    (arrow1b (pts (xy 181.608883 136.747894) (xy 180.482838 136.160593)))
    (arrow2a (pts (xy 100.328883 136.684394) (xy 101.454928 137.271695)))
    (arrow2b (pts (xy 100.328883 136.684394) (xy 101.455845 136.098854)))
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.52 92.075) (xy 115.57 92.075) (xy 118.11 89.535) (xy 150.495 89.535) (xy 151.13 88.9)
        (xy 151.13 86.36) (xy 151.765 85.725) (xy 153.035 84.455) (xy 184.15 84.455) (xy 184.785 85.09)
        (xy 187.325 87.63) (xy 187.325 93.98) (xy 189.865 96.52) (xy 189.865 110.49) (xy 188.595 111.76)
        (xy 188.595 127) (xy 203.2 127) (xy 203.2 27.94) (xy 96.52 27.94)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.06 127) (xy 99.568 127.127) (xy 99.949 127.381) (xy 100.203 127.762) (xy 100.33 128.27)
        (xy 100.33 133.35) (xy 101.6 134.62) (xy 180.34 134.62) (xy 181.61 133.35) (xy 181.61 128.143)
        (xy 181.864 127.508) (xy 182.372 127.127) (xy 182.88 127)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.039639 127) (xy 99.547639 127.127) (xy 99.928639 127.381) (xy 100.182639 127.762) (xy 100.309639 128.27)
        (xy 100.309639 133.35) (xy 101.579639 134.62) (xy 180.319639 134.62) (xy 181.589639 133.35) (xy 181.589639 128.143)
        (xy 181.843639 127.508) (xy 182.351639 127.127) (xy 182.859639 127)
      )
    )
  )
)
