(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 644)
    (no_connects 0)
    (area 25.130762 14.064001 328.840544 149.554001)
    (thickness 1.6)
    (drawings 138)
    (tracks 3530)
    (zones 0)
    (modules 199)
    (nets 216)
  )
  (page A4)
  (title_block
    (title "Snark Barker SB 1.0 Clone")
    (comment 1 "Copyright (C) 2018 Eric Schlaepfer")
    (comment 2 "License. See https://creativecommons.org/licenses/by-sa/4.0/")
    (comment 3 "This work is licensed under a Creative Commons Attribution-ShareAlike 4.0 International")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.3048)
    (user_trace_width 0.635)
    (trace_clearance 0.254)
    (zone_clearance 0.635)
    (zone_45_only no)
    (trace_min 0.3048)
    (segment_width 0.254)
    (edge_width 0.15)
    (via_size 1.143)
    (via_drill 0.5842)
    (via_min_size 1.143)
    (via_min_drill 0.5842)
    (user_via 1.143 0.5842)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF69)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory fab/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 GND)
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C3-Pad2)")
  (net 7 "Net-(C4-Pad2)")
  (net 8 +9VA)
  (net 9 "Net-(C10-Pad1)")
  (net 10 "Net-(C11-Pad2)")
  (net 11 "Net-(C12-Pad2)")
  (net 12 "Net-(C13-Pad1)")
  (net 13 "Net-(C14-Pad1)")
  (net 14 "Net-(C14-Pad2)")
  (net 15 "Net-(C15-Pad1)")
  (net 16 "Net-(C20-Pad1)")
  (net 17 "Net-(C21-Pad1)")
  (net 18 "Net-(C22-Pad1)")
  (net 19 "Net-(C23-Pad1)")
  (net 20 /BUTTON1)
  (net 21 /BUTTON4)
  (net 22 "Net-(C26-Pad1)")
  (net 23 "Net-(C27-Pad1)")
  (net 24 /BUTTON3)
  (net 25 /BUTTON2)
  (net 26 "Net-(C30-Pad1)")
  (net 27 "Net-(C30-Pad2)")
  (net 28 "Net-(C31-Pad1)")
  (net 29 "Net-(C31-Pad2)")
  (net 30 "Net-(C32-Pad2)")
  (net 31 "Net-(C35-Pad1)")
  (net 32 "Net-(C36-Pad1)")
  (net 33 "Net-(C37-Pad2)")
  (net 34 "Net-(C38-Pad1)")
  (net 35 "Net-(C38-Pad2)")
  (net 36 "Net-(C39-Pad1)")
  (net 37 "Net-(C40-Pad1)")
  (net 38 "Net-(C40-Pad2)")
  (net 39 "Net-(C42-Pad1)")
  (net 40 "Net-(C42-Pad2)")
  (net 41 "Net-(C43-Pad1)")
  (net 42 "Net-(C43-Pad2)")
  (net 43 +5VA)
  (net 44 "Net-(C49-Pad2)")
  (net 45 /DIGITAL_OUT)
  (net 46 "Net-(C51-Pad2)")
  (net 47 "Net-(C52-Pad2)")
  (net 48 "Net-(C54-Pad1)")
  (net 49 "Net-(C55-Pad1)")
  (net 50 /OPL2)
  (net 51 /SAA_R)
  (net 52 "Net-(C59-Pad1)")
  (net 53 /SAA_L)
  (net 54 "Net-(C61-Pad1)")
  (net 55 "Net-(C62-Pad1)")
  (net 56 "Net-(C63-Pad1)")
  (net 57 /~ISA_WR)
  (net 58 "Net-(C65-Pad1)")
  (net 59 /DREQUEST)
  (net 60 /~RESET)
  (net 61 /RESET)
  (net 62 VCC)
  (net 63 "Net-(C78-Pad1)")
  (net 64 /~DSP_WRITE)
  (net 65 "Net-(C89-Pad1)")
  (net 66 "Net-(D1-Pad1)")
  (net 67 "Net-(D2-Pad2)")
  (net 68 /DRQ1)
  (net 69 "Net-(IO1-Pad1)")
  (net 70 "Net-(IO1-Pad10)")
  (net 71 "Net-(IO1-Pad3)")
  (net 72 "Net-(IO1-Pad5)")
  (net 73 "Net-(IO1-Pad7)")
  (net 74 "Net-(IO1-Pad11)")
  (net 75 "Net-(IO1-Pad9)")
  (net 76 /IRQ2)
  (net 77 /IRQ3)
  (net 78 /IRQ5)
  (net 79 /IRQ7)
  (net 80 /BUSRESET)
  (net 81 /~IOW)
  (net 82 /~IOR)
  (net 83 /~DACK1)
  (net 84 /CLK_14M318)
  (net 85 /DB7)
  (net 86 /DB6)
  (net 87 /DB5)
  (net 88 /DB4)
  (net 89 /DB3)
  (net 90 /DB2)
  (net 91 /DB1)
  (net 92 /DB0)
  (net 93 /IO_READY)
  (net 94 /AEN)
  (net 95 /A9)
  (net 96 /A8)
  (net 97 /A7)
  (net 98 /A6)
  (net 99 /A5)
  (net 100 /A4)
  (net 101 /A3)
  (net 102 /A2)
  (net 103 /A1)
  (net 104 /A0)
  (net 105 /JOYSTICK_~CS)
  (net 106 /X1)
  (net 107 /Y1)
  (net 108 /X2)
  (net 109 /MIDI_OUT)
  (net 110 /Y2)
  (net 111 /MIDI_IN)
  (net 112 "Net-(R1-Pad1)")
  (net 113 "Net-(R2-Pad1)")
  (net 114 "Net-(R10-Pad2)")
  (net 115 "Net-(R17-Pad1)")
  (net 116 "Net-(R18-Pad1)")
  (net 117 /MIC_COMP)
  (net 118 /MUTE_EN)
  (net 119 "Net-(R34-Pad2)")
  (net 120 "Net-(R35-Pad2)")
  (net 121 "Net-(R38-Pad1)")
  (net 122 "Net-(R39-Pad2)")
  (net 123 "Net-(R40-Pad2)")
  (net 124 "Net-(R41-Pad2)")
  (net 125 "Net-(R44-Pad2)")
  (net 126 "Net-(RP2-Pad2)")
  (net 127 "Net-(RP2-Pad3)")
  (net 128 "Net-(RP2-Pad4)")
  (net 129 "Net-(RP2-Pad5)")
  (net 130 "Net-(RXD1-Pad3)")
  (net 131 "Net-(TXD1-Pad3)")
  (net 132 "Net-(U1-Pad11)")
  (net 133 /~IC)
  (net 134 /~RD)
  (net 135 /D0)
  (net 136 /D7)
  (net 137 /D6)
  (net 138 /D5)
  (net 139 /D4)
  (net 140 /D3)
  (net 141 /D2)
  (net 142 /D1)
  (net 143 /~DB_EN)
  (net 144 "Net-(U24-Pad3)")
  (net 145 /1xx000xxxx)
  (net 146 /~CARD_SELECTED)
  (net 147 /DAV_~CS)
  (net 148 /DSPRD_~CS)
  (net 149 /FM_~CS)
  (net 150 /DSPRST_~CS)
  (net 151 /CMS7-12_~CS)
  (net 152 /CMS1-6_~CS)
  (net 153 /DSPWR_~CS)
  (net 154 /~WR)
  (net 155 "Net-(U10-Pad3)")
  (net 156 "Net-(U10-Pad2)")
  (net 157 "Net-(U10-Pad4)")
  (net 158 "Net-(U10-Pad5)")
  (net 159 "Net-(U10-Pad8)")
  (net 160 /DAC7)
  (net 161 /DAC6)
  (net 162 /DAC5)
  (net 163 /DAC2)
  (net 164 /DAC1)
  (net 165 /DAC0)
  (net 166 /DAC4)
  (net 167 /DAC3)
  (net 168 /IREQUEST)
  (net 169 /DSP_BUSY)
  (net 170 /~DMA_EN)
  (net 171 /~DSP_READ)
  (net 172 /DAV_PC)
  (net 173 /DAV_DSP)
  (net 174 /DD7)
  (net 175 /DD6)
  (net 176 /DD5)
  (net 177 /DD4)
  (net 178 /DD3)
  (net 179 /DD2)
  (net 180 /DD1)
  (net 181 /DD0)
  (net 182 /CLK_7M159)
  (net 183 /~111000xxxx)
  (net 184 /~100jjjxxxx)
  (net 185 "Net-(U16-Pad10)")
  (net 186 /~100000xxxx)
  (net 187 /~ISA_RD)
  (net 188 "Net-(U20-Pad1)")
  (net 189 "Net-(U20-Pad5)")
  (net 190 "Net-(U20-Pad9)")
  (net 191 "Net-(U20-Pad10)")
  (net 192 "Net-(U20-Pad11)")
  (net 193 "Net-(U20-Pad12)")
  (net 194 /~RD_DAV)
  (net 195 "Net-(U21-Pad4)")
  (net 196 "Net-(U21-Pad5)")
  (net 197 "Net-(U23-Pad2)")
  (net 198 /CLK_3M579)
  (net 199 "Net-(U23-Pad12)")
  (net 200 "Net-(U24-Pad11)")
  (net 201 /~DMAOUT)
  (net 202 "Net-(U26-Pad5)")
  (net 203 "Net-(U26-Pad13)")
  (net 204 "Net-(U27-Pad1)")
  (net 205 "Net-(U27-Pad10)")
  (net 206 "Net-(L1-Pad2)")
  (net 207 "Net-(L2-Pad2)")
  (net 208 "Net-(IRQ2-Pad2)")
  (net 209 "Net-(JP1-Pad1)")
  (net 210 VDDA)
  (net 211 GNDA)
  (net 212 +12V)
  (net 213 +5VD)
  (net 214 -12V)
  (net 215 -5VA)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.3048)
    (via_dia 1.143)
    (via_drill 0.5842)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5VA)
    (add_net +5VD)
    (add_net +9VA)
    (add_net -12V)
    (add_net -5VA)
    (add_net /1xx000xxxx)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /AEN)
    (add_net /BUSRESET)
    (add_net /BUTTON1)
    (add_net /BUTTON2)
    (add_net /BUTTON3)
    (add_net /BUTTON4)
    (add_net /CLK_14M318)
    (add_net /CLK_3M579)
    (add_net /CLK_7M159)
    (add_net /CMS1-6_~CS)
    (add_net /CMS7-12_~CS)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /DAC0)
    (add_net /DAC1)
    (add_net /DAC2)
    (add_net /DAC3)
    (add_net /DAC4)
    (add_net /DAC5)
    (add_net /DAC6)
    (add_net /DAC7)
    (add_net /DAV_DSP)
    (add_net /DAV_PC)
    (add_net /DAV_~CS)
    (add_net /DB0)
    (add_net /DB1)
    (add_net /DB2)
    (add_net /DB3)
    (add_net /DB4)
    (add_net /DB5)
    (add_net /DB6)
    (add_net /DB7)
    (add_net /DD0)
    (add_net /DD1)
    (add_net /DD2)
    (add_net /DD3)
    (add_net /DD4)
    (add_net /DD5)
    (add_net /DD6)
    (add_net /DD7)
    (add_net /DIGITAL_OUT)
    (add_net /DREQUEST)
    (add_net /DRQ1)
    (add_net /DSPRD_~CS)
    (add_net /DSPRST_~CS)
    (add_net /DSPWR_~CS)
    (add_net /DSP_BUSY)
    (add_net /FM_~CS)
    (add_net /IO_READY)
    (add_net /IREQUEST)
    (add_net /IRQ2)
    (add_net /IRQ3)
    (add_net /IRQ5)
    (add_net /IRQ7)
    (add_net /JOYSTICK_~CS)
    (add_net /MIC_COMP)
    (add_net /MIDI_IN)
    (add_net /MIDI_OUT)
    (add_net /MUTE_EN)
    (add_net /OPL2)
    (add_net /RESET)
    (add_net /SAA_L)
    (add_net /SAA_R)
    (add_net /X1)
    (add_net /X2)
    (add_net /Y1)
    (add_net /Y2)
    (add_net /~100000xxxx)
    (add_net /~100jjjxxxx)
    (add_net /~111000xxxx)
    (add_net /~CARD_SELECTED)
    (add_net /~DACK1)
    (add_net /~DB_EN)
    (add_net /~DMAOUT)
    (add_net /~DMA_EN)
    (add_net /~DSP_READ)
    (add_net /~DSP_WRITE)
    (add_net /~IC)
    (add_net /~IOR)
    (add_net /~IOW)
    (add_net /~ISA_RD)
    (add_net /~ISA_WR)
    (add_net /~RD)
    (add_net /~RD_DAV)
    (add_net /~RESET)
    (add_net /~WR)
    (add_net GND)
    (add_net GNDA)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C30-Pad1)")
    (add_net "Net-(C30-Pad2)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C31-Pad2)")
    (add_net "Net-(C32-Pad2)")
    (add_net "Net-(C35-Pad1)")
    (add_net "Net-(C36-Pad1)")
    (add_net "Net-(C37-Pad2)")
    (add_net "Net-(C38-Pad1)")
    (add_net "Net-(C38-Pad2)")
    (add_net "Net-(C39-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C40-Pad1)")
    (add_net "Net-(C40-Pad2)")
    (add_net "Net-(C42-Pad1)")
    (add_net "Net-(C42-Pad2)")
    (add_net "Net-(C43-Pad1)")
    (add_net "Net-(C43-Pad2)")
    (add_net "Net-(C49-Pad2)")
    (add_net "Net-(C51-Pad2)")
    (add_net "Net-(C52-Pad2)")
    (add_net "Net-(C54-Pad1)")
    (add_net "Net-(C55-Pad1)")
    (add_net "Net-(C59-Pad1)")
    (add_net "Net-(C61-Pad1)")
    (add_net "Net-(C62-Pad1)")
    (add_net "Net-(C63-Pad1)")
    (add_net "Net-(C65-Pad1)")
    (add_net "Net-(C78-Pad1)")
    (add_net "Net-(C89-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(IO1-Pad1)")
    (add_net "Net-(IO1-Pad10)")
    (add_net "Net-(IO1-Pad11)")
    (add_net "Net-(IO1-Pad3)")
    (add_net "Net-(IO1-Pad5)")
    (add_net "Net-(IO1-Pad7)")
    (add_net "Net-(IO1-Pad9)")
    (add_net "Net-(IRQ2-Pad2)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(L2-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R34-Pad2)")
    (add_net "Net-(R35-Pad2)")
    (add_net "Net-(R38-Pad1)")
    (add_net "Net-(R39-Pad2)")
    (add_net "Net-(R40-Pad2)")
    (add_net "Net-(R41-Pad2)")
    (add_net "Net-(R44-Pad2)")
    (add_net "Net-(RP2-Pad2)")
    (add_net "Net-(RP2-Pad3)")
    (add_net "Net-(RP2-Pad4)")
    (add_net "Net-(RP2-Pad5)")
    (add_net "Net-(RXD1-Pad3)")
    (add_net "Net-(TXD1-Pad3)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U10-Pad2)")
    (add_net "Net-(U10-Pad3)")
    (add_net "Net-(U10-Pad4)")
    (add_net "Net-(U10-Pad5)")
    (add_net "Net-(U10-Pad8)")
    (add_net "Net-(U16-Pad10)")
    (add_net "Net-(U20-Pad1)")
    (add_net "Net-(U20-Pad10)")
    (add_net "Net-(U20-Pad11)")
    (add_net "Net-(U20-Pad12)")
    (add_net "Net-(U20-Pad5)")
    (add_net "Net-(U20-Pad9)")
    (add_net "Net-(U21-Pad4)")
    (add_net "Net-(U21-Pad5)")
    (add_net "Net-(U23-Pad12)")
    (add_net "Net-(U23-Pad2)")
    (add_net "Net-(U24-Pad11)")
    (add_net "Net-(U24-Pad3)")
    (add_net "Net-(U26-Pad13)")
    (add_net "Net-(U26-Pad5)")
    (add_net "Net-(U27-Pad1)")
    (add_net "Net-(U27-Pad10)")
    (add_net VCC)
    (add_net VDDA)
  )
  (module SoundBlaster:Snark_Barker (layer B.Cu) (tedit 0)
    (at 106.5022 30.2768 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 177.165 70.104)
    (fp_text reference C46 (at 5.334 0) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 213 +5VD))
    (pad 2 thru_hole circle (at 1.905 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 203.2 48.26 180)
    (fp_text reference C1 (at -2.286 3.302 180) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 1.905 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 189.23 53.34 270)
    (fp_text reference C2 (at -3.302 0.254 360) (layer F.SilkS))
    (fp_text value "47uF 16V" (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 1.905 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_RADIAL_100_320 (layer F.Cu) (tedit 5B594161)
    (at 203.2 58.42 270)
    (fp_text reference C3 (at -3.302 -2.54 360) (layer F.SilkS))
    (fp_text value "100uF 16V" (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 "Net-(C3-Pad2)"))
  )
  (module SoundBlaster:SB_C_RADIAL_100_320 (layer F.Cu) (tedit 5B594161)
    (at 190.754 63.5 270)
    (fp_text reference C4 (at -3.556 3.556 360) (layer F.SilkS))
    (fp_text value "470uF 16V" (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 "Net-(C4-Pad2)"))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 198.12 63.5 90)
    (fp_text reference C5 (at 7.112 2.032 90) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 6.985 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 195.58 63.5 90)
    (fp_text reference C6 (at 7.112 -2.032 90) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 6.985 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_RADIAL_100_320 (layer F.Cu) (tedit 5B594161)
    (at 203.2 68.58 180)
    (fp_text reference C7 (at -3.302 3.556 180) (layer F.SilkS))
    (fp_text value "100uF 16V" (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 +9VA))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 209.55 70.104)
    (fp_text reference C8 (at 8.636 -0.254) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 +9VA))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 237.998 66.675 270)
    (fp_text reference C9 (at 3.683 2.54 270) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 6.985 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 237.998 63.5 90)
    (fp_text reference C10 (at 4.572 -2.54 90) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 6.985 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_RADIAL_100_320 (layer F.Cu) (tedit 5B594161)
    (at 232.664 63.5 270)
    (fp_text reference C11 (at 6.223 3.048 360) (layer F.SilkS))
    (fp_text value "470uF 16V" (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 10 "Net-(C11-Pad2)"))
  )
  (module SoundBlaster:SB_C_RADIAL_100_320 (layer F.Cu) (tedit 5B594161)
    (at 223.52 60.96 270)
    (fp_text reference C12 (at -3.81 2.794 360) (layer F.SilkS))
    (fp_text value "100uF 16V" (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 11 "Net-(C12-Pad2)"))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 231.14 58.42)
    (fp_text reference C13 (at -3.556 -0.508) (layer F.SilkS))
    (fp_text value "47uF 16V" (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at 1.905 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 236.22 54.102)
    (fp_text reference C14 (at 1.016 -2.54) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 thru_hole circle (at 1.905 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 14 "Net-(C14-Pad2)"))
  )
  (module SoundBlaster:SB_C_RADIAL_100_320 (layer F.Cu) (tedit 5B594161)
    (at 222.25 49.784)
    (fp_text reference C15 (at 6.858 -3.048) (layer F.SilkS))
    (fp_text value "100uF 16V" (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 15 "Net-(C15-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 209.55 83.058)
    (fp_text reference C16 (at 3.556 -2.54) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 212 +12V))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_RADIAL_100_320 (layer F.Cu) (tedit 5B594161)
    (at 223.52 80.518 270)
    (fp_text reference C17 (at -2.54 -4.826 360) (layer F.SilkS))
    (fp_text value "100uF 16V" (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 212 +12V))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_RADIAL_100_320 (layer F.Cu) (tedit 5B594161)
    (at 222.758 72.898 90)
    (fp_text reference C18 (at -1.778 5.588 180) (layer F.SilkS))
    (fp_text value "100uF 16V" (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 +9VA))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 209.55 72.898)
    (fp_text reference C19 (at 7.62 2.286) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 +9VA))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 243.84 88.9 180)
    (fp_text reference C20 (at 2.032 2.54 180) (layer F.SilkS))
    (fp_text value 0.01u (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 16 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B5A685E)
    (at 243.84 91.44 180)
    (fp_text reference C21 (at 2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 0.01u (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 17 "Net-(C21-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B5A684E)
    (at 243.84 93.98 180)
    (fp_text reference C22 (at 2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 0.01u (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 18 "Net-(C22-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B5A6834)
    (at 243.84 96.52 180)
    (fp_text reference C23 (at 2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 0.01u (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 19 "Net-(C23-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B5A681F)
    (at 243.84 99.06 180)
    (fp_text reference C24 (at 2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 0.01u (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 20 /BUTTON1))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B5A680D)
    (at 243.84 101.6 180)
    (fp_text reference C25 (at 2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 0.01u (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 21 /BUTTON4))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B5A67CC)
    (at 243.84 104.14 180)
    (fp_text reference C26 (at 2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 0.01u (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 22 "Net-(C26-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B5A6790)
    (at 243.84 108.458 180)
    (fp_text reference C27 (at 2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 0.01u (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 "Net-(C27-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B5A676C)
    (at 243.84 113.538 180)
    (fp_text reference C28 (at 2.794 0 180) (layer F.SilkS) hide)
    (fp_text value 0.01u (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 24 /BUTTON3))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 243.84 116.078 180)
    (fp_text reference C29 (at 3.81 -2.794 180) (layer F.SilkS))
    (fp_text value 0.01u (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 25 /BUTTON2))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 254.254 35.052 180)
    (fp_text reference C30 (at 0.889 -3.048 180) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 26 "Net-(C30-Pad1)"))
    (pad 2 thru_hole circle (at 1.905 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 27 "Net-(C30-Pad2)"))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 244.602 34.798)
    (fp_text reference C31 (at 2.54 2.286) (layer F.SilkS))
    (fp_text value 1000p (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 28 "Net-(C31-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 29 "Net-(C31-Pad2)"))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 237.49 24.638)
    (fp_text reference C32 (at -1.524 1.524) (layer F.SilkS))
    (fp_text value 330p (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 30 "Net-(C32-Pad2)"))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 228.219 24.638)
    (fp_text reference C33 (at -1.905 1.27) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 215 -5VA))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 232.41 38.1)
    (fp_text reference C34 (at 9.398 0) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 43 +5VA))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 229.87 38.1 180)
    (fp_text reference C35 (at 2.54 -1.778 180) (layer F.SilkS))
    (fp_text value 330p (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 31 "Net-(C35-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 238.76 41.91 270)
    (fp_text reference C36 (at -1.778 -0.762 360) (layer F.SilkS))
    (fp_text value 1000p (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 32 "Net-(C36-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 236.22 49.53 90)
    (fp_text reference C37 (at 0.254 3.048 180) (layer F.SilkS))
    (fp_text value 1000p (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 33 "Net-(C37-Pad2)"))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 211.455 25.4 180)
    (fp_text reference C38 (at 5.715 0 180) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 34 "Net-(C38-Pad1)"))
    (pad 2 thru_hole circle (at 1.905 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 35 "Net-(C38-Pad2)"))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 197.612 29.21 270)
    (fp_text reference C39 (at 4.318 1.016 360) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 36 "Net-(C39-Pad1)"))
    (pad 2 thru_hole circle (at 1.905 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_RADIAL_100_320 (layer F.Cu) (tedit 5B594161)
    (at 193.548 38.1)
    (fp_text reference C40 (at 1.27 5.334) (layer F.SilkS))
    (fp_text value "100uF 16V" (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 37 "Net-(C40-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 38 "Net-(C40-Pad2)"))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 180.34 25.4)
    (fp_text reference C41 (at -4.064 -0.762) (layer F.SilkS))
    (fp_text value 47 (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 37 "Net-(C40-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 34 "Net-(C38-Pad1)"))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 179.324 40.005)
    (fp_text reference C42 (at 5.842 -1.905) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 39 "Net-(C42-Pad1)"))
    (pad 2 thru_hole circle (at 1.905 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 40 "Net-(C42-Pad2)"))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 176.53 51.562)
    (fp_text reference C43 (at 5.842 -1.27) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 41 "Net-(C43-Pad1)"))
    (pad 2 thru_hole circle (at 1.905 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 42 "Net-(C43-Pad2)"))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 180.34 55.88)
    (fp_text reference C44 (at 2.032 -3.556) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 2 thru_hole circle (at 1.905 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 215 -5VA))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 177.165 65.278)
    (fp_text reference C45 (at 5.207 0) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 43 +5VA))
    (pad 2 thru_hole circle (at 1.905 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 166.37 70.358)
    (fp_text reference C47 (at 7.62 -1.524) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 213 +5VD))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 166.37 67.31)
    (fp_text reference C48 (at 7.62 -1.524) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 212 +12V))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 171.45 64.008 180)
    (fp_text reference C49 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 1000p (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 41 "Net-(C43-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 44 "Net-(C49-Pad2)"))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 166.37 45.085)
    (fp_text reference C50 (at 10.668 0.635) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 215 -5VA))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 170.688 30.48 270)
    (fp_text reference C51 (at -2.54 1.524 270) (layer F.SilkS))
    (fp_text value 2200p (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 45 /DIGITAL_OUT))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 46 "Net-(C51-Pad2)"))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 168.148 30.48 270)
    (fp_text reference C52 (at -2.54 1.016 270) (layer F.SilkS))
    (fp_text value 330p (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 47 "Net-(C52-Pad2)"))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 151.638 38.1)
    (fp_text reference C53 (at -3.556 0) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 214 -12V))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 163.83 40.005 180)
    (fp_text reference C54 (at 10.668 0 180) (layer F.SilkS))
    (fp_text value 1000p (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 48 "Net-(C54-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 39 "Net-(C42-Pad1)"))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 156.845 64.516)
    (fp_text reference C55 (at 5.461 0.762) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 49 "Net-(C55-Pad1)"))
    (pad 2 thru_hole circle (at 1.905 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 139.7 72.39)
    (fp_text reference C56 (at 7.366 -2.794) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 213 +5VD))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 146.05 54.61 270)
    (fp_text reference C57 (at 1.27 -2.032 270) (layer F.SilkS))
    (fp_text value 4700p (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 50 /OPL2))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 146.05 44.958 270)
    (fp_text reference C58 (at -3.302 0 270) (layer F.SilkS))
    (fp_text value 2200p (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 51 /SAA_R))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 139.7 38.1)
    (fp_text reference C59 (at -3.048 0) (layer F.SilkS))
    (fp_text value 47p (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 52 "Net-(C59-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 214 -12V))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 135.89 44.958 270)
    (fp_text reference C60 (at -3.302 0 270) (layer F.SilkS))
    (fp_text value 2200p (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 53 /SAA_L))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 69.85 30.48 270)
    (fp_text reference C61 (at 8.382 0 270) (layer F.SilkS))
    (fp_text value 30p (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 54 "Net-(C61-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 72.39 35.56 90)
    (fp_text reference C62 (at -3.302 0 90) (layer F.SilkS))
    (fp_text value 30p (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 55 "Net-(C62-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 127 59.69)
    (fp_text reference C63 (at 2.54 -2.286) (layer F.SilkS))
    (fp_text value 1000p (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 56 "Net-(C63-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 96.52 91.44)
    (fp_text reference C64 (at -3.81 0.254) (layer F.SilkS))
    (fp_text value 330p (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 57 /~ISA_WR))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 63.5 55.88)
    (fp_text reference C65 (at 8.382 0) (layer F.SilkS))
    (fp_text value 270p (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 58 "Net-(C65-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 60.96 55.88 180)
    (fp_text reference C66 (at 8.382 0 180) (layer F.SilkS))
    (fp_text value 680p (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 59 /DREQUEST))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 63.5 71.12)
    (fp_text reference C67 (at 8.382 0) (layer F.SilkS))
    (fp_text value 470p (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 60 /~RESET))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 43.18 53.34)
    (fp_text reference C68 (at -3.302 0) (layer F.SilkS))
    (fp_text value 270p (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 61 /RESET))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 29.21 26.162 270)
    (fp_text reference C69 (at 10.16 0.254 270) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 6.985 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 29.21 74.041 270)
    (fp_text reference C70 (at -2.667 0.254 270) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 6.985 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 29.21 104.648 270)
    (fp_text reference C71 (at -3.302 0.254 270) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 6.985 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 52.07 104.775 270)
    (fp_text reference C72 (at -3.302 0.254 270) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 6.985 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 52.07 74.295 270)
    (fp_text reference C73 (at -2.667 0 270) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 6.985 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 52.07 41.275 270)
    (fp_text reference C74 (at 10.287 0 270) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 6.985 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 76.962 58.928)
    (fp_text reference C75 (at 10.922 0) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 74.93 104.775 270)
    (fp_text reference C76 (at -3.429 0 270) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 6.985 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 113.03 104.775 270)
    (fp_text reference C77 (at -3.429 0.254 270) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 6.985 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 107.95 88.9 90)
    (fp_text reference C78 (at 9.144 0 90) (layer F.SilkS))
    (fp_text value 1000p (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 63 "Net-(C78-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_DISC_200 (layer F.Cu) (tedit 5B594157)
    (at 106.68 64.77 270)
    (fp_text reference C79 (at -5.588 0 270) (layer F.SilkS))
    (fp_text value 330p (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 64 /~DSP_WRITE))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 132.08 53.34 180)
    (fp_text reference C80 (at 10.414 0 180) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 6.985 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 111.76 59.69)
    (fp_text reference C81 (at 3.048 -2.286) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 210 VDDA))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 111.76 78.74)
    (fp_text reference C82 (at 10.922 0) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 210 VDDA))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 136.906 82.423 270)
    (fp_text reference C83 (at -3.429 -0.254 270) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 213 +5VD))
    (pad 2 thru_hole circle (at 6.985 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 140.97 99.06)
    (fp_text reference C84 (at 10.668 0.254) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 6.985 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 191.77 104.775 270)
    (fp_text reference C85 (at -3.429 0.508 270) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 6.985 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 172.974 56.642 90)
    (fp_text reference C86 (at 0 3.302 180) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 43 +5VA))
    (pad 2 thru_hole circle (at 6.985 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 231.775 116.078)
    (fp_text reference C87 (at -2.667 -2.54) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 210 VDDA))
    (pad 2 thru_hole circle (at 1.905 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_C_RADIAL_75_150 (layer F.Cu) (tedit 5B59416E)
    (at 163.83 116.332 180)
    (fp_text reference C88 (at 5.842 0 180) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 1.905 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_C_AXIAL_275 (layer F.Cu) (tedit 5B59414F)
    (at 222.504 33.528 90)
    (fp_text reference C89 (at -2.667 0 90) (layer F.SilkS))
    (fp_text value 0.1u (at 3.683 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 65 "Net-(C89-Pad1)"))
    (pad 2 thru_hole circle (at 6.985 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_D_AXIAL_400 (layer F.Cu) (tedit 5B5941CA)
    (at 207.518 27.94 270)
    (fp_text reference D1 (at 13.208 0 270) (layer F.SilkS))
    (fp_text value 1N4148 (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 66 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_D_AXIAL_400 (layer F.Cu) (tedit 5B5941CA)
    (at 199.898 27.94 270)
    (fp_text reference D2 (at 14.224 0 270) (layer F.SilkS))
    (fp_text value 1N4148 (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 36 "Net-(C39-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 67 "Net-(D2-Pad2)"))
  )
  (module SoundBlaster:SB_HDR_1X2 (layer F.Cu) (tedit 5B5A8285)
    (at 78.74 49.53 90)
    (fp_text reference DRQ1 (at 10.414 0.254 90) (layer F.SilkS))
    (fp_text value "DMA ENABLE JUMPER" (at 1.27 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 "Net-(C65-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 68 /DRQ1))
  )
  (module SoundBlaster:SB_HDR_2X6 (layer F.Cu) (tedit 5B5A655D)
    (at 173.99 96.52)
    (fp_text reference IO1 (at 6.35 -6.604) (layer F.SilkS) hide)
    (fp_text value "I/O ADDX" (at 6.223 -1.397) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 69 "Net-(IO1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 "Net-(IO1-Pad10)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 71 "Net-(IO1-Pad3)"))
    (pad 4 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 "Net-(IO1-Pad10)"))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 "Net-(IO1-Pad5)"))
    (pad 6 thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 "Net-(IO1-Pad10)"))
    (pad 7 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 "Net-(IO1-Pad7)"))
    (pad 11 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 "Net-(IO1-Pad11)"))
    (pad 12 thru_hole circle (at 12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 "Net-(IO1-Pad10)"))
    (pad 8 thru_hole circle (at 7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 "Net-(IO1-Pad10)"))
    (pad 9 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 "Net-(IO1-Pad9)"))
    (pad 10 thru_hole circle (at 10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 "Net-(IO1-Pad10)"))
  )
  (module SoundBlaster:SB_HDR_1X2 (layer F.Cu) (tedit 5B5941DC)
    (at 104.775 111.76 180)
    (fp_text reference IRQ2 (at -4.699 -0.254 180) (layer F.SilkS))
    (fp_text value Conn_02x01 (at 1.27 0 360) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 /IRQ2))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 208 "Net-(IRQ2-Pad2)"))
  )
  (module SoundBlaster:SB_HDR_1X2 (layer F.Cu) (tedit 5B5941DC)
    (at 104.775 109.22 180)
    (fp_text reference IRQ3 (at -4.699 0 180) (layer F.SilkS))
    (fp_text value Conn_02x01 (at 1.27 0 360) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 /IRQ3))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 208 "Net-(IRQ2-Pad2)"))
  )
  (module SoundBlaster:SB_HDR_1X2 (layer F.Cu) (tedit 5B5941DC)
    (at 104.775 106.68 180)
    (fp_text reference IRQ5 (at -4.699 0 180) (layer F.SilkS))
    (fp_text value Conn_02x01 (at 1.27 0 360) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 /IRQ5))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 208 "Net-(IRQ2-Pad2)"))
  )
  (module SoundBlaster:SB_HDR_1X2 (layer F.Cu) (tedit 5B5941DC)
    (at 104.775 104.14 180)
    (fp_text reference IRQ7 (at -4.699 0 180) (layer F.SilkS))
    (fp_text value Conn_02x01 (at 1.27 0 360) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 /IRQ7))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 208 "Net-(IRQ2-Pad2)"))
  )
  (module SoundBlaster:BUS_PC (layer F.Cu) (tedit 5B5A8497)
    (at 195.58 125.73)
    (descr "Connecteur Bus AT ISA 16 bits")
    (tags "CONN BUS ISA")
    (fp_text reference J1 (at -40.132 0) (layer F.SilkS) hide)
    (fp_text value Bus_ISA_8bit (at -43.815 -6.985) (layer F.Fab))
    (pad 1 connect rect (at 38.1 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 211 GNDA))
    (pad 2 connect rect (at 35.56 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 80 /BUSRESET))
    (pad 3 connect rect (at 33.02 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 210 VDDA))
    (pad 4 connect rect (at 30.48 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 76 /IRQ2))
    (pad 5 connect rect (at 27.94 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 6 connect rect (at 25.4 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 22.86 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 214 -12V))
    (pad 8 connect rect (at 20.32 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 9 connect rect (at 17.78 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 212 +12V))
    (pad 10 connect rect (at 15.24 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 11 connect rect (at 12.7 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 12 connect rect (at 10.16 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 13 connect rect (at 7.62 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 81 /~IOW))
    (pad 14 connect rect (at 5.08 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 82 /~IOR))
    (pad 15 connect rect (at 2.54 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 16 connect rect (at 0 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 17 connect rect (at -2.54 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 83 /~DACK1))
    (pad 18 connect rect (at -5.08 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 68 /DRQ1))
    (pad 19 connect rect (at -7.62 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 20 connect rect (at -10.16 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 21 connect rect (at -12.7 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 79 /IRQ7))
    (pad 22 connect rect (at -15.24 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 23 connect rect (at -17.78 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 78 /IRQ5))
    (pad 24 connect rect (at -20.32 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 25 connect rect (at -22.86 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 77 /IRQ3))
    (pad 26 connect rect (at -25.4 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 27 connect rect (at -27.94 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 28 connect rect (at -30.48 0.381) (size 1.524 6.858) (layers B.Cu B.Mask))
    (pad 29 connect rect (at -33.02 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 62 VCC))
    (pad 30 connect rect (at -35.56 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 84 /CLK_14M318))
    (pad 31 connect rect (at -38.1 0.381) (size 1.524 6.858) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 32 connect rect (at 38.1 0.381) (size 1.524 6.858) (layers F.Cu F.Mask))
    (pad 33 connect rect (at 35.56 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 85 /DB7))
    (pad 34 connect rect (at 33.02 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 86 /DB6))
    (pad 35 connect rect (at 30.48 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 87 /DB5))
    (pad 36 connect rect (at 27.94 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 88 /DB4))
    (pad 37 connect rect (at 25.4 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 89 /DB3))
    (pad 38 connect rect (at 22.86 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 90 /DB2))
    (pad 39 connect rect (at 20.32 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 91 /DB1))
    (pad 40 connect rect (at 17.78 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 92 /DB0))
    (pad 41 connect rect (at 15.24 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 93 /IO_READY))
    (pad 42 connect rect (at 12.7 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 94 /AEN))
    (pad 43 connect rect (at 10.16 0.381) (size 1.524 6.858) (layers F.Cu F.Mask))
    (pad 44 connect rect (at 7.62 0.381) (size 1.524 6.858) (layers F.Cu F.Mask))
    (pad 45 connect rect (at 5.08 0.381) (size 1.524 6.858) (layers F.Cu F.Mask))
    (pad 46 connect rect (at 2.54 0.381) (size 1.524 6.858) (layers F.Cu F.Mask))
    (pad 47 connect rect (at 0 0.381) (size 1.524 6.858) (layers F.Cu F.Mask))
    (pad 48 connect rect (at -2.54 0.381) (size 1.524 6.858) (layers F.Cu F.Mask))
    (pad 49 connect rect (at -5.08 0.381) (size 1.524 6.858) (layers F.Cu F.Mask))
    (pad 50 connect rect (at -7.62 0.381) (size 1.524 6.858) (layers F.Cu F.Mask))
    (pad 51 connect rect (at -10.16 0.381) (size 1.524 6.858) (layers F.Cu F.Mask))
    (pad 52 connect rect (at -12.7 0.381) (size 1.524 6.858) (layers F.Cu F.Mask))
    (pad 53 connect rect (at -15.24 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 95 /A9))
    (pad 54 connect rect (at -17.78 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 96 /A8))
    (pad 55 connect rect (at -20.32 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 97 /A7))
    (pad 56 connect rect (at -22.86 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 98 /A6))
    (pad 57 connect rect (at -25.4 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 99 /A5))
    (pad 58 connect rect (at -27.94 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 100 /A4))
    (pad 59 connect rect (at -30.48 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 101 /A3))
    (pad 60 connect rect (at -33.02 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 102 /A2))
    (pad 61 connect rect (at -35.56 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 103 /A1))
    (pad 62 connect rect (at -38.1 0.381) (size 1.524 6.858) (layers F.Cu F.Mask)
      (net 104 /A0))
  )
  (module SoundBlaster:SB_HDR_1X2 (layer F.Cu) (tedit 5B5941DC)
    (at 71.12 101.6 180)
    (fp_text reference JP1 (at 6.858 0 180) (layer F.SilkS))
    (fp_text value "JOYSTICK EN" (at 1.27 0 360) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 209 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 105 /JOYSTICK_~CS))
  )
  (module SoundBlaster:SB_L_AXIAL_500 (layer F.Cu) (tedit 5B5941F6)
    (at 232.664 76.2)
    (fp_text reference L1 (at 0 1.778) (layer F.SilkS))
    (fp_text value ? (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 10 "Net-(C11-Pad2)"))
    (pad 2 thru_hole circle (at 12.7 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 206 "Net-(L1-Pad2)"))
  )
  (module SoundBlaster:SB_L_AXIAL_500 (layer F.Cu) (tedit 5B5941F6)
    (at 232.664 80.01)
    (fp_text reference L2 (at 0 2.286) (layer F.SilkS))
    (fp_text value ? (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 12.7 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 207 "Net-(L2-Pad2)"))
  )
  (module SoundBlaster:SB_L_AXIAL_500 (layer F.Cu) (tedit 5B5941F6)
    (at 231.14 110.998)
    (fp_text reference L3 (at -2.794 0) (layer F.SilkS))
    (fp_text value ? (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 210 VDDA))
    (pad 2 thru_hole circle (at 12.7 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 "Net-(C27-Pad1)"))
  )
  (module SoundBlaster:SB_TO220 (layer F.Cu) (tedit 5B5954A7)
    (at 209.55 80.518)
    (fp_text reference P2 (at -19.05 -9.144) (layer F.SilkS))
    (fp_text value L7809 (at -8.89 -2.54) (layer F.Fab))
    (fp_text user OUT (at -2.032 -5.715 90) (layer F.SilkS))
    (fp_text user IN (at -2.032 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 212 +12V))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 3 thru_hole circle (at 0 -5.08 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 +9VA))
    (pad 2 thru_hole circle (at -17.78 -2.54 270) (size 4.445 4.445) (drill 3.81) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 203.2 53.34 180)
    (fp_text reference R1 (at 9.652 2.286 180) (layer F.SilkS))
    (fp_text value 270 (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 112 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 220.98 55.118)
    (fp_text reference R2 (at 9.652 -2.286) (layer F.SilkS))
    (fp_text value 270 (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 113 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 "Net-(C13-Pad1)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 230.378 44.45 180)
    (fp_text reference R3 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 10K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 33 "Net-(C37-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 42 "Net-(C43-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 236.22 41.91 180)
    (fp_text reference R4 (at 0.254 1.778 180) (layer F.SilkS))
    (fp_text value 10K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 32 "Net-(C36-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 40 "Net-(C42-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 244.602 24.638)
    (fp_text reference R5 (at 12.7 0) (layer F.SilkS))
    (fp_text value 470K (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 30 "Net-(C32-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 254.762 27.178 180)
    (fp_text reference R6 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 68K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 29 "Net-(C31-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 30 "Net-(C32-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 254.762 29.718 180)
    (fp_text reference R7 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 68K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 26 "Net-(C30-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 29 "Net-(C31-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 254.762 32.258 180)
    (fp_text reference R8 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 10K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 35 "Net-(C38-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 28 "Net-(C31-Pad1)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 215.9 24.638)
    (fp_text reference R9 (at -2.032 1.27) (layer F.SilkS))
    (fp_text value 470K (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 37 "Net-(C40-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 34 "Net-(C38-Pad1)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 220.218 38.1 90)
    (fp_text reference R10 (at -3.302 0 90) (layer F.SilkS))
    (fp_text value 39K (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 46 "Net-(C51-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 114 "Net-(R10-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 217.678 38.1 90)
    (fp_text reference R11 (at -3.302 0 90) (layer F.SilkS))
    (fp_text value 68K (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 31 "Net-(C35-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 46 "Net-(C51-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 215.138 38.1 90)
    (fp_text reference R12 (at -3.302 0 90) (layer F.SilkS))
    (fp_text value 470K (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 31 "Net-(C35-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 212.598 27.94 270)
    (fp_text reference R13 (at 13.462 0 270) (layer F.SilkS))
    (fp_text value "39.0K 1%" (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 65 "Net-(C89-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 210.058 38.1 90)
    (fp_text reference R14 (at -3.302 0 90) (layer F.SilkS))
    (fp_text value "100.0K 1%" (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 213 +5VD))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 65 "Net-(C89-Pad1)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 204.978 27.94 270)
    (fp_text reference R15 (at 13.462 0 270) (layer F.SilkS))
    (fp_text value 470 (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 66 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 38 "Net-(C40-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 202.438 27.94 270)
    (fp_text reference R16 (at 13.462 0 270) (layer F.SilkS))
    (fp_text value 470 (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 67 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 38 "Net-(C40-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 192.278 25.4)
    (fp_text reference R17 (at -3.302 -0.254) (layer F.SilkS))
    (fp_text value 33K (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 115 "Net-(R17-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 36 "Net-(C39-Pad1)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 189.23 27.178 270)
    (fp_text reference R18 (at 13.462 0 270) (layer F.SilkS))
    (fp_text value "1.5K 1%" (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 116 "Net-(R18-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 114 "Net-(R10-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 176.53 84.582)
    (fp_text reference R19 (at -3.048 -0.254) (layer F.SilkS))
    (fp_text value 390 (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 215 -5VA))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 214 -12V))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 176.53 78.74 180)
    (fp_text reference R20 (at -3.302 0 180) (layer F.SilkS))
    (fp_text value 390 (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 212 +12V))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 43 +5VA))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 176.53 72.898 180)
    (fp_text reference R21 (at -3.302 0 180) (layer F.SilkS))
    (fp_text value 390 (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 212 +12V))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 213 +5VD))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 166.37 61.468)
    (fp_text reference R22 (at 13.716 0) (layer F.SilkS))
    (fp_text value 27K (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 44 "Net-(C49-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 45 /DIGITAL_OUT))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 176.53 58.928 180)
    (fp_text reference R23 (at -3.556 -0.508 180) (layer F.SilkS))
    (fp_text value 10K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 41 "Net-(C43-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 44 "Net-(C49-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 176.53 42.545 180)
    (fp_text reference R24 (at -8.636 0.254 180) (layer F.SilkS))
    (fp_text value 10K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 39 "Net-(C42-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 48 "Net-(C54-Pad1)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 166.37 40.005)
    (fp_text reference R25 (at 18.796 0) (layer F.SilkS))
    (fp_text value 27K (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 48 "Net-(C54-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 45 /DIGITAL_OUT))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 173.228 25.4 270)
    (fp_text reference R26 (at 2.286 2.286 270) (layer F.SilkS))
    (fp_text value 4.7K (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 43 +5VA))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 117 /MIC_COMP))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 157.48 25.4)
    (fp_text reference R27 (at 12.7 -0.762) (layer F.SilkS))
    (fp_text value 27K (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 118 /MUTE_EN))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 47 "Net-(C52-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 163.83 42.545 180)
    (fp_text reference R28 (at 13.716 0 180) (layer F.SilkS))
    (fp_text value 15K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 48 "Net-(C54-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 50 /OPL2))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 163.83 45.085 180)
    (fp_text reference R29 (at 13.716 0 180) (layer F.SilkS))
    (fp_text value 47K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 48 "Net-(C54-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 51 /SAA_R))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 163.83 58.928 180)
    (fp_text reference R30 (at 10.922 -1.524 180) (layer F.SilkS))
    (fp_text value 47K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 44 "Net-(C49-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 53 /SAA_L))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 163.83 61.468 180)
    (fp_text reference R31 (at 10.16 -1.778 180) (layer F.SilkS))
    (fp_text value 15K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 44 "Net-(C49-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 50 /OPL2))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 142.24 69.85 90)
    (fp_text reference R32 (at 13.97 1.778 90) (layer F.SilkS))
    (fp_text value 1.5K (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 56 "Net-(C63-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 213 +5VD))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 139.7 69.85 90)
    (fp_text reference R33 (at 13.97 0.508 90) (layer F.SilkS))
    (fp_text value 1.5K (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 63 "Net-(C78-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 213 +5VD))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 137.16 59.69 270)
    (fp_text reference R34 (at -3.81 0.254 270) (layer F.SilkS))
    (fp_text value 10K (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 213 +5VD))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 119 "Net-(R34-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 149.86 58.42 90)
    (fp_text reference R35 (at -3.556 0 90) (layer F.SilkS))
    (fp_text value 2.2K (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 50 /OPL2))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 120 "Net-(R35-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 142.24 44.958 270)
    (fp_text reference R36 (at -3.048 0 450) (layer F.SilkS))
    (fp_text value 10K (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 51 /SAA_R))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 56 "Net-(C63-Pad1)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 138.43 44.958 270)
    (fp_text reference R37 (at -3.302 0 270) (layer F.SilkS))
    (fp_text value 10K (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 53 /SAA_L))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 63 "Net-(C78-Pad1)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 144.78 25.4)
    (fp_text reference R38 (at -3.556 0) (layer F.SilkS))
    (fp_text value "2.70K 1%" (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 121 "Net-(R38-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 213 +5VD))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 137.16 72.39 180)
    (fp_text reference R39 (at 13.462 0 180) (layer F.SilkS))
    (fp_text value 4.7K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 213 +5VD))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 122 "Net-(R39-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 134.62 91.44 180)
    (fp_text reference R40 (at 13.716 0 180) (layer F.SilkS))
    (fp_text value 10K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 213 +5VD))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 123 "Net-(R40-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 116.84 101.6)
    (fp_text reference R41 (at 13.97 0) (layer F.SilkS))
    (fp_text value 4.7K (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 124 "Net-(R41-Pad2)"))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 96.52 100.33 180)
    (fp_text reference R42 (at 14.732 0.254 180) (layer F.SilkS))
    (fp_text value 4.7K (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 105 /JOYSTICK_~CS))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B594215)
    (at 76.2 43.18 270)
    (fp_text reference R43 (at -3.302 -0.762 270) (layer F.SilkS))
    (fp_text value 1K (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 58 "Net-(C65-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_R_AXIAL_400 (layer F.Cu) (tedit 5B5A557F)
    (at 33.02 101.6)
    (fp_text reference R44 (at 14.224 0) (layer F.SilkS))
    (fp_text value 4.7K (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 125 "Net-(R44-Pad2)"))
  )
  (module SoundBlaster:SB_RP_4B (layer F.Cu) (tedit 5B594201)
    (at 236.22 106.68 90)
    (fp_text reference RP1 (at 20.32 1.27 180) (layer F.SilkS))
    (fp_text value 2.2K (at 8.89 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 110 /Y2))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 22 "Net-(C26-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 108 /X2))
    (pad 4 thru_hole circle (at 7.62 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 17 "Net-(C21-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 107 /Y1))
    (pad 6 thru_hole circle (at 12.7 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 18 "Net-(C22-Pad1)"))
    (pad 7 thru_hole circle (at 15.24 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 106 /X1))
    (pad 8 thru_hole circle (at 17.78 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 16 "Net-(C20-Pad1)"))
  )
  (module SoundBlaster:SB_RP_4C (layer F.Cu) (tedit 5B59420B)
    (at 223.52 99.06 90)
    (fp_text reference RP2 (at -3.81 0 90) (layer F.SilkS))
    (fp_text value 1K (at 5.461 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 210 VDDA))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 126 "Net-(RP2-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 127 "Net-(RP2-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 128 "Net-(RP2-Pad4)"))
    (pad 5 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 129 "Net-(RP2-Pad5)"))
  )
  (module SoundBlaster:SB_RP_4C (layer F.Cu) (tedit 5B59420B)
    (at 195.58 86.36)
    (fp_text reference RP3 (at 14.224 0) (layer F.SilkS))
    (fp_text value 1K (at 5.461 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 25 /BUTTON2))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 20 /BUTTON1))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 24 /BUTTON3))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 21 /BUTTON4))
  )
  (module SoundBlaster:SB_HDR_1X3 (layer F.Cu) (tedit 5B5A81CD)
    (at 79.248 33.02 90)
    (fp_text reference RXD1 (at 6.096 2.794 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 1.27 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 111 /MIDI_IN))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 130 "Net-(RXD1-Pad3)"))
  )
  (module SoundBlaster:SB_TO92 (layer F.Cu) (tedit 5B594142)
    (at 163.83 34.29 180)
    (fp_text reference T1 (at 0.508 2.54 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 0.127 -1.27 180) (layer F.Fab))
    (fp_text user C (at 2.54 -3.302 270) (layer F.SilkS))
    (fp_text user B (at 2.54 -1.27 270) (layer F.SilkS))
    (fp_text user E (at 2.54 0.889 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 2 thru_hole circle (at -1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 47 "Net-(C52-Pad2)"))
    (pad 3 thru_hole circle (at 0 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 46 "Net-(C51-Pad2)"))
  )
  (module SoundBlaster:SB_TO92 (layer F.Cu) (tedit 5B594142)
    (at 193.04 31.242)
    (fp_text reference T2 (at -1.016 2.286) (layer F.SilkS))
    (fp_text value 2N3904 (at 0.127 -1.27) (layer F.Fab))
    (fp_text user C (at 2.54 -3.302 90) (layer F.SilkS))
    (fp_text user B (at 2.54 -1.27 90) (layer F.SilkS))
    (fp_text user E (at 2.54 0.889 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 2 thru_hole circle (at -1.27 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 115 "Net-(R17-Pad1)"))
    (pad 3 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 35 "Net-(C38-Pad2)"))
  )
  (module SoundBlaster:SB_HDR_1X3 (layer F.Cu) (tedit 5B5A81D0)
    (at 76.708 33.02 90)
    (fp_text reference TXD1 (at 6.096 -2.54 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 1.27 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 109 /MIDI_OUT))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 131 "Net-(TXD1-Pad3)"))
  )
  (module SoundBlaster:SB_DIP16_300 (layer F.Cu) (tedit 5B594181)
    (at 233.68 106.68 90)
    (fp_text reference U1 (at -1.524 -10.668 180) (layer F.SilkS))
    (fp_text value NE558 (at 7.62 -3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 127 "Net-(RP2-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 22 "Net-(C26-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 132 "Net-(U1-Pad11)"))
    (pad 4 thru_hole circle (at 7.62 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 19 "Net-(C23-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 210 VDDA))
    (pad 6 thru_hole circle (at 12.7 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 132 "Net-(U1-Pad11)"))
    (pad 7 thru_hole circle (at 15.24 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 17 "Net-(C21-Pad1)"))
    (pad 10 thru_hole circle (at 15.24 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 18 "Net-(C22-Pad1)"))
    (pad 11 thru_hole circle (at 12.7 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 132 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at 10.16 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 13 thru_hole circle (at 7.62 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 133 /~IC))
    (pad 14 thru_hole circle (at 5.08 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 132 "Net-(U1-Pad11)"))
    (pad 15 thru_hole circle (at 2.54 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 16 "Net-(C20-Pad1)"))
    (pad 16 thru_hole circle (at 0 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 126 "Net-(RP2-Pad2)"))
    (pad 8 thru_hole circle (at 17.78 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 128 "Net-(RP2-Pad4)"))
    (pad 9 thru_hole circle (at 17.78 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 129 "Net-(RP2-Pad5)"))
  )
  (module SoundBlaster:SB_DIP20_300 (layer F.Cu) (tedit 5B59419A)
    (at 195.58 111.76)
    (fp_text reference U2 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS245 (at 12.192 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 134 /~RD))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 92 /DB0))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 91 /DB1))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 90 /DB2))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 89 /DB3))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 88 /DB4))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 87 /DB5))
    (pad 18 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 135 /D0))
    (pad 11 thru_hole circle (at 22.86 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 136 /D7))
    (pad 12 thru_hole circle (at 20.32 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 137 /D6))
    (pad 13 thru_hole circle (at 17.78 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 138 /D5))
    (pad 14 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 139 /D4))
    (pad 15 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 140 /D3))
    (pad 16 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 141 /D2))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 86 /DB6))
    (pad 17 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 142 /D1))
    (pad 9 thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 85 /DB7))
    (pad 10 thru_hole circle (at 22.86 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 19 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 143 /~DB_EN))
    (pad 20 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP20_300 (layer F.Cu) (tedit 5B59419A)
    (at 195.58 96.52)
    (fp_text reference U3 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS244 (at 12.192 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 144 "Net-(U24-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 126 "Net-(RP2-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 136 /D7))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 129 "Net-(RP2-Pad5)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 137 /D6))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 128 "Net-(RP2-Pad4)"))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 138 /D5))
    (pad 18 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 135 /D0))
    (pad 11 thru_hole circle (at 22.86 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 20 /BUTTON1))
    (pad 12 thru_hole circle (at 20.32 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 140 /D3))
    (pad 13 thru_hole circle (at 17.78 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 25 /BUTTON2))
    (pad 14 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 141 /D2))
    (pad 15 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 21 /BUTTON4))
    (pad 16 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 142 /D1))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 127 "Net-(RP2-Pad3)"))
    (pad 17 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 24 /BUTTON3))
    (pad 9 thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 139 /D4))
    (pad 10 thru_hole circle (at 22.86 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 19 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 144 "Net-(U24-Pad3)"))
    (pad 20 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP16_300 (layer F.Cu) (tedit 5B594181)
    (at 217.17 66.04 90)
    (fp_text reference U4 (at -0.508 2.794 90) (layer F.SilkS))
    (fp_text value TEA2025B (at 7.62 -3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 11 "Net-(C12-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 5 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 6 thru_hole circle (at 12.7 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 113 "Net-(R2-Pad1)"))
    (pad 7 thru_hole circle (at 15.24 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 10 thru_hole circle (at 15.24 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 11 thru_hole circle (at 12.7 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 112 "Net-(R1-Pad1)"))
    (pad 12 thru_hole circle (at 10.16 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 13 thru_hole circle (at 7.62 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 14 thru_hole circle (at 5.08 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 15 thru_hole circle (at 2.54 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (pad 16 thru_hole circle (at 0 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 +9VA))
    (pad 8 thru_hole circle (at 17.78 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 15 "Net-(C15-Pad1)"))
    (pad 9 thru_hole circle (at 17.78 -7.62 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 226.06 35.56)
    (fp_text reference U5 (at -2.794 4.572 90) (layer F.SilkS))
    (fp_text value LM324 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 45 /DIGITAL_OUT))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 45 /DIGITAL_OUT))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 31 "Net-(C35-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 43 +5VA))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 30 "Net-(C32-Pad2)"))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 28 "Net-(C31-Pad1)"))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 28 "Net-(C31-Pad1)"))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 114 "Net-(R10-Pad2)"))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 116 "Net-(R18-Pad1)"))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 215 -5VA))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 65 "Net-(C89-Pad1)"))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 34 "Net-(C38-Pad1)"))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 37 "Net-(C40-Pad1)"))
  )
  (module SoundBlaster:SB_DIP8_300 (layer F.Cu) (tedit 5B5941BF)
    (at 177.8 35.56)
    (fp_text reference U6 (at -0.762 2.54) (layer F.SilkS))
    (fp_text value LM393 (at 3.556 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 117 /MIC_COMP))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 37 "Net-(C40-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 114 "Net-(R10-Pad2)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 6 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 7 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 43 +5VA))
  )
  (module SoundBlaster:SB_DIP16_300 (layer F.Cu) (tedit 5B594181)
    (at 168.91 111.76)
    (fp_text reference U7 (at -1.27 3.302) (layer F.SilkS))
    (fp_text value 74LS138 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 100 /A4))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 99 /A5))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 98 /A6))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 94 /AEN))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 95 /A9))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 75 "Net-(IO1-Pad9)"))
    (pad 11 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 73 "Net-(IO1-Pad7)"))
    (pad 12 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 72 "Net-(IO1-Pad5)"))
    (pad 13 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 71 "Net-(IO1-Pad3)"))
    (pad 14 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 69 "Net-(IO1-Pad1)"))
    (pad 15 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 145 /1xx000xxxx))
    (pad 16 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 9 thru_hole circle (at 17.78 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 74 "Net-(IO1-Pad11)"))
  )
  (module SoundBlaster:SB_DIP16_300 (layer F.Cu) (tedit 5B594181)
    (at 140.97 111.76)
    (fp_text reference U8 (at -1.27 3.302) (layer F.SilkS))
    (fp_text value 74LS138 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 103 /A1))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 102 /A2))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 101 /A3))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 146 /~CARD_SELECTED))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 94 /AEN))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 95 /A9))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 147 /DAV_~CS))
    (pad 10 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 148 /DSPRD_~CS))
    (pad 11 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 149 /FM_~CS))
    (pad 12 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 150 /DSPRST_~CS))
    (pad 13 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 151 /CMS7-12_~CS))
    (pad 15 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 152 /CMS1-6_~CS))
    (pad 16 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 9 thru_hole circle (at 17.78 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 153 /DSPWR_~CS))
  )
  (module SoundBlaster:SB_DIP8_300 (layer F.Cu) (tedit 5B5941BF)
    (at 153.67 75.692)
    (fp_text reference U10 (at -0.508 -10.414) (layer F.SilkS))
    (fp_text value YM3014B (at 3.556 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 210 VDDA))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 156 "Net-(U10-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 155 "Net-(U10-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 157 "Net-(U10-Pad4)"))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 158 "Net-(U10-Pad5)"))
    (pad 6 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 7 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 49 "Net-(C55-Pad1)"))
    (pad 8 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 159 "Net-(U10-Pad8)"))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 153.67 55.88)
    (fp_text reference U11 (at 20.32 -7.874) (layer F.SilkS))
    (fp_text value NJM3403A (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 159 "Net-(U10-Pad8)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 159 "Net-(U10-Pad8)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 49 "Net-(C55-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 43 +5VA))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 44 "Net-(C49-Pad2)"))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 41 "Net-(C43-Pad1)"))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 39 "Net-(C42-Pad1)"))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 48 "Net-(C54-Pad1)"))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 215 -5VA))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 156 "Net-(U10-Pad2)"))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 120 "Net-(R35-Pad2)"))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 120 "Net-(R35-Pad2)"))
  )
  (module SoundBlaster:SB_DIP16_300 (layer F.Cu) (tedit 5B594181)
    (at 139.7 35.56)
    (fp_text reference U12 (at -5.334 -7.62) (layer F.SilkS))
    (fp_text value MC1408_DIP (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 214 -12V))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 116 "Net-(R18-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 160 /DAC7))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 161 /DAC6))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 162 /DAC5))
    (pad 10 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 163 /DAC2))
    (pad 11 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 164 /DAC1))
    (pad 12 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 165 /DAC0))
    (pad 13 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 210 VDDA))
    (pad 14 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 121 "Net-(R38-Pad1)"))
    (pad 15 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 16 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 52 "Net-(C59-Pad1)"))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 166 /DAC4))
    (pad 9 thru_hole circle (at 17.78 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 167 /DAC3))
  )
  (module SoundBlaster:SB_DIP40_600 (layer F.Cu) (tedit 5B5941B5)
    (at 132.08 35.56 180)
    (fp_text reference U13 (at 0.635 3.302 180) (layer F.SilkS))
    (fp_text value 805X (at 22.86 -7.62 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 165 /DAC0))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 164 /DAC1))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 163 /DAC2))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 167 /DAC3))
    (pad 5 thru_hole circle (at 10.16 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 166 /DAC4))
    (pad 6 thru_hole circle (at 12.7 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 162 /DAC5))
    (pad 7 thru_hole circle (at 15.24 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 161 /DAC6))
    (pad 18 thru_hole circle (at 43.18 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 54 "Net-(C61-Pad1)"))
    (pad 11 thru_hole circle (at 25.4 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 131 "Net-(TXD1-Pad3)"))
    (pad 12 thru_hole circle (at 27.94 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 168 /IREQUEST))
    (pad 13 thru_hole circle (at 30.48 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 169 /DSP_BUSY))
    (pad 14 thru_hole circle (at 33.02 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 170 /~DMA_EN))
    (pad 15 thru_hole circle (at 35.56 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 59 /DREQUEST))
    (pad 16 thru_hole circle (at 38.1 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 64 /~DSP_WRITE))
    (pad 8 thru_hole circle (at 17.78 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 160 /DAC7))
    (pad 17 thru_hole circle (at 40.64 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 171 /~DSP_READ))
    (pad 9 thru_hole circle (at 20.32 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 61 /RESET))
    (pad 10 thru_hole circle (at 22.86 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 130 "Net-(RXD1-Pad3)"))
    (pad 19 thru_hole circle (at 45.72 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 55 "Net-(C62-Pad1)"))
    (pad 20 thru_hole circle (at 48.26 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 21 thru_hole circle (at 48.26 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 118 /MUTE_EN))
    (pad 22 thru_hole circle (at 45.72 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 43.18 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at 40.64 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 38.1 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at 35.56 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 117 /MIC_COMP))
    (pad 27 thru_hole circle (at 33.02 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 172 /DAV_PC))
    (pad 28 thru_hole circle (at 30.48 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 173 /DAV_DSP))
    (pad 29 thru_hole circle (at 27.94 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 30 thru_hole circle (at 25.4 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at 22.86 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 32 thru_hole circle (at 20.32 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 174 /DD7))
    (pad 33 thru_hole circle (at 17.78 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 175 /DD6))
    (pad 34 thru_hole circle (at 15.24 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 176 /DD5))
    (pad 35 thru_hole circle (at 12.7 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 177 /DD4))
    (pad 36 thru_hole circle (at 10.16 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 178 /DD3))
    (pad 37 thru_hole circle (at 7.62 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 179 /DD2))
    (pad 38 thru_hole circle (at 5.08 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 180 /DD1))
    (pad 39 thru_hole circle (at 2.54 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 181 /DD0))
    (pad 40 thru_hole circle (at 0 -15.24 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP18_300 (layer F.Cu) (tedit 5B594191)
    (at 111.76 69.85)
    (fp_text reference U14 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value SAA1099 (at 9.906 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 154 /~WR))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 151 /CMS7-12_~CS))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 104 /A0))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 56 "Net-(C63-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 63 "Net-(C78-Pad1)"))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 119 "Net-(R34-Pad2)"))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 122 "Net-(R39-Pad2)"))
    (pad 18 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 210 VDDA))
    (pad 11 thru_hole circle (at 17.78 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 142 /D1))
    (pad 12 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 141 /D2))
    (pad 13 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 140 /D3))
    (pad 14 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 139 /D4))
    (pad 15 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 138 /D5))
    (pad 16 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 137 /D6))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 182 /CLK_7M159))
    (pad 17 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 136 /D7))
    (pad 9 thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 10 thru_hole circle (at 20.32 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 135 /D0))
  )
  (module SoundBlaster:SB_DIP18_300 (layer F.Cu) (tedit 5B594191)
    (at 111.76 88.9)
    (fp_text reference U15 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value SAA1099 (at 9.906 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 154 /~WR))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 152 /CMS1-6_~CS))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 104 /A0))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 56 "Net-(C63-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 63 "Net-(C78-Pad1)"))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 123 "Net-(R40-Pad2)"))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 122 "Net-(R39-Pad2)"))
    (pad 18 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 210 VDDA))
    (pad 11 thru_hole circle (at 17.78 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 142 /D1))
    (pad 12 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 141 /D2))
    (pad 13 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 140 /D3))
    (pad 14 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 139 /D4))
    (pad 15 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 138 /D5))
    (pad 16 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 137 /D6))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 182 /CLK_7M159))
    (pad 17 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 136 /D7))
    (pad 9 thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 10 thru_hole circle (at 20.32 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 135 /D0))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 116.84 111.76)
    (fp_text reference U16 (at -0.508 3.302) (layer F.SilkS))
    (fp_text value 74LS08 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 183 /~111000xxxx))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 184 /~100jjjxxxx))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 146 /~CARD_SELECTED))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 81 /~IOW))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 124 "Net-(R41-Pad2)"))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 154 /~WR))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 143 /~DB_EN))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 146 /~CARD_SELECTED))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 185 "Net-(U16-Pad10)"))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP16_300 (layer F.Cu) (tedit 5B594181)
    (at 78.74 111.76)
    (fp_text reference U17 (at -0.508 3.302) (layer F.SilkS))
    (fp_text value 74LS139 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 145 /1xx000xxxx))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 96 /A8))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 97 /A7))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 186 /~100000xxxx))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 183 /~111000xxxx))
    (pad 10 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 184 /~100jjjxxxx))
    (pad 13 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 97 /A7))
    (pad 14 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 96 /A8))
    (pad 15 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 70 "Net-(IO1-Pad10)"))
    (pad 16 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 9 thru_hole circle (at 17.78 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
  )
  (module SoundBlaster:SB_DIP20_300 (layer F.Cu) (tedit 5B59419A)
    (at 78.74 88.9)
    (fp_text reference U18 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS374 (at 12.192 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 171 /~DSP_READ))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 181 /DD0))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 135 /D0))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 142 /D1))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 180 /DD1))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 179 /DD2))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 141 /D2))
    (pad 18 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 136 /D7))
    (pad 11 thru_hole circle (at 22.86 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 57 /~ISA_WR))
    (pad 12 thru_hole circle (at 20.32 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 177 /DD4))
    (pad 13 thru_hole circle (at 17.78 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 139 /D4))
    (pad 14 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 138 /D5))
    (pad 15 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 176 /DD5))
    (pad 16 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 175 /DD6))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 140 /D3))
    (pad 17 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 137 /D6))
    (pad 9 thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 178 /DD3))
    (pad 10 thru_hole circle (at 22.86 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 19 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 174 /DD7))
    (pad 20 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP20_300 (layer F.Cu) (tedit 5B59419A)
    (at 78.74 69.85)
    (fp_text reference U19 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS374 (at 12.192 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 187 /~ISA_RD))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 135 /D0))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 181 /DD0))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 180 /DD1))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 142 /D1))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 141 /D2))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 179 /DD2))
    (pad 18 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 174 /DD7))
    (pad 11 thru_hole circle (at 22.86 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 64 /~DSP_WRITE))
    (pad 12 thru_hole circle (at 20.32 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 139 /D4))
    (pad 13 thru_hole circle (at 17.78 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 177 /DD4))
    (pad 14 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 176 /DD5))
    (pad 15 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 138 /D5))
    (pad 16 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 137 /D6))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 178 /DD3))
    (pad 17 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 175 /DD6))
    (pad 9 thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 140 /D3))
    (pad 10 thru_hole circle (at 22.86 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 19 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 136 /D7))
    (pad 20 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 55.88 50.8)
    (fp_text reference U20 (at -0.508 2.54) (layer F.SilkS))
    (fp_text value 74LS74 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 188 "Net-(U20-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 59 /DREQUEST))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 189 "Net-(U20-Pad5)"))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 190 "Net-(U20-Pad9)"))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 191 "Net-(U20-Pad10)"))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 192 "Net-(U20-Pad11)"))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 193 "Net-(U20-Pad12)"))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 55.88 66.04)
    (fp_text reference U21 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS125 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 194 /~RD_DAV))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 172 /DAV_PC))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 136 /D7))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 195 "Net-(U21-Pad4)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 196 "Net-(U21-Pad5)"))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 136 /D7))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 93 /IO_READY))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 190 "Net-(U20-Pad9)"))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 58 "Net-(C65-Pad1)"))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 189 "Net-(U20-Pad5)"))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 170 /~DMA_EN))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 55.88 81.28)
    (fp_text reference U22 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS74 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 187 /~ISA_RD))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 60 /~RESET))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 64 /~DSP_WRITE))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 172 /DAV_PC))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 173 /DAV_DSP))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 57 /~ISA_WR))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 60 /~RESET))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 171 /~DSP_READ))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 55.88 96.52)
    (fp_text reference U23 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS74 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 197 "Net-(U23-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 182 /CLK_7M159))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 198 /CLK_3M579))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 197 "Net-(U23-Pad2)"))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 199 "Net-(U23-Pad12)"))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 182 /CLK_7M159))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 84 /CLK_14M318))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 199 "Net-(U23-Pad12)"))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 55.88 111.76)
    (fp_text reference U24 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS32 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 105 /JOYSTICK_~CS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 134 /~RD))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 144 "Net-(U24-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 101 /A3))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 186 /~100000xxxx))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 209 "Net-(JP1-Pad1)"))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 132 "Net-(U1-Pad11)"))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 105 /JOYSTICK_~CS))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 154 /~WR))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 200 "Net-(U24-Pad11)"))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 150 /DSPRST_~CS))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 154 /~WR))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 33.02 111.76)
    (fp_text reference U25 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS08 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 201 /~DMAOUT))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 105 /JOYSTICK_~CS))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 185 "Net-(U16-Pad10)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 122 "Net-(R39-Pad2)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 133 /~IC))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 191 "Net-(U20-Pad10)"))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 134 /~RD))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 82 /~IOR))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 125 "Net-(R44-Pad2)"))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 193 "Net-(U20-Pad12)"))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 152 /CMS1-6_~CS))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 151 /CMS7-12_~CS))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 33.02 96.52)
    (fp_text reference U26 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS74 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 133 /~IC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 135 /D0))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 200 "Net-(U24-Pad11)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 202 "Net-(U26-Pad5)"))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 208 "Net-(IRQ2-Pad2)"))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 168 /IREQUEST))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 203 "Net-(U26-Pad13)"))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 33.02 81.28)
    (fp_text reference U27 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS32 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 204 "Net-(U27-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 134 /~RD))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 187 /~ISA_RD))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 134 /~RD))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 147 /DAV_~CS))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 194 /~RD_DAV))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 57 /~ISA_WR))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 154 /~WR))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 205 "Net-(U27-Pad10)"))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 195 "Net-(U21-Pad4)"))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 153 /DSPWR_~CS))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 134 /~RD))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 33.02 66.04)
    (fp_text reference U28 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS08 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 60 /~RESET))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 201 /~DMAOUT))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 188 "Net-(U20-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 201 /~DMAOUT))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 148 /DSPRD_~CS))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 204 "Net-(U27-Pad1)"))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 203 "Net-(U26-Pad13)"))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 194 /~RD_DAV))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 60 /~RESET))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 205 "Net-(U27-Pad10)"))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 153 /DSPWR_~CS))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 201 /~DMAOUT))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 33.02 50.8)
    (fp_text reference U29 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS14 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 80 /BUSRESET))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 133 /~IC))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 61 /RESET))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 60 /~RESET))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 192 "Net-(U20-Pad11)"))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 154 /~WR))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_DIP14_300 (layer F.Cu) (tedit 5B594178)
    (at 33.02 35.56)
    (fp_text reference U30 (at 0.635 3.302) (layer F.SilkS))
    (fp_text value 74LS32 (at 7.62 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 170 /~DMA_EN))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 83 /~DACK1))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 201 /~DMAOUT))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 169 /DSP_BUSY))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 173 /DAV_DSP))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 196 "Net-(U21-Pad5)"))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 61 /RESET))
    (pad 9 thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 202 "Net-(U26-Pad5)"))
    (pad 10 thru_hole circle (at 10.16 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 80 /BUSRESET))
    (pad 11 thru_hole circle (at 7.62 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
  )
  (module SoundBlaster:SB_XTAL_HC49U_RA (layer F.Cu) (tedit 5B594AA1)
    (at 67.31 35.56)
    (fp_text reference XTL1 (at -12.954 -9.906) (layer F.SilkS))
    (fp_text value 12MHz (at -9.652 -2.54) (layer F.Fab))
    (pad 2 thru_hole circle (at -9.652 3.302 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 55 "Net-(C62-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5.08 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 54 "Net-(C61-Pad1)"))
    (pad 4 thru_hole circle (at -9.652 -8.382 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module SoundBlaster:SB_D_AXIAL_400_ALT (layer F.Cu) (tedit 5B5941D3)
    (at 166.37 75.438)
    (fp_text reference ZD1 (at 13.462 0) (layer F.SilkS))
    (fp_text value 5.1V (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 213 +5VD))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_D_AXIAL_400_ALT (layer F.Cu) (tedit 5B5941D3)
    (at 186.69 81.28 180)
    (fp_text reference ZD2 (at 12.954 -0.254 180) (layer F.SilkS))
    (fp_text value 5.1V (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 215 -5VA))
  )
  (module SoundBlaster:SB_D_AXIAL_400_ALT (layer F.Cu) (tedit 5B5941D3)
    (at 154.94 78.74 180)
    (fp_text reference ZD3 (at -3.302 0 180) (layer F.SilkS))
    (fp_text value 5.1V (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 43 +5VA))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_DIP24_600 (layer F.Cu) (tedit 5B5941AB)
    (at 140.97 96.52)
    (fp_text reference U9 (at -3.048 3.048) (layer F.SilkS))
    (fp_text value YM3812 (at 13.208 -7.747) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 133 /~IC))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 104 /A0))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 154 /~WR))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 134 /~RD))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 149 /FM_~CS))
    (pad 18 thru_hole circle (at 15.24 -15.24) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 136 /D7))
    (pad 11 thru_hole circle (at 25.4 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 142 /D1))
    (pad 12 thru_hole circle (at 27.94 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 13 thru_hole circle (at 27.94 -15.24) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 141 /D2))
    (pad 14 thru_hole circle (at 25.4 -15.24) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 140 /D3))
    (pad 15 thru_hole circle (at 22.86 -15.24) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 139 /D4))
    (pad 16 thru_hole circle (at 20.32 -15.24) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 138 /D5))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 17.78 -15.24) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 137 /D6))
    (pad 9 thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 22.86 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 135 /D0))
    (pad 19 thru_hole circle (at 12.7 -15.24) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 10.16 -15.24) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 155 "Net-(U10-Pad3)"))
    (pad 21 thru_hole circle (at 7.62 -15.24) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 157 "Net-(U10-Pad4)"))
    (pad 22 thru_hole circle (at 5.08 -15.24) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 2.54 -15.24) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 158 "Net-(U10-Pad5)"))
    (pad 24 thru_hole circle (at 0 -15.24) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 198 /CLK_3M579))
  )
  (module SoundBlaster:SB_MH_125 (layer F.Cu) (tedit 5B5A750A)
    (at 254 55.372)
    (fp_text reference J2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "Bracket Mount" (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.81 3.81) (drill 3.175) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module SoundBlaster:SB_SJ1-3553 (layer F.Cu) (tedit 5B5A79D5)
    (at 256.286 83.486 180)
    (fp_text reference S1 (at 10.16 -0.08 180) (layer F.SilkS))
    (fp_text value OUT (at 2.54 0 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 1 thru_hole circle (at 5 5 180) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 206 "Net-(L1-Pad2)"))
    (pad 2 thru_hole circle (at 5 -5 180) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 207 "Net-(L2-Pad2)"))
    (pad 0 thru_hole circle (at 0 -5 180) (size 2 2) (drill 1.6) (layers *.Cu *.Mask))
    (pad 0 thru_hole circle (at 0 5 180) (size 2 2) (drill 1.6) (layers *.Cu *.Mask))
    (pad 0 thru_hole circle (at 5 0 180) (size 2 2) (drill 1.6) (layers *.Cu *.Mask))
  )
  (module SoundBlaster:SB_MJ-3536N (layer F.Cu) (tedit 5B5A7B4B)
    (at 257.048 45.212)
    (fp_text reference MIC1 (at -12.954 6.35) (layer F.SilkS))
    (fp_text value Microphone (at -6.35 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 270) (size 3.556 3.556) (drill 3.048) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 3 thru_hole circle (at -11.2014 -5.207 270) (size 3.556 3.556) (drill 3.048) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 1 thru_hole circle (at -13.6906 0 270) (size 3.556 3.556) (drill 3.048) (layers *.Cu *.Mask)
      (net 27 "Net-(C30-Pad2)"))
  )
  (module SoundBlaster:SB_NPTH_110 (layer F.Cu) (tedit 5B5A7EF7)
    (at 256.54 119.38)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value SB_NPTH_110 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.794 2.794) (drill 2.794) (layers *.Cu *.Mask))
  )
  (module SoundBlaster:SB_NPTH_110 (layer F.Cu) (tedit 5B5A7EF7)
    (at 30.48 119.38)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value SB_NPTH_110 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.794 2.794) (drill 2.794) (layers *.Cu *.Mask))
  )
  (module SoundBlaster:SB_DB15_152-3415 (layer F.Cu) (tedit 5B5E041F)
    (at 248.92 119.38)
    (fp_text reference P1 (at -4.572 0.508) (layer F.SilkS))
    (fp_text value Joystick/MIDI (at 6.223 -9.398 90) (layer F.Fab))
    (pad 7 thru_hole circle (at 0 -2.794 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 25 /BUTTON2))
    (pad 8 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 23 "Net-(C27-Pad1)"))
    (pad 6 thru_hole circle (at 0 -5.588 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 107 /Y1))
    (pad 5 thru_hole circle (at 0 -8.382 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 4 thru_hole circle (at 0 -11.176 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 3 thru_hole circle (at 0 -13.97 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 106 /X1))
    (pad 2 thru_hole circle (at 0 -16.764 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 20 /BUTTON1))
    (pad 1 thru_hole circle (at 0 -19.558 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 23 "Net-(C27-Pad1)"))
    (pad 15 thru_hole circle (at 2.8702 -1.397 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 111 /MIDI_IN))
    (pad 14 thru_hole circle (at 2.8702 -4.191 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 24 /BUTTON3))
    (pad 13 thru_hole circle (at 2.8702 -6.985 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 110 /Y2))
    (pad 12 thru_hole circle (at 2.8702 -9.779 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 109 /MIDI_OUT))
    (pad 11 thru_hole circle (at 2.8702 -12.573 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 108 /X2))
    (pad 10 thru_hole circle (at 2.8702 -15.367 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 21 /BUTTON4))
    (pad 9 thru_hole circle (at 2.8702 -18.161 270) (size 1.524 1.524) (drill 1.0922) (layers *.Cu *.Mask)
      (net 23 "Net-(C27-Pad1)"))
    (pad 0 thru_hole circle (at 1.4351 7.0612 270) (size 3.556 3.556) (drill 2.8702) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 0 thru_hole circle (at 1.4351 -26.2128 270) (size 3.556 3.556) (drill 2.8702) (layers *.Cu *.Mask)
      (net 211 GNDA))
  )
  (module Conn:MNT_KEYSTONE_9200 (layer F.Cu) (tedit 5A7A8805)
    (at 236.22 121.92)
    (fp_text reference REF** (at 18.796 -60.071) (layer F.SilkS) hide)
    (fp_text value MNT_KEYSTONE_9200 (at 18.796 -61.46) (layer F.Fab) hide)
    (model "C:/Data/Projects/Adlib/mech/keystone 9202.wrl"
      (at (xyz 1 -1.05 0.255))
      (scale (xyz 10 10 10))
      (rotate (xyz 0 0 0))
    )
  )
  (module SoundBlaster:SB_ALPS_RK08_DUAL (layer F.Cu) (tedit 5C3FC2DB)
    (at 252.476 64.008 180)
    (fp_text reference S2 (at -0.127 6.604 180) (layer F.SilkS))
    (fp_text value ALPS_RK08H_DUAL (at 0 0 180) (layer F.Fab))
    (pad 1B thru_hole circle (at 3.302 -3.302 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(C37-Pad2)"))
    (pad 3 thru_hole circle (at -3.302 -3.302 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 211 GNDA))
    (pad 1A thru_hole circle (at 0 -4.699 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(C36-Pad1)"))
    (pad 2B thru_hole circle (at 3.937 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 14 "Net-(C14-Pad2)"))
    (pad 2A thru_hole circle (at -3.937 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Symbols:WEEE-Logo_8.4x12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 62.103 30.226 180)
    (descr "Waste Electrical and Electronic Equipment Directive")
    (tags "Logo WEEE")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value WEEE-Logo_8.4x12mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module SoundBlaster:Snark_Barker (layer F.Cu) (tedit 0)
    (at 106.426 30.226)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text "Foone: testing" (at 132.588 57.912) (layer B.SilkS))
  (dimension 6.2738 (width 0.3) (layer Dwgs.User)
    (gr_text "0.2470 in" (at 289.7759 134.8016) (layer Dwgs.User))
    (feature1 (pts (xy 292.9128 126.4412) (xy 292.9128 136.1516)))
    (feature2 (pts (xy 286.639 126.4412) (xy 286.639 136.1516)))
    (crossbar (pts (xy 286.639 133.4516) (xy 292.9128 133.4516)))
    (arrow1a (pts (xy 292.9128 133.4516) (xy 291.786296 134.038021)))
    (arrow1b (pts (xy 292.9128 133.4516) (xy 291.786296 132.865179)))
    (arrow2a (pts (xy 286.639 133.4516) (xy 287.765504 134.038021)))
    (arrow2b (pts (xy 286.639 133.4516) (xy 287.765504 132.865179)))
  )
  (gr_text "SHOUTS TO cr1901, CommodoreZ, glitch, and Trixter" (at 101.6 117.856) (layer B.SilkS))
  (gr_text "Special thanks to ##yamahasynths" (at 125.984 66.548) (layer B.SilkS))
  (gr_text "Lord_Nightmare, balrog, kevtris: lots of info" (at 132.588 55.372) (layer B.SilkS))
  (gr_text "digshadow: misc reversing" (at 132.461 48.26) (layer B.SilkS))
  (gr_text "GoodTofuFriday: PCB photography" (at 132.588 45.72) (layer B.SilkS))
  (gr_text "also firmware analysis" (at 117.348 43.18) (layer B.SilkS))
  (gr_text "TubeTimeUS: PCB reversing and forwarding," (at 132.588 40.64) (layer B.SilkS))
  (gr_text CREDITS (at 128.016 38.1) (layer B.SilkS))
  (dimension 66.065576 (width 0.3) (layer Dwgs.User)
    (gr_text "2.6010 in" (at 278.704363 62.229611 89.86783004) (layer Dwgs.User))
    (feature1 (pts (xy 284.4546 29.21) (xy 277.430567 29.193797)))
    (feature2 (pts (xy 284.3022 95.2754) (xy 277.278167 95.259197)))
    (crossbar (pts (xy 279.97816 95.265425) (xy 280.13056 29.200025)))
    (arrow1a (pts (xy 280.13056 29.200025) (xy 280.714381 30.327879)))
    (arrow1b (pts (xy 280.13056 29.200025) (xy 279.541542 30.325173)))
    (arrow2a (pts (xy 279.97816 95.265425) (xy 280.567178 94.140277)))
    (arrow2b (pts (xy 279.97816 95.265425) (xy 279.394339 94.137571)))
  )
  (dimension 10.668 (width 0.3) (layer Dwgs.User)
    (gr_text "0.4200 in" (at 286.639 131.257181) (layer Dwgs.User))
    (feature1 (pts (xy 281.305 119.4562) (xy 281.305 132.607181)))
    (feature2 (pts (xy 291.973 119.4562) (xy 291.973 132.607181)))
    (crossbar (pts (xy 291.973 129.907181) (xy 281.305 129.907181)))
    (arrow1a (pts (xy 281.305 129.907181) (xy 282.431504 129.32076)))
    (arrow1b (pts (xy 281.305 129.907181) (xy 282.431504 130.493602)))
    (arrow2a (pts (xy 291.973 129.907181) (xy 290.846496 129.32076)))
    (arrow2b (pts (xy 291.973 129.907181) (xy 290.846496 130.493602)))
  )
  (dimension 33.27401 (width 0.3) (layer Dwgs.User)
    (gr_text "1.3100 in" (at 310.812367 109.818532 89.95626277) (layer Dwgs.User))
    (feature1 (pts (xy 292.0238 126.4412) (xy 312.149667 126.456563)))
    (feature2 (pts (xy 292.0492 93.1672) (xy 312.175067 93.182563)))
    (crossbar (pts (xy 309.475068 93.180502) (xy 309.449668 126.454502)))
    (arrow1a (pts (xy 309.449668 126.454502) (xy 308.864107 125.327551)))
    (arrow1b (pts (xy 309.449668 126.454502) (xy 310.036948 125.328446)))
    (arrow2a (pts (xy 309.475068 93.180502) (xy 308.887788 94.306558)))
    (arrow2b (pts (xy 309.475068 93.180502) (xy 310.060629 94.307453)))
  )
  (dimension 63.957205 (width 0.3) (layer Dwgs.User)
    (gr_text "2.5180 in" (at 323.304829 61.201008 89.97724552) (layer Dwgs.User))
    (feature1 (pts (xy 292.0492 93.1672) (xy 324.642129 93.180144)))
    (feature2 (pts (xy 292.0746 29.21) (xy 324.667529 29.222944)))
    (crossbar (pts (xy 321.967529 29.221872) (xy 321.942129 93.179072)))
    (arrow1a (pts (xy 321.942129 93.179072) (xy 321.356156 92.052335)))
    (arrow1b (pts (xy 321.942129 93.179072) (xy 322.528997 92.052801)))
    (arrow2a (pts (xy 321.967529 29.221872) (xy 321.380661 30.348143)))
    (arrow2b (pts (xy 321.967529 29.221872) (xy 322.553502 30.348609)))
  )
  (dimension 54.2798 (width 0.3) (layer Dwgs.User)
    (gr_text "2.1370 in" (at 317.75067 56.3499 270) (layer Dwgs.User))
    (feature1 (pts (xy 292.0746 83.4898) (xy 319.10067 83.4898)))
    (feature2 (pts (xy 292.0746 29.21) (xy 319.10067 29.21)))
    (crossbar (pts (xy 316.40067 29.21) (xy 316.40067 83.4898)))
    (arrow1a (pts (xy 316.40067 83.4898) (xy 315.814249 82.363296)))
    (arrow1b (pts (xy 316.40067 83.4898) (xy 316.987091 82.363296)))
    (arrow2a (pts (xy 316.40067 29.21) (xy 315.814249 30.336504)))
    (arrow2b (pts (xy 316.40067 29.21) (xy 316.987091 30.336504)))
  )
  (dimension 22.606 (width 0.3) (layer Dwgs.User)
    (gr_text "0.8900 in" (at 309.657556 40.513 270) (layer Dwgs.User))
    (feature1 (pts (xy 292.0746 51.816) (xy 311.007556 51.816)))
    (feature2 (pts (xy 292.0746 29.21) (xy 311.007556 29.21)))
    (crossbar (pts (xy 308.307556 29.21) (xy 308.307556 51.816)))
    (arrow1a (pts (xy 308.307556 51.816) (xy 307.721135 50.689496)))
    (arrow1b (pts (xy 308.307556 51.816) (xy 308.893977 50.689496)))
    (arrow2a (pts (xy 308.307556 29.21) (xy 307.721135 30.336504)))
    (arrow2b (pts (xy 308.307556 29.21) (xy 308.893977 30.336504)))
  )
  (dimension 16.002 (width 0.3) (layer Dwgs.User)
    (gr_text "0.6300 in" (at 302.9496 37.211 90) (layer Dwgs.User))
    (feature1 (pts (xy 292.0746 29.21) (xy 304.2996 29.21)))
    (feature2 (pts (xy 292.0746 45.212) (xy 304.2996 45.212)))
    (crossbar (pts (xy 301.5996 45.212) (xy 301.5996 29.21)))
    (arrow1a (pts (xy 301.5996 29.21) (xy 302.186021 30.336504)))
    (arrow1b (pts (xy 301.5996 29.21) (xy 301.013179 30.336504)))
    (arrow2a (pts (xy 301.5996 45.212) (xy 302.186021 44.085496)))
    (arrow2b (pts (xy 301.5996 45.212) (xy 301.013179 44.085496)))
  )
  (dimension 3.429 (width 0.3) (layer Dwgs.User)
    (gr_text "0.1350 in" (at 288.3535 49.4246) (layer Dwgs.User))
    (feature1 (pts (xy 290.068 51.816) (xy 290.068 48.0746)))
    (feature2 (pts (xy 286.639 51.816) (xy 286.639 48.0746)))
    (crossbar (pts (xy 286.639 50.7746) (xy 290.068 50.7746)))
    (arrow1a (pts (xy 290.068 50.7746) (xy 288.941496 51.361021)))
    (arrow1b (pts (xy 290.068 50.7746) (xy 288.941496 50.188179)))
    (arrow2a (pts (xy 286.639 50.7746) (xy 287.765504 51.361021)))
    (arrow2b (pts (xy 286.639 50.7746) (xy 287.765504 50.188179)))
  )
  (dimension 0.8382 (width 0.3) (layer Dwgs.User)
    (gr_text "0.0330 in" (at 287.0581 38.0454) (layer Dwgs.User))
    (feature1 (pts (xy 287.4772 45.212) (xy 287.4772 36.6954)))
    (feature2 (pts (xy 286.639 45.212) (xy 286.639 36.6954)))
    (crossbar (pts (xy 286.639 39.3954) (xy 287.4772 39.3954)))
    (arrow1a (pts (xy 287.4772 39.3954) (xy 286.350696 39.981821)))
    (arrow1b (pts (xy 287.4772 39.3954) (xy 286.350696 38.808979)))
    (arrow2a (pts (xy 286.639 39.3954) (xy 287.765504 39.981821)))
    (arrow2b (pts (xy 286.639 39.3954) (xy 287.765504 38.808979)))
  )
  (dimension 24.384 (width 0.3) (layer Dwgs.User)
    (gr_text "0.9600 in" (at 299.927 64.008 90) (layer Dwgs.User))
    (feature1 (pts (xy 293.624 51.816) (xy 301.277 51.816)))
    (feature2 (pts (xy 293.624 76.2) (xy 301.277 76.2)))
    (crossbar (pts (xy 298.577 76.2) (xy 298.577 51.816)))
    (arrow1a (pts (xy 298.577 51.816) (xy 299.163421 52.942504)))
    (arrow1b (pts (xy 298.577 51.816) (xy 297.990579 52.942504)))
    (arrow2a (pts (xy 298.577 76.2) (xy 299.163421 75.073496)))
    (arrow2b (pts (xy 298.577 76.2) (xy 297.990579 75.073496)))
  )
  (dimension 4.699 (width 0.3) (layer Dwgs.User)
    (gr_text "0.1850 in" (at 287.7185 66.341) (layer Dwgs.User))
    (feature1 (pts (xy 285.369 76.2) (xy 285.369 64.991)))
    (feature2 (pts (xy 290.068 76.2) (xy 290.068 64.991)))
    (crossbar (pts (xy 290.068 67.691) (xy 285.369 67.691)))
    (arrow1a (pts (xy 285.369 67.691) (xy 286.495504 67.104579)))
    (arrow1b (pts (xy 285.369 67.691) (xy 286.495504 68.277421)))
    (arrow2a (pts (xy 290.068 67.691) (xy 288.941496 67.104579)))
    (arrow2b (pts (xy 290.068 67.691) (xy 288.941496 68.277421)))
  )
  (dimension 28.829 (width 0.3) (layer Dwgs.User)
    (gr_text "1.1350 in" (at 277.7452 109.6899 90) (layer Dwgs.User))
    (feature1 (pts (xy 284.3276 95.2754) (xy 276.3952 95.2754)))
    (feature2 (pts (xy 284.3276 124.1044) (xy 276.3952 124.1044)))
    (crossbar (pts (xy 279.0952 124.1044) (xy 279.0952 95.2754)))
    (arrow1a (pts (xy 279.0952 95.2754) (xy 279.681621 96.401904)))
    (arrow1b (pts (xy 279.0952 95.2754) (xy 278.508779 96.401904)))
    (arrow2a (pts (xy 279.0952 124.1044) (xy 279.681621 122.977896)))
    (arrow2b (pts (xy 279.0952 124.1044) (xy 278.508779 122.977896)))
  )
  (dimension 106.68 (width 0.3) (layer Dwgs.User)
    (gr_text "4.2000 in" (at 268.05 76.2 90) (layer Dwgs.User))
    (feature1 (pts (xy 259.08 22.86) (xy 269.4 22.86)))
    (feature2 (pts (xy 259.08 129.54) (xy 269.4 129.54)))
    (crossbar (pts (xy 266.7 129.54) (xy 266.7 22.86)))
    (arrow1a (pts (xy 266.7 22.86) (xy 267.286421 23.986504)))
    (arrow1b (pts (xy 266.7 22.86) (xy 266.113579 23.986504)))
    (arrow2a (pts (xy 266.7 129.54) (xy 267.286421 128.413496)))
    (arrow2b (pts (xy 266.7 129.54) (xy 266.113579 128.413496)))
  )
  (dimension 231.14 (width 0.3) (layer Dwgs.User)
    (gr_text "9.1000 in" (at 143.51 15.414001) (layer Dwgs.User))
    (feature1 (pts (xy 27.94 21.59) (xy 27.94 14.064001)))
    (feature2 (pts (xy 259.08 21.59) (xy 259.08 14.064001)))
    (crossbar (pts (xy 259.08 16.764001) (xy 27.94 16.764001)))
    (arrow1a (pts (xy 27.94 16.764001) (xy 29.066504 16.17758)))
    (arrow1b (pts (xy 27.94 16.764001) (xy 29.066504 17.350422)))
    (arrow2a (pts (xy 259.08 16.764001) (xy 257.953496 16.17758)))
    (arrow2b (pts (xy 259.08 16.764001) (xy 257.953496 17.350422)))
  )
  (gr_text 1 (at 235.204 120.904) (layer F.SilkS))
  (gr_text 31 (at 154.686 120.65) (layer F.SilkS))
  (gr_text 01/19 (at 31.75 24.13) (layer F.SilkS))
  (gr_text "MADE IN ANGER" (at 212.09 117.602) (layer F.SilkS))
  (gr_text VCC (at 82.042 32.766 90) (layer F.SilkS))
  (gr_text GND (at 74.168 32.766 90) (layer F.SilkS))
  (gr_text TXD (at 74.168 27.686 90) (layer F.SilkS))
  (gr_text RXD (at 82.042 27.686 90) (layer F.SilkS))
  (gr_text © (at 77.724 117.856) (layer F.SilkS))
  (gr_text " CC BY-SA (Attribution-ShareAlike)" (at 77.724 117.856) (layer F.SilkS))
  (gr_text 260 (at 186.69 100.33 90) (layer F.SilkS))
  (gr_text 250 (at 184.15 100.33 90) (layer F.SilkS))
  (gr_text 240 (at 181.61 100.33 90) (layer F.SilkS))
  (gr_text 230 (at 179.07 100.33 90) (layer F.SilkS))
  (gr_text 220 (at 176.53 100.33 90) (layer F.SilkS))
  (gr_text 210 (at 173.99 100.33 90) (layer F.SilkS))
  (gr_text "I/O ADDX" (at 181.864 89.916) (layer F.SilkS))
  (gr_text CT-1320C (at 41.402 120.396) (layer F.SilkS))
  (gr_line (start 259.08 129.54) (end 259.08 22.86) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 246.38 129.54) (end 259.08 129.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 128.27) (end 154.94 121.92) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.21 129.54) (end 154.94 128.27) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 234.95 129.54) (end 156.21 129.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 236.22 128.27) (end 234.95 129.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 246.38 121.92) (end 246.38 129.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 236.22 121.92) (end 246.38 121.92) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 236.22 128.27) (end 236.22 121.92) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 27.94 121.92) (end 154.94 121.92) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 27.94 22.86) (end 27.94 121.92) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 259.08 22.86) (end 27.94 22.86) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57.658 26.8386) (xy 57.15 27.178) (xy 53.594 27.178) (xy 52.324 28.448) (xy 52.324 37.338)
        (xy 53.848 38.862) (xy 62.738 38.862) (xy 64.77 36.7446) (xy 64.77 28.6166) (xy 66.548 26.8386)
      )
    )
  )
  (zone (net 211) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.69 81.28) (xy 189.23 83.82) (xy 212.344 83.82) (xy 213.36 84.328) (xy 220.472 84.328)
        (xy 244.602 84.328) (xy 246.126 85.852) (xy 246.126 104.14) (xy 237.744 104.14) (xy 237.744 112.268)
        (xy 234.696 112.268) (xy 233.172 113.792) (xy 233.172 123.952) (xy 234.188 123.952) (xy 236.22 121.92)
        (xy 246.38 121.92) (xy 246.38 129.54) (xy 259.08 129.54) (xy 259.08 22.86) (xy 245.872 22.86)
        (xy 245.872 23.876) (xy 247.396 25.4) (xy 256.032 25.4) (xy 256.54 25.908) (xy 256.54 36.576)
        (xy 256.032 37.084) (xy 234.696 37.084) (xy 234.188 37.592) (xy 234.188 39.116) (xy 233.68 39.624)
        (xy 227.076 39.624) (xy 226.568 40.132) (xy 198.628 40.132) (xy 188.468 40.132) (xy 186.944 38.862)
        (xy 182.88 38.862) (xy 182.88 41.91) (xy 184.15 43.18) (xy 187.96 43.18) (xy 187.96 44.7675)
        (xy 182.88 44.7675) (xy 182.88 45.4025) (xy 186.69 45.4025)
      )
    )
  )
  (zone (net 23) (net_name "Net-(C27-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 243.078 107.696) (xy 243.586 107.188) (xy 244.602 107.188) (xy 245.11 106.68) (xy 245.11 99.822)
        (xy 245.872 99.06) (xy 248.666 99.06) (xy 248.92 99.06) (xy 249.682 99.822) (xy 249.682 104.648)
        (xy 249.682 116.078) (xy 249.682 119.634) (xy 248.412 120.396) (xy 245.872 120.396) (xy 245.11 119.634)
        (xy 245.11 112.522) (xy 244.602 112.014) (xy 243.586 112.014) (xy 243.078 111.506)
      )
    )
  )
  (zone (net 23) (net_name "Net-(C27-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 247.65 99.822) (xy 248.92 99.822) (xy 251.46 102.362) (xy 252.73 102.362) (xy 253.238 101.854)
        (xy 253.238 98.298) (xy 251.46 96.52) (xy 247.142 96.52) (xy 246.634 97.028) (xy 246.634 98.806)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 233.68 116.84) (xy 232.918 116.332) (xy 232.918 115.316) (xy 231.394 113.792) (xy 222.758 113.792)
        (xy 220.472 111.506) (xy 220.472 110.49) (xy 220.472 109.474) (xy 221.234 108.712) (xy 222.504 108.712)
        (xy 224.282 110.49) (xy 227.838 110.49) (xy 230.124 108.204) (xy 236.728 108.204) (xy 237.998 106.934)
        (xy 237.998 87.884) (xy 238.76 87.122) (xy 241.046 87.122) (xy 241.808 87.884) (xy 241.808 98.298)
        (xy 241.808 115.57) (xy 240.538 116.84)
      )
    )
  )
  (zone (net 211) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.96 82.804) (xy 185.42 82.804) (xy 184.15 81.534) (xy 184.15 49.022) (xy 186.182 46.99)
        (xy 186.182 42.164) (xy 187.198 41.148) (xy 203.708 41.148) (xy 204.216 40.64) (xy 221.234 40.64)
        (xy 224.79 37.084) (xy 251.46 37.084) (xy 252.222 36.322) (xy 254.762 36.322) (xy 256.286 34.798)
        (xy 256.286 25.908) (xy 255.778 25.4) (xy 254.762 25.4) (xy 254.762 23.876) (xy 259.08 23.876)
        (xy 259.08 129.54) (xy 246.38 129.54) (xy 246.38 121.412) (xy 252.222 121.412) (xy 252.984 120.65)
        (xy 252.984 96.012) (xy 249.428 96.012) (xy 246.634 93.218) (xy 246.634 86.106) (xy 244.856 84.328)
        (xy 210.058 84.328) (xy 209.55 83.82) (xy 188.976 83.82)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.94 121.92) (xy 154.94 128.27) (xy 156.21 129.54) (xy 234.95 129.54) (xy 236.22 128.27)
        (xy 236.22 121.92)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.94 121.92) (xy 154.94 128.27) (xy 156.21 129.54) (xy 234.95 129.54) (xy 236.22 128.27)
        (xy 236.22 121.92)
      )
    )
  )
)
