# Transmitters

###

Testing and adjustment of transmitters should be done on a dummy load.

The most important adjustment is the audio level. Excess audio will cause over-modulation in all its forms and hence interference to other users of the bands.

An oscilloscope is invaluable for adjustment of an SSB transmitter (see Chapter 10).

-

Back | Index |  | Next

page (c4-1-12)
Click here for important Copyright information
| Web Space provided by Hostroute.com Ltd
email the Project Co-ordinator