The Amateur Radio Project - Transmitter interference

# Transmitter interference

### Question 4 of 17

With double sideband, full carrier amplitude modulated transmission, an AF bandwidth of 3kHz will produce an RF bandwidth of

1. 6kHz
2. 3kHz
3. 1.5kHz
4. 0.75kHz

1 | 2 | 3 | 4

Back |

page (tq2404)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details