# Section 5 - Antennas & Feeders

## 5.4 - 5.6 The end-fed antenna

This antenna is often used at the lower frequencies (HF) where space limitations prevent the use of a dipole or similar resonant antenna. A wire of convenient length is suspended between two supports, often the house and a tree or mast at the bottom of the garden. One end of this wire is connected to the radio, hence the name "end-fed", the radio energy is fed in at one end of the antenna.

Such an antenna is often used over a range of frequencies and is often not a perfect half or quarter wave at any of them. For this reason it is not by itself a suitable antenna for direct connection to the transmitter. A high SWR would be shown and transmitter damage would likely occur if connected directly to the transmitter. A device called an antenna tuning unit (ATU) is usually used to allow the antenna to accept the signal from the radio without the high SWR which would otherwise be present.

Because there is no feeder, the radiating antenna runs all the way into the house. This can mean high RF voltages or currents are present close to the building, and interference to other electrical equipment (e.g. televisions) is likely to occur.

Back | Index | Next

Page f5-1-3
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
email the Project Co-ordinator