# Measurements

### Multi-range meters

Many commercial multi-range meters are available, in both digital and analogue form. These consist of a number of voltage multipliers and current shunts, an instrument rectifier and current transformer, all of which are switched to provide a large number of DC and AC voltage and current ranges on a high-sensitivity meter.

A photo of a typical analogue Multi-Meter

A photo of a typical Digital LCD Multi-Meter

Back | Index |  | Next

page (c10-1-4)
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
email the Project Co-ordinator