# Section 2 - Licensing Conditions

## 2.13 The Schedule

The schedule is a table printed at the back of the terms and conditions document BR68F. It tells you where and how you may operate. For each band it tells you permitted modes, maximum power output allowed as well as the frequencies defining the edges of the band. You will be provided with a copy of this document during the training course and during the assessment. You should seek to obtain an up to date copy of this document and learn as much of it as possible. When you get your license you will need to know where you can operate.

Frequency Bands in MHz | Status of Allocations in the United Kingdom to the Amateur Service | Power | Mode of transmission
0.1357 - 0.1378 | Secondary. Available on the basis of non-interference to other services (inside or outside the United Kingdom) | 1W (0dBW) erp | Morse, Telephony, RTTY, Data, Facsimile, SSTV
1.810 - 1.830 | Primary. Available on the basis of non-interference to other services (outside the United Kingdom) | Power fed to the antenna 10W (10dBW)
1.830 - 1.850 | Primary
1.850 - 2.000 | Available on the basis of non-interference to other services (inside or outside the United Kingdom)
3.500 - 3.800 | Primary. Shared with other services
7.000 - 7.100 | Primary
10.100 - 10.150 | Secondary
14.000 - 14.250 | Primary
14.250 - 14.350
18.068 - 18.168
21.000 - 21.450
24.890 - 24.990
50.00 - 51.00 | Primary. Available on the basis of non-interference to other services (outside the United Kingdom)
51.00 - 52.00 | Secondary. Available on the basis of non-interference to other services (inside or outside the United Kingdom)
70.00 - 70.50
144.0 - 146.0 | Primary |
430.0 - 431.0 | Secondary | 10W (10dBW) erp
431.0 - 432.0 | Secondary. Not available for use within a 100km radius of Charing Cross, London (51º30'30"N, 00º07'24"W)
432.0 - 438.0 | Secondary | 10W (10dBW)
438.0 - 440.0 | Secondary

Column 1 of the schedule shows us where the foundation licensee may operate.

Column 2 gives the status of the allocation. Secondary status means we must not interfere with those users who have primary status within the band.

Column 3 tells us how much power we may use. Power is usually measured at the antenna terminals. At the higher frequencies, a significant power loss may occur in the feeder connecting the transmitter to the antenna. It is permissible to increase our transmitter power output to compensate for this loss. It is however much better to use a different kind of feeder with a lower loss, since losses in the feeder will affect the received signal too.

Note that for the frequencies 430-432MHz. the maximum power allowed is expressed as 10W erp (effective radiated power). This is not the same as power at the antenna terminals. Effective radiated power erp = power x antenna gain. So, if we were using an antenna with a gain of 4 (6dB) then we must ensure that we do not exceed 2.5W at the antenna terminals, erp = 2.5 x 4 = 10W.

Column 4 tells us which methods of communication we may use. Note that for the foundation license they are all the same for every band. We will learn more about the different kinds of communication we may use later in the course.

Extracts from the syllabus and BR68F ©Crown copyright Radiocommunications Agency

Back | Index | Next

Page f2-1-6
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
email the Project Co-ordinator