SBD16.EXE is a 16 Bit demo of 'Speaker Box Design v2.1'.
This EXE file contains the installation program, uninstall
program, and all the files needed to run the program. The default
directory for the installation is 'C:\SPEAKER' but you
may chang this to any directory you wish. To install the program,
from the Program Manager's File menu choose RUN, in the Command-Line
box type d:\sub\SBD16.EXE. Where 'd:' is the drive letter the program
is on and 'sub' is the sub-directory it is in.
The program helps in the design of Closed, Vented, Passive,
and Bandpass enclosures. It also designs passive and active
crossover systems, impedance matching and notch filter networks,
and helps in the design of the coils if you wish to make your own.
The program has graphics, printing, and load/save capabilities.
With this version you need a VGA monitor, 8 Megs of RAM (16 recomended),
and Windows 3.1 or greater. If you are using Win95 or Windows NT,
please use the 32 Bit version 'SBD32.EXE'.
If you have any trouble installing the software or have any questions,
I can be reached at:
E-mail - bodtrons@nauticom.net
Mail -  Al Bodnar
        650 N. Pike Rd.
        Cabot, Pa. 16023

