The Amateur Radio Project - Resistors in series and parallel; power

# Resistors in series and parallel; power

### Question 12 of 15

A p.d. of 15V is applied across the ends of two resistors connected in series. The power dissipated in the resistors is 0.5W and 2W respectively. The total power dissipated will be

1. 2.5W
2. 2W
3. 1.5W
4. 0.4W

1 | 2 | 3 | 4

Back |

page (tq0312)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details