# Section 5 - Antennas & Feeders

## 5.4 - 5.6 The Vertical Monopole Antenna

The antenna in the picture on the left is known as a quarter wave vertical antenna, because it radiates from a vertical element which is one quarter of a wavelength long. It will only radiate efficiently if the vertical element is exactly one-quarter of a wavelength long at the frequency of operation.

Radiation from the antenna is in all directions equally, roughly at right angles to the antenna element. The radio signals are actually directed slightly above an imaginary horizontal line from the antenna base. There is no radiation off the end of the element i.e. straight upwards. The four horizontal elements are called radials and provide a ground-plane for the antenna. A ground plane is an artificial earth close to the antenna. This acts like a mirror to the radio waves and helps shape the pattern of radiation from the antenna.

In practice the radials are often bent downwards to improve matching.

The five-eighth wave vertical is a development of the quarter wave vertical shown above. In this instance the antenna's radiating element is five-eighths of a wavelength long. This antenna is very popular for use on the VHF and UHF bands. At HF frequencies its sheer size makes it impossible for most to utilise.

Again it is omni-directional, but the longer element gives this antenna the characteristic that the signals radiating from it are directed much more towards the horizon. There is much less upwards radiation from this antenna than the quarter wave vertical shown above.

The coil at the bottom of the antenna, is part of a matching circuit necessary to couple this type of antenna to the coaxial feeder.

Back | Index | Next

Page f5-1-2
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
email the Project Co-ordinator